3GPP TS 29.502 V15.1.0 (2018-09)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Core Network and Terminals;

5G System; Session Management Services;

Stage 3

(Release 15)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

3GPP, 5G System

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2018, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 7

1 Scope 8

2 References 8

3 Definitions and abbreviations 9

3.1 Definitions 9

3.2 Abbreviations 9

4 Overview 9

4.1 Introduction 9

5 Services offered by the SMF 10

5.1 Introduction 10

5.2 Nsmf\_PDUSession Service 10

5.2.1 Service Description 10

5.2.2 Service Operations 11

5.2.2.1 Introduction 11

5.2.2.2 Create SM Context service operation 11

5.2.2.2.1 General 11

5.2.2.2.2 EPS to 5GS Idle mode mobility using N26 interface 13

5.2.2.2.3 EPS to 5GS Handover Preparation using N26 interface 15

5.2.2.3 Update SM Context service operation 16

5.2.2.3.1 General 16

5.2.2.3.2 Activation and Deactivation of the User Plane connection of a PDU session 17

5.2.2.3.2.1 General 17

5.2.2.3.2.2 Activation of User Plane connectivity of a PDU session 17

5.2.2.3.2.3 Deactivation of User Plane connectivity of a PDU session 18

5.2.2.3.3 Xn Handover 19

5.2.2.3.4 N2 Handover 20

5.2.2.3.4.1 General 20

5.2.2.3.4.2 N2 Handover Preparation 20

5.2.2.3.4.3 N2 Handover Execution 22

5.2.2.3.4.4 N2 Handover Cancellation 23

5.2.2.3.5 Handover between 3GPP and untrusted non-3GPP access procedures 23

5.2.2.3.5.1 General 23

5.2.2.3.5.2 Handover of a PDU session without AMF change or with target AMF in same PLMN 23

5.2.2.3.6 Inter-AMF change or mobility 24

5.2.2.3.7 RAN Initiated QoS Flow Mobility 25

5.2.2.3.8 EPS to 5GS Handover using N26 interface 25

5.2.2.3.8.1 General 25

5.2.2.3.8.2 EPS to 5GS Handover Preparation 25

5.2.2.3.8.3 EPS to 5GS Handover Execution 26

5.2.2.3.8.4 EPS to 5GS Handover Cancellation 26

5.2.2.3.9 5GS to EPS Handover using N26 interface 26

5.2.2.3.10 P-CSCF Restoration Procedure via AMF 27

5.2.2.4 Release SM Context service operation 28

5.2.2.4.1 General 28

5.2.2.5 Notify SM Context Status service operation 29

5.2.2.5.1 General 29

5.2.2.6 Retrieve SM Context service operation 30

5.2.2.6.1 General 30

5.2.2.7 Create service operation 30

5.2.2.7.1 General 30

5.2.2.7.2 EPS to 5GS Idle mode mobility 32

5.2.2.7.3 EPS to 5GS Handover Preparation 32

5.2.2.8 Update service operation 33

5.2.2.8.1 General 33

5.2.2.8.2 Update service operation towards H-SMF 34

5.2.2.8.2.1 General 34

5.2.2.8.2.2 UE or visited network requested PDU session modification 34

5.2.2.8.2.3 UE requested PDU session release 35

5.2.2.8.2.4 EPS to 5GS Handover Execution 35

5.2.2.8.2.5 Handover between 3GPP and untrusted non-3GPP access (Home Routed PDU session) 35

5.2.2.8.2.6 P-CSCF Restoration Procedure via AMF (Home Routed PDU session) 35

5.2.2.8.3 Update service operation towards V-SMF 35

5.2.2.8.3.1 General 35

5.2.2.8.3.2 Home network requested PDU session modification 36

5.2.2.8.3.3 Home network requested PDU session release 37

5.2.2.8.3.4 Handover between 3GPP and untrusted non-3GPP access, from 5GC-N3IWF to EPS or from 5GS to EPC/ePDG 37

5.2.2.8.3.5 EPS Bearer ID allocation 37

5.2.2.9 Release service operation 38

5.2.2.9.1 General 38

5.2.2.10 Notify Status service operation 38

5.2.2.10.1 General 38

5.2.3 General procedures 39

5.2.3.1 Transfer of NAS SM information between UE and H-SMF for Home Routed PDU sessions 39

5.2.3.1.1 General 39

5.2.3.1.2 V-SMF Behaviour 39

5.2.3.1.3 H-SMF Behaviour 40

6 API Definitions 40

6.1 Nsmf\_PDUSession Service API 40

6.1.1 API URI 40

6.1.2 Usage of HTTP 40

6.1.2.1 General 40

6.1.2.2 HTTP standard headers 41

6.1.2.2.1 General 41

6.1.2.2.2 Content type 41

6.1.2.3 HTTP custom headers 41

6.1.2.3.1 General 41

6.1.2.4 HTTP multipart messages 41

6.1.2.5 HTTP/2 request retries 42

6.1.3 Resources 42

6.1.3.1 Overview 42

6.1.3.2 Resource: SM contexts collection 44

6.1.3.2.1 Description 44

6.1.3.2.2 Resource Definition 44

6.1.3.2.3 Resource Standard Methods 44

6.1.3.2.3.1 POST 44

6.1.3.2.4 Resource Custom Operations 46

6.1.3.3 Resource: Individual SM context 46

6.1.3.3.1 Description 46

6.1.3.3.2 Resource Definition 46

6.1.3.3.3 Resource Standard Methods 46

6.1.3.3.4 Resource Custom Operations 46

6.1.3.3.4.1 Overview 46

6.1.3.3.4.2 Operation: modify 46

6.1.3.3.4.2.1 Description 46

6.1.3.3.4.2.2 Operation Definition 46

6.1.3.3.4.3 Operation: release 47

6.1.3.3.4.3.1 Description 47

6.1.3.3.4.3.2 Operation Definition 47

6.1.3.3.4.4 Operation: retrieve 48

6.1.3.3.4.4.1 Description 48

6.1.3.3.4.4.2 Operation Definition 48

6.1.3.5 Resource: PDU sessions collection (H-SMF) 48

6.1.3.5.1 Description 48

6.1.3.5.2 Resource Definition 48

6.1.3.5.3 Resource Standard Methods 48

6.1.3.5.3.1 POST 48

6.1.3.5.4 Resource Custom Operations 50

6.1.3.5.4.1 Overview 50

6.1.3.6 Resource: Individual PDU session (H-SMF) 51

6.1.3.6.1 Description 51

6.1.3.6.2 Resource Definition 51

6.1.3.6.3 Resource Standard Methods 51

6.1.3.6.4 Resource Custom Operations 51

6.1.3.6.4.1 Overview 51

6.1.3.6.4.2 Operation: modify 51

6.1.3.6.4.2.1 Description 51

6.1.3.6.4.2.2 Operation Definition 51

6.1.3.6.4.3 Operation: release 52

6.1.3.6.4.3.1 Description 52

6.1.3.6.4.3.2 Operation Definition 52

6.1.3.7 Resource: Individual PDU session (V-SMF) 53

6.1.3.7.1 Description 53

6.1.3.7.2 Resource Definition 53

6.1.3.7.3 Resource Standard Methods 53

6.1.3.7.3.1 POST 53

6.1.3.7.4 Resource Custom Operations 54

6.1.3.7.4.1 Overview 54

6.1.3.7.4.2 Operation: modify 54

6.1.3.7.4.2.1 Description 54

6.1.3.7.4.2.2 Operation Definition 54

6.1.4 Custom Operations without associated resources 55

6.1.5 Notifications 55

6.1.5.1 General 55

6.1.5.2 SM Context Status Notification 56

6.1.5.2.1 Description 56

6.1.5.2.2 Notification Definition 56

6.1.6 Data Model 56

6.1.6.1 General 56

6.1.6.2 Structured data types 58

6.1.6.2.1 Introduction 58

6.1.6.2.2 Type: SmContextCreateData 59

6.1.6.2.3 Type: SMContextCreatedData 62

6.1.6.2.4 Type: SMContextUpdateData 63

6.1.6.2.5 Type: SMContextUpdatedData 66

6.1.6.2.6 Type: SMContextReleaseData 67

6.1.6.2.7 Type: SMContextRetrieveData 67

6.1.6.2.8 Type: SMContextStatusNotification 68

6.1.6.2.9 Type: PduSessionCreateData 69

6.1.6.2.10 Type: PduSessionCreatedData 72

6.1.6.2.11 Type: HsmfUpdateData 73

6.1.6.2.12 Type: HsmfUpdatedData 75

6.1.6.2.13 Type: ReleaseData 75

6.1.6.2.14 Type: HsmfUpdateError 76

6.1.6.2.15 Type: VsmfUpdateData 77

6.1.6.2.16 Type: VsmfUpdatedData 78

6.1.6.2.17 Type: StatusNotification 78

6.1.6.2.18 Type: QosFlowItem 79

6.1.6.2.19 Type: QosFlowSetupItem 79

6.1.6.2.20 Type: QosFlowAddModifyRequestItem 79

6.1.6.2.21 Type: QosFlowReleaseRequestItem 80

6.1.6.2.22 Type: QosFlowProfile 80

6.1.6.2.23 Type: GbrQosFlowInformation 81

6.1.6.2.24 Type: QosFlowNotifyItem 81

6.1.6.2.25 Type: Void 81

6.1.6.2.26 Type: Void 81

6.1.6.2.27 Type: SMContextRetrievedData 81

6.1.6.2.28 Type: TunnelInfo 82

6.1.6.2.29 Type: StatusInfo 82

6.1.6.2.30 Type: VsmfUpdateError 83

6.1.6.2.31 Type: EpsPdnCnxInfo 83

6.1.6.2.32 Type: EpsBearerInfo 84

6.1.6.2.33 Type: PduSessionNotifyItem 84

6.1.6.2.34 Type: EbiArpMapping 84

6.1.6.2.35 Type: SmContextCreateError 84

6.1.6.2.36 Type: SMContextUpdateError 85

6.1.6.2.37 Type: PduSessionCreateError 85

6.1.6.2.38 Type: MmeCapabilities 86

6.1.6.2.39 Type: Void 86

6.1.6.3 Simple data types and enumerations 86

6.1.6.3.1 Introduction 86

6.1.6.3.2 Simple data types 86

6.1.6.3.3 Enumeration: UpCnxState 87

6.1.6.3.4 Enumeration: HoState 87

6.1.6.3.5 Enumeration: RequestType 88

6.1.6.3.6 Enumeration: RequestIndication 88

6.1.6.3.7 Enumeration: NotificationCause 88

6.1.6.3.8 Enumeration: Cause 89

6.1.6.3.9 Enumeration: ResourceStatus 89

6.1.6.3.10 Enumeration: DnnSelectionMode 89

6.1.6.3.11 Enumeration: EpsInterworkingIndication 89

6.1.6.3.12 Enumeration: N2SmInfoType 90

6.1.6.4 Binary data 90

6.1.6.4.1 Introduction 90

6.1.6.4.2 N1 SM Message 90

6.1.6.4.3 N2 SM Information 91

6.1.6.4.4 n1SmInfoFromUe, n1SmInfoToUe, unknownN1SmInfo 92

6.1.7 Error Handling 93

6.1.7.1 General 93

6.1.7.2 Protocol Errors 93

6.1.7.3 Application Errors 93

6.1.8 Feature Negotiation 95

6.1.9 Security 95

Annex A (normative): OpenAPI specification 97

A.1 General 97

A.2 Nsmf\_PDUSession API 97

Annex B (Informative): HTTP Multipart Messages 125

B.1 Example of HTTP multipart message 125

B.1.1 General 125

B.1.2 Example HTTP multipart message with N1 SM Message binary data 125

Annex C (informative): Change history 126

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies the stage 3 protocol and data model for the Nsmf Service Based Interface. It provides stage 3 protocol definitions and message flows, and specifies the API for each service offered by the SMF other than the Session Management Event Exposure service.

The 5G System stage 2 architecture and procedures are specified in 3GPP TS 23.501 [2] and 3GPP TS 23.502 [3].

The Technical Realization of the Service Based Architecture and the Principles and Guidelines for Services Definition are specified in 3GPP TS 29.500 [4] and 3GPP TS 29.501 [5].

The Session Management Event Exposure Service is specified in 3GPP TS 29.508 [6].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[5] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[6] 3GPP TS 29.508: "5G System; Session Management Event Exposure Service; Stage 3".

[7] 3GPP TS 24.501: "Non-Access-Stratum (NAS) protocol for 5G System (5GS); Stage 3".

[8] 3GPP TS 24.007: "Mobile radio interface signalling layer 3; General aspects".

[9] 3GPP TS 38.413: "NG Radio Access Network (NG-RAN); NG Application Protocol (NGAP)".

[10] IETF RFC 2387: "The MIME Multipart/Related Content-type".

[11] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[12] IETF RFC 2045: "Multipurpose Internet Mail Extensions (MIME) Part One: Format of Internet Message Bodies".

[13] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[14] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2)".

[15] OpenAPI Initiative, "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>

[16] 3GPP TS 29.274: "3GPP Evolved Packet System (EPS); Evolved General Packet Radio Service (GPRS) Tunnelling Protocol for Control plane (GTPv2-C); Stage 3".

[17] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[18] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[19] 3GPP TS 29.510: "Network Function Repository Services; Stage 3".

[20] 3GPP TS 29.518: "5G System; Access and Mobility Management Service; Stage 3".

[21] 3GPP TS 23.380: "IMS Restoration Procedures".

[22] 3GPP TS 32.422: "Telecommunication management; Subscriber and equipment trace; Trace control and configuration management".

[23] IETF RFC 7807: "Problem Details for HTTP APIs".

[24] 3GPP TS 23.527: "5G System; Restoration Procedures".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

DNN Data Network Name

HR Home Routed

JSON Javascript Object NotationNAS Non-Access Stratum

LADN Local Area Data Network

SM Session Management

SMF Session Management Function

# 4 Overview

## 4.1 Introduction

Within the 5GC, the SMF offers services to the AMF, other SMF (V-SMF or H-SMF), PCF and NEF via the Nsmf service based interface (see 3GPP TS 23.501 [2] and 3GPP TS 23.502 [3]).

Figure 4.1-1 provides the reference model (in service based interface representation and in reference point representation), with focus on the SMF and the scope of the present specification.



Figure 4.1-1: Reference model – SMF

The functionalities supported by the SMF are listed in subclause 6.2.2 of 3GPP TS 23.501 [2].

# 5 Services offered by the SMF

## 5.1 Introduction

The SMF supports the following services.

Table 5.1-1: NF Services provided by SMF

| Service Name | Description | Example Consumer |
| --- | --- | --- |
| Nsmf\_PDUSession | This service manages the PDU sessions and uses the policy and charging rules received from the PCF. The service operations exposed by this NF service allows the consumer NFs to establish, modify and delete the PDU sessions. | V-SMF, H-SMF, AMF |
| Nsmf\_EventExposure | This service exposes the events happening on the PDU sessions to the consumer NFs. | PCF, NEF, AMF |

The Nsmf\_EventExposure service is specified in 3GPP TS 29.508 [6].

## 5.2 Nsmf\_PDUSession Service

### 5.2.1 Service Description

The Nsmf\_PDUSession service operates on the PDU Sessions. The service operations exposed by this service allow other NFs to establish, modify and release the PDU Sessions. The following are the key functionalities of this NF service:

- Creation, modification and deletion of SM contexts for PDU Sessions upon receiving N1 message notification from AMF carrying the NAS SM messages; an SM context represents an association between the NF Service Consumer (e.g. AMF) and the SMF for a PDU session;

- Retrieval of SM contexts of PDU sessions, e.g. to move PDU sessions towards the EPC using the N26 interface;

- Creation, modification and deletion of PDU sessions between the V-SMF and H-SMF, in HR roaming scenarios;

- Association of policy and charging rules with PDU Sessions and binding the policy and charging rules to flows;

- Interacting with the UPF over N4 for creating, modifying and releasing user plane sessions;

- Process user plane events from the UPF and apply the corresponding policy and charging rules.

The Nsmf\_PDUSession service supports the following service operations.

Table 5.2.1-1: Service operations supported by the Nsmf\_PDUSession service

|  |  |  |  |
| --- | --- | --- | --- |
| Service Operations | Description | Operation  Semantics | Example Consumer(s) |
| Create SM Context | Create an SM context in SMF, or in V-SMF in HR roaming scenarios, for a PDU session. | Request/Response | AMF |
| Update SM Context | Update the SM context of a PDU session and/or provide the SMF with N1 or N2 SM information received from the UE or from the AN. | Request/Response | AMF |
| Release SM Context | Release the SM context of a PDU session when the PDU session has been released. | Request/Response | AMF |
| Notify SM Context Status  (see NOTE 1) | Notify the NF Service Consumer about the status of an SM Context of a PDU session (e.g. the SM Context is released within the SMF). | Subscribe/Notify | AMF |
| Retrieve SM Context  (see NOTE 2) | Retrieve an SM context of a PDU session from SMF, or from V-SMF in HR roaming scenarios, for 5GS to EPS mobility. | Request/Response | AMF |
| Create | Create a PDU session in the H-SMF, in HR roaming scenarios. | Request/Response | V-SMF |
| Update | Update a PDU session in the H-SMF or V-SMF, in HR roaming scenarios. | Request/Response | V-SMF, H-SMF |
| Release | Release a PDU session in the H-SMF, in HR roaming scenarios. | Request/Response | V-SMF |
| Notify Status  (see NOTE 3) | Notify the NF Service Consumer about the status of a PDU session (e.g. the PDU session is released due to local reasons within the H-SMF). | Subscribe/Notify | V-SMF |
| NOTE 1: This corresponds to the SMContextStatusNotify service operation defined in 3GPP TS 23.502 [3].  NOTE 2: This corresponds to the ContextRequest service operation defined in 3GPP TS 23.502 [3].  NOTE 3: This corresponds to the StatusNotify service operation defined in 3GPP TS 23.502 [3]. | | | |

### 5.2.2 Service Operations

#### 5.2.2.1 Introduction

See Table 5.2.1-1 for an overview of the service operations supported by the Nsmf\_PDUSession service.

#### 5.2.2.2 Create SM Context service operation

##### 5.2.2.2.1 General

The Create SM Context service operation shall be used to create an individual SM context, for a given PDU session, in the SMF, or in the V-SMF for HR roaming scenarios.

It is used in the following procedures:

- UE requested PDU Session Establishment (see subclause 4.3.2 of 3GPP TS 23.502 [3]);

- EPS to 5GS Idle mode mobility or handover using N26 interface (see subclause 4.11 of 3GPP TS 23.502 [3]);

- EPS to 5GS mobility without N26 interface (see subclause 4.11.2.3 3GPP TS 23.502 [3]);

- Handover of a PDU session between 3GPP access and non-3GPP access, when the target AMF does not know the SMF resource identifier of the SM context used by the source AMF, e.g. when the target AMF is not in the PLMN of the N3IWF (see subclause 4.9.2.3.2 of 3GPP TS 23.502 [3]), or when the UE is roaming and the selected N3IWF is in the HPLMN (see subclause 4.9.2.4.2 of 3GPP TS 23.502 [3]);

- Handover from EPS to 5GC-N3IWF (see subclause 4.11.3.1 of 3GPP TS 23.502 [3]);

- Handover from EPC/ePDG to 5GS (see subclause 4.11.4.1 of 3GPP TS 23.502 [3]).

There shall be only one individual SM context per PDU session.

The NF Service Consumer (e.g. AMF) shall create an SM context by using the HTTP POST method as shown in Figure 5.2.2.2.1-1.



Figure 5.2.2.2.1-1: SM context creation

1. The NF Service Consumer shall send a POST request to the resource representing the SM contexts collection resource of the SMF. The payload body of the POST request shall contain:

- a representation of the individual SM context resource to be created;

- the Request Type IE, if it is received from the UE and if the request refers to an existing PDU session or an existing Emergency PDU session; the Request Type IE may be included otherwise;

- the Old PDU Session ID, if it is received from the UE (i.e. for a PDU session establishment for the SSC mode 3 operation);

- the indication that the UE is inside or outside of the LADN (Local Area Data Network) service area, if the DNN corresponds to a LADN;

- a subscription for SM context status notification;

- the amfId identifying the serving AMF;

- trace control and configuration parameters, if trace is to be activated (see 3GPP TS 32.422 [22]).

For the UE requested PDU Session Establishment procedure in home routed roaming scenario (see subclause 4.3.2.2.2 of 3GPP TS 23.502 [3]), the NF Service Consumer shall provide the URI of the Nsmf\_PDUSession service of the H-SMF in the hSmfUri IE and may provide the URI of the Nsmf\_PDUSession service of additional H-SMFs. The V-SMF shall try to create the PDU session using the hSmfUri IE. If due to communication failure on the N16 interface the V-SMF does not receive any response from the H-SMF, then:

- depending on operator policy, the V-SMF may try reaching the hSmfUri via an alternate path; or

- if additional H-SMF URI is provided, the V-SMF may try to create the PDU session on one of the additional H-SMF(s) provided.

The payload body of the POST request may further contain:

- the name of the AMF service to which SM context status notification are to be sent (see subclause 6.5.2.2 of 3GPP TS 29.500 [4]), encoded in the serviceName attribute.

2a. On success, "201 Created" shall be returned, the payload body of the POST response shall contain the representation describing the status of the request and the "Location" header shall be present and shall contain the URI of the created resource. The authority and/or deployment-specific string of the apiRoot of the created resource URI may differ from the authority and/or deployment-specific string of the apiRoot of the request URI received in the POST request.  
  
If the Request Type was received in the request and indicates this is a request for an existing PDU session or an existing emergency PDU session, the SMF shall identify the existing PDU session or emergency PDU session based on the PDU Session ID; in this case, the SMF shall not create a new SM context but instead update the existing SM context and provide the representation of the updated SM context in the "201 Created" response to the NF Service Consumer.

The POST request shall be considered as colliding with an existing SM context if:

- it includes the same SUPI, or PEI for an emergency registered UE without a UICC or without an authenticated SUPI, and the same PDU Session ID as for an existing SM context; and

- this is a request to establish a new PDU session, i.e. the RequestType is absent in the request or is present and set to INITIAL\_REQUEST or INITIAL\_EMERGENCY\_REQUEST.

A POST request that collides with an existing SM context shall be treated as a request for a new SM context. Before creating the new SM context, the SMF should delete the existing SM context locally and any associated resources in the UPF and PCF. If the smContextStatusUri of the existing SM context differs from the smContextStatusUri received in the POST request, the SMF shall also send an SM context status notification (see subclause 5.2.2.5) targeting the smContextStatusUri of the existing SM context to notify the release of the existing SM context. For a HR PDU session, if the H-SMF URI in the request is different from the H-SMF URI of the existing PDU session, the V-SMF should also delete the existing PDU session in the H-SMF by invoking the Release service operation (see subclause 5.2.2.9).

If the Request Type was received in the request and indicates this is a request for a new PDU session (i.e. INITIAL\_REQUEST) and if the Old PDU Session ID was also included in the request, the SMF shall identify the existing PDU session to release and to which the new PDU session establishment relates, based on the Old PDU Session ID.

2b. If the request does not include the "UE presence in LADN service area" indication and the SMF determines that the DNN corresponds to a LADN, then the SMF shall consider that the UE is outside of the LADN service area. The SMF shall reject the request if the UE is outside of the LADN service area.

On failure, or redirection during a UE requested PDU Session Establishment, one of the HTTP status code listed in Table 6.1.3.2.3.1-3 shall be returned. For a 4xx/5xx response, the message body shall contain an SmContextCreateError structure, including:

- a ProblemDetails structure with the "cause" attribute set to one of the application error listed in Table 6.1.3.2.3.1-3;

- N1 SM information (PDU Session Reject), if the request included N1 SM information, except if the error prevents the SMF from generating a response to the UE (e.g. invalid request format).

##### 5.2.2.2.2 EPS to 5GS Idle mode mobility using N26 interface

The NF Service Consumer (e.g. AMF) shall request the SMF to move a UE EPS PDN connection to 5GS using N26 interface, as follows.



Figure 5.2.2.2.2-1: EPS to 5GS Idle mode mobility using N26 interface

1. The NF Service Consumer shall send a POST request, as specified in subclause 5.2.2.2.1, with the following additional information:

- UE EPS PDN connection, including the EPS bearer contexts, received from the MME, representing the individual SM context resource to be created;

- pduSessionsActivateList, including the PDU Session ID of all the PDU session(s) to be re-activated.

2a. Upon receipt of such a request, if a corresponding PDU session is found based on the EPS bearer contexts (after invoking a Create service operation towards the H-SMF, for a Home Routed PDU session) and if it is possible to proceed with moving the PDN connection to 5GS, the SMF shall return a 201 Created response including the following information:

- PDU Session ID corresponding to the default EPS bearer ID of the EPS PDN connection;

- allocatedEbiList, containing the EBI(s) allocated to the PDU session;

and, if the PDU session was requested to be re-activated, i.e. if the PDU Session ID was present in the pduSessionsActivateList:

- upCnxState attribute set to ACTIVATING;

- N2 SM information to request the 5G-AN to assign resources to the PDU session (see PDU Session Resource Setup procedure in subclause 8.2.1 of 3GPP TS 38.413 [9]), including the transport layer address and tunnel endpoint of the uplink termination point for the user plane data for this PDU session (i.e. UPF's GTP-U F-TEID for uplink traffic).

The "Location" header shall be present in the POST response and shall contain the URI of the created SM context resource.  
  
The NF Service Consumer (e.g. AMF) shall store the association of the PDU Session ID and the SMF ID, and store the allocated EBI(s) associated to the PDU Session ID.

NOTE: The behaviour specified in this step also applies if the POST request collides with an existing SM context, i.e. if the POST request includes the same SUPI, or PEI for an emergency registered UE without a UICC or without an authenticated SUPI, and the default EPS bearer ID received in the UE EPS PDN connection is the same as in the existing SM context.

2b. Same as step 2b of figure 5.2.2.2.1-1. Steps 3 to 4 are skipped in this case.

If the SMF determines that seamless session continuity from EPS to 5GS is not supported for the PDU session, the SMF shall set the "cause" attribute in the ProblemDetails structure to "NO\_EPS\_5GS\_CONTINUITY".

3. Same as step 3 of figure 5.2.2.3.2.2-1, if the SMF returned a 201 Created response with the upConnectionState set to ACTIVATING and N2 SM Information,

4. Same as step 4 of figure 5.2.2.3.2.2-1.

##### 5.2.2.2.3 EPS to 5GS Handover Preparation using N26 interface

The NF Service Consumer (e.g. AMF) shall request the SMF to handover a UE EPS PDN connection to 5GS using N26 interface, as follows.



Figure 5.2.2.2.3-1: EPS to 5GS handover using N26 interface

1. The NF Service Consumer shall send a POST request, as specified in subclause 5.2.2.2.1, with the following additional information:

- UE EPS PDN connection, including the EPS bearer contexts, representing the individual SM context resource to be created;

- hoState attribute set to PREPARING (see subclause 5.2.2.3.4.1);

2a. Upon receipt of such a request, if a corresponding PDU session is found based on the EPS bearer contexts (after invoking a Create service operation towards the H-SMF, for a Home Routed PDU session) and it is possible to proceed with handing over the PDN connection to 5GS, the SMF shall return a 201 Created response including the following information:

- hoState attribute set to PREPARING and N2 SM information to request the target 5G-AN to assign resources to the PDU session, as specified in step 2 of Figure 5.2.2.3.4.2-1;

- PDU Session ID corresponding to the default EPS bearer ID of the EPS PDN connection;

The "Location" header shall be present in the POST response and shall contain the URI of the created SM context resource.  
  
The NF Service Consumer (e.g. AMF) shall store the association of the PDU Session ID and the SMF ID, and store the allocated EBI(s) associated to the PDU Session ID.

NOTE: The behaviour specified in this step also applies if the POST request collides with an existing SM context, i.e. if the POST request includes the same SUPI, or PEI for an emergency registered UE without a UICC or without an authenticated SUPI, and the default EPS bearer ID received in the UE EPS PDN connection is the same as in the existing SM context.

2b. Same as step 2b of figure 5.2.2.2.1-1 with the following additions. Steps 3 to 4' are skipped in this case.

The error response shall include the following additional information:

- hoState attribute set to NONE.

If the SMF determines that seamless session continuity from EPS to 5GS is not supported for the PDU session, the SMF shall set the "cause" attribute in the ProblemDetails structure to "NO\_EPS\_5GS\_CONTINUITY".

#### 5.2.2.3 Update SM Context service operation

##### 5.2.2.3.1 General

The Update SM Context service operation shall be used to update an individual SM context and/or provide N1 or N2 SM information received from the UE or the AN, for a given PDU session, towards the SMF, or the V-SMF for HR roaming scenarios.

It is used in the following procedures:

- PDU Session modification (see subclause 4.3.3 of 3GPP TS 23.502 [3]);

- UE requested PDU session release (see subclause 4.3.4.2 and subclause 4.3.4.3 of 3GPP TS 23.502 [3]);

- Activation or Deactivation of the User Plane connection of an existing PDU session, i.e. establishment or release of the N3 tunnel between the AN and serving CN (see subclause 5.6.8 of 3GPP TS 23.501 [2] and subclauses 4.2.3 and 4.2.6 of 3GPP TS 23.502 [3]);

- Xn and N2 Handover procedures (see subclauses 4.9.1 of 3GPP TS 23.502 [3]);

- Handover between 3GPP and untrusted non-3GPP access procedures (see subclause 4.9.2 of 3GPP TS 23.502 [3]);

- Inter-AMF change due to AMF planned maintenance or AMF failure (see subclause 5.21.2 of 3GPP TS 23.501 [2]), or inter-AMF mobility in CM-IDLE mode (see subclause 4.2.2.2 of 3GPP TS 23.502 [3]);

- RAN Initiated QoS Flow Mobility (see subclause 4.14.1 of 3GPP TS 23.502 [3] and subclause 8.2.5 of 3GPP TS 38.413 [9]);

- All procedures requiring to provide N1 or N2 SM information to the SMF, e.g. UE requested PDU Session Establishment procedure (see subclause 4.3.2.2 of 3GPP TS 23.502 [3]);

- EPS to 5GS Idle mode mobility or handover using N26 interface (see subclause 4.11 of 3GPP TS 23.502 [3]);

- 5GS to EPS Handover using N26 interface (see subclause 4.11.1.2 of 3GPP TS 23.502 [3]);

- PDU Session Reactivation during P-CSCF Restoration procedure via AMF (see subclause 5.8.4.3 of 3GPP TS 23.380 [21]).

The NF Service Consumer (e.g. AMF) shall update an individual SM context and/or provide N1 or N2 SM information to the SMF by using the HTTP POST method (modify custom operation) as shown in Figure 5.2.2.3.1-1.



Figure 5.2.2.3.1-1: SM context update

1. The NF Service Consumer shall send a POST request to the resource representing the individual SM context resource in the SMF. The payload body of the POST request shall contain the modification instructions and/or the N1 or N2 SM information.

2a. On success, "204 No Content" or "200 OK" shall be returned; in the latter case, the payload body of the POST response shall contain the representation describing the status of the request and/or N1 or N2 SM information.

The SMF may indicate to the NF Service Consumer that it shall release EBI(s) that were assigned to the PDU session by including the releaseEbiList IE, e.g. when a QoS flow is released.

2b. On failure, one of the HTTP status code listed in Table 6.1.3.3.3.2-3 shall be returned. For a 4xx/5xx response, the message body shall contain an SmContextUpdateError structure, including:

- a ProblemDetails structure with the "cause" attribute set to one of the application error listed in Table 6.1.3.3.3.2-3;

- N1 SM information, if the SMF needs and can return a response to the UE;

- N2 SM information, if the SMF needs and can return a response to the NG-RAN.

The following subclauses specify additional requirements applicable to specific scenarios.

##### 5.2.2.3.2 Activation and Deactivation of the User Plane connection of a PDU session

###### 5.2.2.3.2.1 General

The upCnxState attribute of an SM context represents the state of the UP connection of the PDU session. The upCnxState attribute may take the following values:

- ACTIVATED: a N3 tunnel is established between the 5G-AN and UPF (F-TEIDs assigned for both uplink and downlink traffic);

- DEACTIVATED: no N3 tunnel is established between the 5G-AN and UPF;

- ACTIVATING: a N3 tunnel is being established (5G-AN's F-TEID for downlink traffic is not assigned yet).

###### 5.2.2.3.2.2 Activation of User Plane connectivity of a PDU session

The NF Service Consumer (e.g. AMF) shall request the SMF to activate the User Plane connection of an existing PDU session, i.e. establish the N3 tunnel between the 5G-AN and UPF, as follows.



Figure 5.2.2.3.2.2-1: Activation of the User Plane connection of a PDU session

1. The NF Service Consumer shall request the SMF to activate the user plane connection of the PDU session by sending a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- the upCnxState attribute set to ACTIVATING;

- the user location and access type associated to the PDU session, if modified;

- the indication that the UE is inside or outside of the LADN service area, if the DNN of the established PDU session corresponds to a LADN;

- other information, if necessary.

2a. Upon receipt of such a request, if the SMF can proceed with activating the user plane connection of the PDU session (see subclause 4.2.3 of 3GPP TS 23.501 [2], the SMF shall set the upCnxState attribute to ACTIVATING and shall return a 200 OK response including the following information:

- upCnxState attribute set to ACTIVATING;

- N2 SM information to request the 5G-AN to assign resources to the PDU session (see PDU Session Resource Setup procedure in subclause 8.2.1 of 3GPP TS 38.413 [9]), including the transport layer address and tunnel endpoint of the uplink termination point for the user plane data for this PDU session (i.e. UPF's GTP-U F-TEID for uplink traffic).

If the SMF finds the PDU session already activated when receiving the request in step 1, the SMF shall delete the N3 tunnel information and update the UPF accordingly (see step 8a of subclause 4.2.3.2 of 3GPP TS 23.502 [3]).

2b. If the request does not include the "UE presence in LADN service area" indication and the SMF determines that the DNN corresponds to a LADN, then the SMF shall consider that the UE is outside of the LADN service area. The SMF shall reject the request if the UE is outside of the LADN service area.

If the SMF cannot proceed with activating the user plane connection of the PDU session (e.g. if the PDU session corresponds to a PDU session of SSC mode 2 and the SMF decides to change the PDU Session Anchor), the SMF shall return an error response, as specified for step 2b of figure 5.2.2.3.1-1. For a 4xx/5xx response, the SmContextUpdateError structure shall include the following additional information:

- upCnxState attribute set to DEACTIVATED.

3. If the SMF returned a 200 OK response, the NF Service Consumer (e.g. AMF) shall subsequently update the SM context in the SMF by sending POST request, as specified in subclause 5.2.2.3.1, with the following information:

- N2 SM information received from the 5G-AN, including the transport layer address and tunnel endpoint of the downlink termination point for the user data for this PDU session (i.e. 5G-AN's GTP-U F-TEID for downlink traffic), if the 5G-AN succeeded in establishing resources for the PDU sessions; or

- N2 SM information including the Cause of the failure, if resources failed to be established for the PDU sessions.

Upon receipt of this request, the SMF shall:

- update the UPF with the 5G-AN's F-TEID and set the upCnxState attribute to ACTIVATED, if the 5G-AN succeeded in establishing resources for the PDU sessions; or

- consider that the activation of the UP connection has failed and set the upCnxState attribute to DEACTIVATED" otherwise.

4. The SMF shall then return a 200 OK response including the upCnxState attribute representing the final state of the user plane connection.

###### 5.2.2.3.2.3 Deactivation of User Plane connectivity of a PDU session

The NF Service Consumer (e.g. AMF) shall request the SMF to deactivate the User Plane connectivity of an existing PDU session, i.e. release the N3 tunnel, as follows.



Figure 5.2.2.3.2.2-1: Deactivation of the User Plane connection of a PDU session

1. The NF Service Consumer shall request the SMF to deactivate the user plane connection of the PDU session by sending a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- upCnxState attribute set to DEACTIVATED;

- user location and user location timestamp;

- cause of the user plane deactivation; the cause may indicate a cause received from the 5G-AN or due to an AMF internal event;

- other information, if necessary.

2. Upon receipt of such a request, the SMF shall deactivate release the N3 tunnel of the PDU session, set the upCnxState attribute to DEACTIVATED and return a 200 OK response including the upCnxState attribute set to DEACTIVATED.

##### 5.2.2.3.3 Xn Handover

The NF Service Consumer (e.g. AMF) shall request the SMF to switch the downlink N3 tunnel of the PDU session towards a new GTP tunnel endpoint as follows.



Figure 5.2.2.3.3-1: Xn handover

1. The NF Service Consumer shall request the SMF to switch the downlink N3 tunnel of the PDU session towards a new GTP tunnel endpoint by sending a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- the indication that the PDU session is to be switched;

- N2 SM information received from the 5G-AN (see PDU Session Path Switch Request Transfer IE in subclause 9.3.1.21 of 3GPP TS 38.413 [9]), including the new transport layer address and tunnel endpoint of the downlink termination point for the user data for this PDU session (i.e. 5G-AN's GTP-U F-TEID for downlink traffic);

- the user location associated to the PDU session;

- the indication that the UE is inside or outside of the LADN service area, if the DNN of the established PDU session corresponds to a LADN;

- other information, if necessary.

2a. Upon receipt of such a request, if the SMF can proceed with switching the user plane connection of the PDU session, the SMF shall return a 200 OK response including the following information:

- N2 SM information (see PDU Session Path Switch Request Ack Transfer IE in subclause 9.3.1.22 of 3GPP TS 38.413 [9]), including the transport layer address and tunnel endpoint of the uplink termination point for the user data for this PDU session (i.e. UPF's GTP-U F-TEID for uplink traffic).

If the request does not include the "UE presence in LADN service area" indication and the SMF determines that the DNN corresponds to a LADN, then the SMF shall consider that the UE is outside of the LADN service area. The SMF shall proceed as specified in subclause 5.6.5 of 3GPP TS 23.501 [2].

2b. Same as step 2b of figure 5.2.2.3.1-1.

For a PDU session that is rejected by the target RAN (i.e. a PDU session indicated as failed to setup in the PATH SWITCH REQUEST), the NF Service Consumer (e.g. AMF) shall indicate the failure to setup the PDU session in the target RAN as follows.



Figure 5.2.2.3.3-2: Xn handover – PDU session rejected by the target RAN

1. The NF Service Consumer shall indicate to the SMF that the PDU session could not be setup in the target RAN by sending a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- the indication that the PDU session failed to be switched;

- N2 SM information received from the 5G-AN (see PDU Session Path Switch Request Setup Failed Transfer IE in subclause 9.3.4.15 of 3GPP TS 38.413 [9]), including the cause why the session could not be setup;

- other information, if necessary.

2a. Upon receipt of such a request, the SMF shall return a "204 No Content" response. The SMF shall decide whether to release the PDU session or deactivate the user plane connection of the PDU session, as specified in subclause 4.9.1.2 of 3GPP TS 23.502 [3].

2b. Same as step 2b of figure 5.2.2.3.1-1.

##### 5.2.2.3.4 N2 Handover

###### 5.2.2.3.4.1 General

The hoState attribute of an SM context represents the handover state of the PDU session. The hoState attribute may take the following values:

- NONE: no handover is in progress for the PDU session;

- PREPARING: a handover is in preparation for the PDU session; SMF is preparing the N3 tunnel between the target 5G-AN and UPF, i.e. the UPF's F-TEID is assigned for uplink traffic;

- PREPARED: a handover is prepared for the PDU session; SMF is updated for the N3 tunnel between the target 5G-AN and UPF, with the target 5G-AN's F-TEID to be assigned for downlink traffic upon handover execution;

- COMPLETED: the handover is completed (successfully);

- CANCELLED: the handover is cancelled.

###### 5.2.2.3.4.2 N2 Handover Preparation

The NF Service Consumer (e.g. AMF) shall request the SMF to prepare the handover of an existing PDU session, i.e. prepare the N3 tunnel between the target 5G-AN and UPF, as follows.



Figure 5.2.2.3.4.2-1: N2 Handover Preparation

1. The NF Service Consumer shall request the SMF to prepare the handover of the PDU session by sending a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- updating the hoState attribute of the individual SM Context resource in the SMF to PREPARING;

- target user location (e.g. target TAI or target RAN ID);

- Target AMF ID, for a N2 handover with AMF change;

- other information, if necessary.

2a. Upon receipt of such a request, if the SMF can proceed with preparing the handover of the PDU session (see subclause 4.9.1.3 of 3GPP TS 23.501 [2]), the SMF shall set the hoState attribute to PREPARING and shall return a 200 OK response including the following information:

- hoState attribute set to PREPARING;

- N2 SM information to request the target 5G-AN to assign resources to the PDU session (see Handover Preparation procedure in subclause 8.4.1 of 3GPP TS 38.413 [9]), including (among others) the transport layer address and tunnel endpoint of the uplink termination point for the user plane data for this PDU session (i.e. UPF's GTP-U F-TEID for uplink traffic).

The SMF shall store the Target AMF ID, if received in the request, but the SMF shall still consider the AMF (previously) received in the amfId IE as the serving AMF for the UE.

2b. If the SMF cannot proceed with preparing the handover of the PDU session (e.g. the UE moves into a non-allowed service area), the SMF shall return an error response, as specified in step 2b of figure 5.2.2.3.1-1. For a 4xx/5xx response, the SmContextUpdateError structure shall include the following additional information:

- hoState attribute set to NONE.

3. If the SMF returned a 200 OK response, the NF Service Consumer (e.g. AMF) shall subsequently update the SM context in the SMF by sending POST request, as specified in subclause 5.2.2.3.1, with the following information:

- hoState attribute set to PREPARED;

- N2 SM information received from the target 5G-AN, including the transport layer address and tunnel endpoint of the downlink termination point for the user data for this PDU session (i.e. target 5G-AN's GTP-U F-TEID for downlink traffic), if the target 5G-AN succeeded in establishing resources for the PDU session;

- N2 SM information including the Cause of the failure, if resources failed to be established for the PDU sessions.

4a. If the 5G-AN succeeded in establishing resources for the PDU sessions, the SMF shall set the hoState attribute to PREPARED and return a 200 OK response including the following information:

- hoState attribute to PREPARED;

- N2 SM information containing DL forwarding tunnel information to be sent to the source 5G-AN by the AMF (see step 11f of subclause 4.9.1.3.2 of 3GPP TS 23.502 [3]).

If indirect data forwarding applies, the SMF shall start an indirect data forwarding timer, to be used to release the resource of indirect data forwarding tunnel.

4b. If the SMF cannot proceed with preparing the handover of the PDU session (e.g. the target 5G-AN failed to establish resources for the PDU session), the SMF shall set the hoState to NONE, release resources reserved for the handover to the target 5G-AN, and return an error response as specified in step 2b of figure 5.2.2.3.1-1. For a 4xx/5xx response, the SmContextUpdateError structure shall include the following additional information:

- hoState attribute set to NONE.

###### 5.2.2.3.4.3 N2 Handover Execution

The NF Service Consumer (e.g. AMF) shall request the SMF to complete the execution the handover of an existing PDU session, upon being notified by the target 5G-AN that the handover to the target 5G-AN has been successful, as follows.



Figure 5.2.2.3.4.3-1: N2 Handover Execution

1. The NF Service Consumer shall request the SMF to complete the execution of the handover of the PDU session by sending a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- updating the hoState attribute of the individual SM Context resource in the SMF to COMPLETED;

- amfId set to the new serving AMF Id, for a N2 handover with AMF change;

- the indication that the UE is inside or outside of the LADN service area, if the DNN of the established PDU session corresponds to a LADN;

- other information, if necessary.

2. Upon receipt of such a request, the SMF shall return a 200 OK response including the following information:

- hoState attribute set to COMPLETED.

The SMF shall complete the execution of the handover, e.g. switch the PDU session towards the downlink termination point for the user data received from the target 5G-AN (i.e. target 5G-AN's GTP-U F-TEID for downlink traffic), set the hoState to NONE and delete any stored Target AMF ID.

If the request does not include the "UE presence in LADN service area" indication and the SMF determines that the DNN corresponds to a LADN, then the SMF shall consider that the UE is outside of the LADN service area. The SMF shall proceed as specified in subclause 5.6.5 of 3GPP TS 23.501 [2].

###### 5.2.2.3.4.4 N2 Handover Cancellation

The NF Service Consumer (e.g. AMF) shall request the SMF to cancel the handover of an existing PDU session, e.g. upon receipt of such a request from the source 5G-AN, as follows.



Figure 5.2.2.3.4.3-1: N2 Handover Cancellation

1. The NF Service Consumer shall request the SMF to complete the execution of the handover of the PDU session by sending a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- updating the hoState attribute of the individual SM Context resource in the SMF to CANCELLED;

- cause information;

- other information, if necessary.

2. Upon receipt of such a request, the SMF return a 200 OK response including the following information:

- hoState attribute set to CANCELLED.

The SMF shall cancel the execution of the handover, e.g. release resources reserved for the handover to the target 5G-AN, set the hoState to NONE and delete any stored Target AMF ID.

##### 5.2.2.3.5 Handover between 3GPP and untrusted non-3GPP access procedures

###### 5.2.2.3.5.1 General

The handover of a PDU session between 3GPP and untrusted non-3GPP access shall be supported as specified in subclause 4.9.2 of 3GPP TS 23.502 [3]. Such a handover may involve:

- the same AMF, or a target AMF in the same PLMN as the source AMF (see subclauses 4.9.2.1, 4.9.2.2, 4.9.2.3.1 and 4.9.2.4.1 of 3GPP TS 23.502 [3]); or

- a target AMF in a different PLMN than the source AMF (see subclauses 4.9.2.3.2 and 4.9.2.4.2 of 3GPP TS 23.502 [3]).

For a Home-Routed PDU session, the target AMF may be located in the VPLMN, or in the HPLMN when the N3IWF is in the HPLMN.

###### 5.2.2.3.5.2 Handover of a PDU session without AMF change or with target AMF in same PLMN

In these scenarios, the same V-SMF is used before and after the handover.

The NF Service Consumer (e.g. AMF) shall request the SMF to handover an existing PDU session from 3GPP access to untrusted non-3GPP access, or vice-versa, as follows.



Figure 5.2.2.3.5.2-1: Handover between 3GPP and untrusted non-3GPP access

1. The NF Service Consumer shall request the SMF to handover an existing PDU session from 3GPP access to untrusted non-3GPP access, or vice-versa, by sending a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- updating the anType attribute of the individual SM Context resource in the SMF to the target access type, i.e. to 3GPP\_ACCESS or NON\_3GPP\_ACCESS;

- other information, if necessary.

2a. Same as step 2a of Figure 5.2.2.3.1-1.

2b. If the SMF cannot proceed with handing over the PDU session to the target access type, the SMF shall return an error response, as specified for step 2b of figure 5.2.2.3.1-1. For a 4xx/5xx response, the SmContextUpdateError structure shall include the following additional information:

- N1 SM Information to reject the UE request.

##### 5.2.2.3.6 Inter-AMF change or mobility

The NF Service Consumer (e.g. new AMF) shall inform the SMF that it has taken over the role of serving the UE (e.g. it has taken the responsibility of the signalling towards the UE), when so required by 3GPP TS 23.501 [2] and 3GPP TS 23.502 [3], as follows.



Figure 5.2.2.3.6-1: Inter-AMF change or mobility

1. The NF Service Consumer shall update the SMF with the new serving AMF, by sending a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- amfId set to the new serving AMF Id;

- other information, if necessary, e.g. to activate the user plane connection of the PDU session (see subclause 5.2.2.3.2.2).

2a. Same as step 2a of Figure 5.2.2.3.1-1.

2b. Same as step 2b of figure 5.2.2.3.1-1.

##### 5.2.2.3.7 RAN Initiated QoS Flow Mobility

The NF Service Consumer (e.g. AMF) shall request the SMF to transfer QoS flows to and from Secondary RAN node, or more generally, handle a NG-RAN PDU Session Resource Modify Indication, as follows.



Figure 5.2.2.3.7-1: RAN Initiated QoS Flow Mobility

1. The NF Service Consumer shall request the SMF to modify the PDU session, as requested by the NG-RAN, by sending a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- N2 SM information received from the 5G-AN (see PDU Session Resource Modify Indication Transfer IE in subclause 9.3.1.19 of 3GPP TS 38.413 [9]), including the transport layer information for the QoS flows of this PDU session (i.e. 5G-AN's GTP-U F-TEIDs for downlink traffic);

- other information, if necessary.

2a. Upon receipt of such a request, if the SMF can proceed with switching the QoS flows of the PDU session, the SMF shall return a 200 OK response including the following information:

- N2 SM information (see PDU Session Resource Modify Confirm Transfer IE in subclause 9.3.1.20 of 3GPP TS 38.413 [9]), including the list of QoS flows which were modified successfully.

2b. If the SMF cannot proceed with switching the QoS flows of the PDU session, the SMF shall return an error response, as specified for step 2b of figure 5.2.2.3.1-1, including:

- N2 SM information (see PDU Session Resource Modify Confirm Transfer IE in subclause 9.3.1.20 of 3GPP TS 38.413 [9]), including the list of QoS flows which failed to be modified.

##### 5.2.2.3.8 EPS to 5GS Handover using N26 interface

###### 5.2.2.3.8.1 General

The NF Service Consumer (e.g. AMF) shall request the SMF to handover a UE EPS PDN connection to 5GS using N26 interface, following the same requirements as specified for N2 handover in subclause 5.2.2.3.4 with the modifications specified in this subclause.

###### 5.2.2.3.8.2 EPS to 5GS Handover Preparation

The requirements specified in subclause 5.2.2.3.4.2 shall apply with the following modifications.



Figure 5.2.2.3.8.2-1: EPS to 5GS Handover Preparation

1. Same as step 1 of Figure 5.2.2.2.3-1.

2a. Same as step 2 of Figure 5.2.2.2.3-1.

2b. Same as step 2b of figure 5.2.2.3.1-1.

3. Same as step 3 of Figure 5.2.2.3.4.2-1.

4a. Same as step 4 of Figure 5.2.2.3.4.2-1, with the following modifications:  
  
The 200 OK response shall not include N2 SM information for DL forwarding tunnel setup, but shall additionally contain:

- the epsBearerSetup IE(s), containing the list of EPS bearer context(s) successfully handed over to the 5GS and the CN tunnel information for data forwarding, generated based on the list of accepted QFI(s) received from the 5G-RAN;

4b. Same as step 2b of figure 5.2.2.3.1-1.

###### 5.2.2.3.8.3 EPS to 5GS Handover Execution

The requirements specified in subclause 5.2.2.3.4.3 shall apply, with the following modifications.

In step 2 of Figure 5.2.2.3.4.3-1, for a Home Routed PDU session, the SMF shall complete the execution of the handover by initiating an Update service operation towards the H-SMF in order to switch the PDU session towards the V-UPF (see subclause 5.2.2.8.2.3).

###### 5.2.2.3.8.4 EPS to 5GS Handover Cancellation

The requirements specified in subclause 5.2.2.3.4.4 shall apply.

##### 5.2.2.3.9 5GS to EPS Handover using N26 interface

The NF Service Consumer (e.g. AMF) shall request the SMF to establish indirect data forwarding tunnels during a 5GS to EPS handover, as follows.



Figure 5.2.2.3.9-1: 5GS to EPS Handover using N26 interface (data forwarding tunnels setup)

1. The NF Service Consumer shall send a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- dataForwarding IE set to true;

- EPS bearer contexts received from the MME in the Forward Relocation Response.

2a. Upon receipt of such a request, the SMF shall map the EPS bearers for Data Forwarding to the 5G QoS flows based on the association between the EPS bearer ID(s) and QFI(s) for the QoS flow(s), and shall return a 200 OK response including the following information:

- N2 SM information providing the 5G-AN with the CN transport layer address and tunnel endpoint (i.e. UPF's GTP-U F-TEID) for Data Forwarding and the QoS flows for Data Forwarding for this PDU session.

2b. If the SMF cannot proceed with the request, the SMF shall return an error response, as specified for step 2b of figure 5.2.2.3.1-1.

The NF Service Consumer (e.g. AMF) shall request the SMF to release indirect data forwarding tunnels, as follows.



Figure 5.2.2.3.9-2: 5GS to EPS Handover using N26 interface (data forwarding tunnels release)

1. The NF Service Consumer shall send a POST request, as specified in subclause 5.2.2.3.1, with the following information:

- dataForwarding IE set to false.

2a. Upon receipt of such a request, the SMF shall release the resources used for indirect data forwarding, and shall return a 200 OK response including the following information:

- dataForwarding IE set to false.

2b. If the SMF cannot proceed with the request, the SMF shall return an error response, as specified for step 2b of figure 5.2.2.3.1-1.

##### 5.2.2.3.10 P-CSCF Restoration Procedure via AMF

The requirements specified in subclause 5.2.2.3.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.3.1-1, with the following modifications.

The POST request shall contain:

- the release IE set to true;

- the cause IE set to REL\_DUE\_TO\_REACTIVATION.

#### 5.2.2.4 Release SM Context service operation

##### 5.2.2.4.1 General

The Release SM Context service operation shall be used to release the SM Context of a given PDU session, in the SMF, or in the V-SMF for HR roaming scenarios, in the following procedures:

- UE initiated Deregistration (see subclause 4.2.2.3.2 of 3GPP TS 23.502 [3]);

- Network initiated Deregistration (see subclause 4.2.2.3.2 of 3GPP TS 23.502 [3]), e.g. AMF initiated deregistration;

- Network requested PDU session release (see subclause 4.3.4.2 of 3GPP TS 23.502 [3]), e.g. AMF initiated release when there is a mismatch of the PDU session status between the UE and the AMF or when a required user plane security enforcement cannot be fulfilled by the NG-RAN;

- 5GS to EPS Idle mode mobility or handover for a Home Routed PDU session, to release the SM context in the V-SMF only.

The NF Service Consumer (e.g. AMF) shall release the SM Context of a given PDU session by using the HTTP "release" custom operation as shown in Figure 5.2.2.4.1-1.



Figure 5.2.2.4.1-1: SM context release

1. The NF Service Consumer shall send a POST request to the resource representing the individual SM context to be deleted. The payload body of the POST request shall contain any data that needs to be passed to the SMF.  
  
For a 5GS to EPS Idle mode mobility or handover, for a Home Routed PDU session, the POST request shall contain a vsmfReleaseOnly indication.

2a. On success, the SMF shall return a "204 No Content" response with an empty payload body in the POST response.

If the POST request contains a vsmfReleaseOnly indication (i.e. for a 5GS to EPS Idle mode mobility or handover, for a Home Routed PDU session), the V-SMF shall release its SM context and corresponding PDU session resource locally, i.e. without signalling towards the H-SMF.

2b. On failure, one of the HTTP status code listed in Table 6.1.3.3.4.3.2-2 shall be returned. For a 4xx/5xx response, the message body shall include a ProblemDetails structure with the "cause" attribute set to one of the application error listed in Table 6.1.3.3.4.3.2-2.

#### 5.2.2.5 Notify SM Context Status service operation

##### 5.2.2.5.1 General

The Notify SM Context Status service operation shall be used by the SMF to notify the NF Service Consumer about the status of an SM context related to a PDU session (e.g. when the SM context is released) in the SMF, or the V-SMF for HR roaming scenarios.

It is used in the following procedures:

- UE requested PDU Session Establishment procedure, when the PDU session establishment fails after the Create SM Context response (see subclause 4.3.2.2 of 3GPP TS 23.502 [3]);

- UE or Network requested PDU session release (see subclause 4.3.4.2 of 3GPP TS 23.502 [3]), e.g. SMF initiated release.

The SMF shall notify the NF Service Consumer by using the HTTP POST method as shown in Figure 5.2.2.5.1-1.



Figure 5.2.2.5.1-1: SM context status notification

1. The SMF shall send a POST request to the SM Context Status callback reference provided by the NF Service Consumer during the subscription to this notification. The payload body of the POST request shall contain the notification payload.

2a. On success, "204 No Content" shall be returned and the payload body of the POST response shall be empty.

If the SMF indicated in the request that the SM context resource is released, the NF Service Consumer shall release its association with the SMF for the PDU session and release the EBI(s) that were assigned to the PDU session.

2b. On failure or redirection, one of the HTTP status code listed in Table 6.1.3.7.3.1-2 shall be returned. For a 4xx/5xx response, the message body shall contain a ProblemDetails structure with the "cause" attribute set to one of the application error listed in Table 6.1.3.7.3.1-2.

If the NF Service Consumer (e.g. AMF) is not able to handle the notification but knows by implementation specific means that another NF Service Consumer (e.g. AMF) is able to handle the notification (e.g. AMF deployment with Backup AMF), it shall reply with an HTTP "307 temporary redirect" error response pointing to the URI of the new NF Service Consumer. If the NF Service Consumer is not able to handle the notification but another unknown NF Service Consumer could possibly handle the notification (e.g. AMF deployment with UDSF), it shall reply with an HTTP "404 Not found" error response.

If the SMF receives a "307 temporary redirect" response, the SMF shall use this URI as Notification URI in subsequent communication and shall resend the notification to that URI.

If the SMF becomes aware that a new NF Service Consumer (e.g. AMF) is requiring notifications (e.g. via the "404 Not found" response or via Namf\_Communication service AMFStatusChange Notifications, or via link level failures, see subclause 6.5.2 of 3GPP TS 29.500 [4]), and the SMF knows alternate or backup Address(es) where to send Notifications (e.g. via the GUAMI and/or backupAmfInfo received when the SM context was established or via AMFStatusChange Notifications), the SMF shall exchange the authority part of the corresponding Notification URI with one of those addresses and shall use that URI in subsequent communication; the SMF shall resend the failed request to that URI.

#### 5.2.2.6 Retrieve SM Context service operation

##### 5.2.2.6.1 General

The Retrieve SM Context service operation shall be used to retrieve an individual SM context, for a given PDU session, from the SMF, or from the V-SMF for HR roaming scenarios.

It is used in the following procedures:

- 5GS to EPS handover using N26 interface (see subclause 4.11.1.2.1 of 3GPP TS 23.502 [3]), for PDU sessions associated with 3GPP access;

- 5GS to EPS Idle mode mobility using N26 interface (see subclause 4.11.1.3.2 of 3GPP TS 23.502 [3]), for PDU sessions associated with 3GPP access.

The NF Service Consumer (e.g. AMF) shall retrieve an SM context by using the HTTP POST method (retrieve custom operation) as shown in Figure 5.2.2.6.1-1.



Figure 5.2.2.6.1-1: SM context retrieval

1. The NF Service Consumer shall send a POST request to the resource representing the individual SM context to be retrieved. The POST request may contain a payload body with the following parameters:

- target MME capabilities, if available, to allow the SMF to determine whether to include EPS bearer contexts for non-IP PDN type or not.

2a. On success, "200 OK" shall be returned; the payload body of the POST response shall contain the mapped EPS bearer contexts.   
  
If the target MME capabilities were provided in the request parameters, and if the target MME supports the non-IP PDN type, the SMF shall return, for a PDU session with PDU session type "Ethernet" or "Unstructured", an EPS bearer context with the "non-IP" PDN type.

2b. On failure, one of the HTTP status code listed in Table 6.1.3.3.4.4.2-2 shall be returned. For a 4xx/5xx response, the message body shall contain a ProblemDetails structure with the "cause" attribute set to one of the application error listed in Table 6.1.3.3.4.4.2-2.

#### 5.2.2.7 Create service operation

##### 5.2.2.7.1 General

The Create service operation shall be used to create an individual PDU session in the H-SMF for HR roaming scenarios.

It is used in the following procedures:

- UE requested PDU Session Establishment (see subclause 4.3.2.2.2 of 3GPP TS 23.502 [3]);

- EPS to 5GS Idle mode mobility or handover using N26 interface (see subclause 4.11 of 3GPP TS 23.502 [3]);- EPS to 5GS mobility without N26 interface (see subclause 4.11.2.3 3GPP TS 23.502 [3]);

- Handover of a PDU session between 3GPP access and non-3GPP access, when the target AMF does not know the SMF resource identifier of the SM context used by the source AMF, e.g. when the target AMF is not in the PLMN of the N3IWF (see subclause 4.9.2.3.2 of 3GPP TS 23.502 [3]);

- Handover from EPS to 5GC-N3IWF (see subclause 4.11.3.1 of 3GPP TS 23.502 [3]);

- Handover from EPC/ePDG to 5GS (see subclause 4.11.4.1 of 3GPP TS 23.502 [3]).

The NF Service Consumer (e.g. V-SMF) shall create a PDU session by using the HTTP POST method as shown in Figure 5.2.2.7.1-1.



Figure 5.2.2.7.1-1: PDU session creation

1. The NF Service Consumer shall send a POST request to the resource representing the PDU sessions collection resource of the H-SMF. The payload body of the POST request shall contain:

- a representation of the individual PDU session resource to be created;

- the Request Type IE, if it is received from the UE and if the request refers to an existing PDU session or an existing Emergency PDU session; the Request Type may be included otherwise;

- the vsmfId IE identifying the serving SMF;

- the vcnTunnelInfo;

- the anType;

- a URI ({vsmfPduSessionUri}) representing the PDU session resource in the V-SMF, for possible use by the H-SMF to subsequently modify or release the PDU session.

2a. On success, "201 Created" shall be returned, the payload body of the POST response shall contain:

- the representation describing the status of the request;

- the QoS flow(s) to establish for the PDU session;

- the epsPdnCnxInfo IE and, for each EPS bearer, an epsBearerInfo IE, if the PDU session may be moved to EPS during its lifetime;

- the "Location" header containing the URI of the created resource.

The authority and/or deployment-specific string of the apiRoot of the created resource URI may differ from the authority and/or deployment-specific string of the apiRoot of the request URI received in the POST request.

If the Request Type was received in the request and indicates this is a request for an existing PDU session or an existing emergency PDU session, the SMF shall identify the existing PDU session or emergency PDU session based on the PDU Session ID; in this case, the SMF shall not create a new PDU session or emergency PDU session but instead update the existing PDU session or emergency PDU session and provide the representation of the updated PDU session or emergency PDU session in the response to the NF Service Consumer.

The POST request shall be considered as colliding with an existing PDU session context if:

- it includes the same SUPI, or PEI for an emergency registered UE without a UICC or without an authenticated SUPI, and the same PDU Session ID as for an existing PDU session context; and

- this is a request to establish a new PDU session, i.e. the RequestType is absent in the request or is present and set to INITIAL\_REQUEST or INITIAL\_EMERGENCY\_REQUEST.

A POST request that collides with an existing PDU session context shall be treated as a request for a new PDU session context. Before creating the new PDU session context, the SMF should delete the existing PDU session context locally and any associated resources in the UPF and PCF. If the vsmfPduSessionUri of the existing PDU session context differs from the vsmfPduSessionUri received in the POST request, the SMF shall also send a status notification (see subclause 5.2.2.10) targeting the vsmfPduSessionUri of the existing PDU session context to notify the release of the existing PDU session context.

The NF Service Consumer shall store any epsPdnCnxInfo and EPS bearer information received from the H-SMF.

2b. On failure , or redirection during a UE requested PDU Session Establishment, one of the HTTP status code listed in Table 6.1.3.5.3.1-3 shall be returned. For a 4xx/5xx response, the message body shall contain a PduSessionCreateError structure, including:

- a ProblemDetails structure with the "cause" attribute set to one of the application error listed in Table 6.1.3.5.3.1-3;

- the n1SmCause IE with the 5GSM cause that the H-SMF requires the V-SMF to return to the UE, if the request included n1SmInfoFromUe;

- n1SmInfoToUe with any information to be sent to the UE (in the PDU Session Establishment Reject).

##### 5.2.2.7.2 EPS to 5GS Idle mode mobility

The requirements specified in subclause 5.2.2.7.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.7.1-1, with the following additions.

The POST request shall contain:

- the list of EPS Bearer Ids received from the MME;

- the PGW S8-C F-TEID received from the MME.

2a. Same as step 2 of Figure 5.2.2.7.1-1, with the following modifications.   
  
If the H-SMF finds a corresponding PDU session based on the EPS Bearer Ids and PGW S8-C F-TEID received in the request, and if it can proceed with moving the PDN connection to 5GS, the H-SMF shall return a 201 Created response including the following additional information:

- PDU Session ID corresponding to the EPS PDN connection;

- other PDU session parameters, such as PDU Session Type, Session AMBR, QoS flows information.

NOTE: The behaviour specified in this step also applies if the POST request collides with an existing PDU session context, i.e. if the POST request includes the same SUPI, or PEI for an emergency registered UE without a UICC or without an authenticated SUPI, and the received EPS bearer ID is the same as in the existing PDU session context.

2b. Same as step 2b of Figure 5.2.2.7.1-1, with the following additions.

If the H-SMF determines that seamless session continuity from EPS to 5GS is not supported for the PDU session, the H-SMF shall set the "cause" attribute in the ProblemDetails structure to "NO\_EPS\_5GS\_CONTINUITY".

##### 5.2.2.7.3 EPS to 5GS Handover Preparation

The requirements specified in subclause 5.2.2.7.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.7.1-1, with the following modifications.

The POST request shall contain:

- the list of EPS Bearer Ids received from the MME;

- the PGW S8-C F-TEID received from the MME;

- the hoPreparationIndication IE set to "true", to indicate that a handover preparation is in progress and the PGW-C/SMF shall not switch the DL user plane of the PDU session yet.

2a. Same as step 2 of Figure 5.2.2.7.1-1, with the following modifications.

If the SMF finds a corresponding PDU session based on the EPS Bearer Ids and PGW S8-C F-TEID received in the request, and if it can proceed with the procedure, the SMF shall return a 201 Created response including the following information:

- PDU Session ID corresponding to the EPS PDN connection;

- other PDU session parameters, such as PDU Session Type, Session AMBR, QoS flows information.

The SMF shall not switch the DL user plane of the PDU session, if the hoPreparationIndication IE was set to "true" in the request.

NOTE: The behaviour specified in this step also applies if the POST request collides with an existing PDU session context, i.e. if the POST request includes the same SUPI, or PEI for an emergency registered UE without a UICC or without an authenticated SUPI, and the received EPS bearer ID is the same as in the existing PDU session context.

2b. Same as step 2b of Figure 5.2.2.7.1-1, with the following additions.

If the H-SMF determines that seamless session continuity from EPS to 5GS is not supported for the PDU session, the H-SMF shall set the "cause" attribute in the ProblemDetails structure to "NO\_EPS\_5GS\_CONTINUITY".

#### 5.2.2.8 Update service operation

##### 5.2.2.8.1 General

The Update service operation shall be used in HR roaming scenarios to:

- update an individual PDU session in the H-SMF and/or provide the H-SMF with information received by the V-SMF in N1 SM signalling from the UE;

- update an individual PDU session in the V-SMF and/or provide information necessary for the V-SMF to send N1 SM signalling to the UE.

It is invoked by the V-SMF in the following procedures:

- UE or visited network requested PDU session modification (see subclause 4.3.3.3 of 3GPP TS 23.502 [3]);

- UE requested PDU session release (see subclause 4.3.4.3 of 3GPP TS 23.502 [3]);

- EPS to 5GS handover execution using N26 interface (see subclause 4.11 of 3GPP TS 23.502 [3]);

- Handover between 3GPP and untrusted non-3GPP access procedures (see subclause 4.9.2 of 3GPP TS 23.502 [3]), for a Home Routed PDU session, without AMF change or with target AMF in same PLMN;

- All procedures requiring to provide the H-SMF with information received by the V-SMF in N1 SM signalling from the UE to the H-SMF.

It is invoked by the H-SMF in the following procedures:

- Home network requested PDU session modification (see subclause 4.3.3.3 of 3GPP TS 23.502 [3]);

- Home network requested PDU session release (see subclause 4.3.4.3 of 3GPP TS 23.502 [3]);

- All procedures requiring to provide information necessary for the V-SMF to send N1 SM signalling to the UE;

- EPS Bearer ID allocation (see subclause 4.11.1.4.1 of 3GPP TS 23.502 [3]).

##### 5.2.2.8.2 Update service operation towards H-SMF

###### 5.2.2.8.2.1 General

The NF Service Consumer (e.g. V-SMF) shall update a PDU session in the H-SMF and/or provide the H-SMF with information received by the V-SMF in N1 SM signalling from the UE, by using the HTTP POST method (modify custom operation) as shown in Figure 5.2.2.8.2-1.



Figure 5.2.2.8.2-1: PDU session update towards H-SMF

1. The NF Service Consumer shall send a POST request to the resource representing the individual PDU session resource in the H-SMF. The payload body of the POST request shall contain:

- the requestIndication IE indicating the request type;

- the modification instructions and/or the information received by the V-SMF in N1 signalling from the UE.

2a. On success, "204 No Content" or "200 OK" shall be returned; in the latter case, the payload body of the POST response shall contain the representation describing the status of the request and/or information necessary for the V-SMF to send N1 SM signalling to the UE.

2b. On failure, one of the HTTP status code listed in Table 6.1.3.3.3.2-3 shall be returned. For a 4xx/5xx response, the message body shall contain a HsmfUpdateError structure, including:

- a ProblemDetails structure with the "cause" attribute set to one of the application error listed in Table 6.1.3.3.3.2-3;

- the n1SmCause IE with the 5GSM cause the H-SMF requires the V-SMF to return to the UE, if the request included n1SmInfoFromUe;

- n1SmInfoToUe binary data, if the SMF needs to return NAS SM information which the V-SMF does not need to interpret;

- the procedure transaction id that was that received in the request, if this is a response sent to a UE requested PDU session modification.

###### 5.2.2.8.2.2 UE or visited network requested PDU session modification

The requirements specified in subclause 5.2.2.8.2.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.8.2-1, with the following modifications.

The POST request shall contain:

- the requestIndication set to UE\_REQ\_PDU\_SES\_MOD, and the modifications requested by the UE, e.g. UE requested QoS rules or UE requested Qos flow descriptions, in an N1 SM container IE as specified in subclause 5.2.3.1, for a UE requested PDU session modification; or

- the requestIndication set to NW\_REQ\_PDU\_SES\_MOD, and the modifications requested by the visited network or the notifications initiated by the visited network, e.g. to report the release of QoS flow(s) or notifying QoS flow(s) whose targets QoS are no longer fulfilled, or to report that the user plane security enforcement with a value Preferred is not fulfilled or is fulfilled again, for a visited network requested PDU session modification;

###### 5.2.2.8.2.3 UE requested PDU session release

The requirements specified in subclause 5.2.2.8.2.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.8.2-1, with the following modifications.

The POST request shall contain:

- the requestIndication set to UE\_REQ\_PDU\_SES\_REL.

###### 5.2.2.8.2.4 EPS to 5GS Handover Execution

The requirements specified in subclause 5.2.2.8.2.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.8.2-1, with the following modifications.

The POST request shall contain:

- the list of EPS Bearer Ids successfully handed over to 5GS;

- the hoPreparationIndication IE set to "false", to indicate that there is no handover preparation in progress anymore and the PGW-C/SMF shall switch the DL user plane of the PDU session.

2. Same as step 2 of Figure 5.2.2.8.2-1, with the following modifications.

The SMF shall return a 200 OK response. The SMF shall switch the DL user plane of the PDU session using the N9 tunnel information that has been received in the vcnTunnelInfo, if the hoPreparationIndication IE was set to "false" in the request.

###### 5.2.2.8.2.5 Handover between 3GPP and untrusted non-3GPP access (Home Routed PDU session)

For Handover between 3GPP and untrusted non-3GPP access procedures, for a Home Routed PDU session, without AMF change or with the target AMF in the same PLMN, the requirements specified in subclause 5.2.2.8.2.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.8.2-1, with the following modifications.

The POST request shall contain the anType set to the target access type, i.e. to 3GPP\_ACCESS or NON\_3GPP\_ACCESS.

The requestIndication IE shall be set to PDU\_SES\_MOB.

###### 5.2.2.8.2.6 P-CSCF Restoration Procedure via AMF (Home Routed PDU session)

The requirements specified in subclause 5.2.2.8.2.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.8.2-1, with the following modifications:

The POST request shall contain:

- the requestIndication IE set to NW\_REQ\_PDU\_SES\_REL;

- the cause IE set to REL\_DUE\_TO\_REACTIVATION.

##### 5.2.2.8.3 Update service operation towards V-SMF

###### 5.2.2.8.3.1 General

The NF Service Consumer (e.g. H-SMF) shall update a PDU session in the V-SMF and/or provide information necessary for the V-SMF to send N1 SM signalling to the UE, or request to allocate EPS Bearer ID(s) for the PDU session, by using the HTTP "modify" custom operation as shown in Figure 5.2.2.8.3.1-1.



Figure 5.2.2.8.3.1-1: PDU session update towards V-SMF

1. The NF Service Consumer shall send a POST request to the resource representing the individual PDU session resource in the V-SMF. The payload body of the POST request shall contain:

- the requestIndication IE indicating the request type;

- the modification instructions and/or the information necessary for the V-SMF to send N1 SM signalling to the UE.

2a. On success, "204 No Content" or "200 OK" shall be returned; in the latter case, the payload body of the POST response shall contain the representation describing the status of the request and/or information received by the V-SMF in N1 signalling from the UE.

2b. On failure, one of the HTTP status code listed in Table 6.1.3.7.4.2.2-1 shall be returned. For a 4xx/5xx response, the message body shall contain a VsmfUpdateError structure, including:

- a ProblemDetails structure with the "cause" attribute set to one of the application error listed in Table 6.1.3.7.4.2.2-1;

- the n1SmCause IE with the 5GSM cause returned by the UE, if available;

- n1SmInfoFromUe and/or unknownN1SmInfo binary data, if NAS SM information has been received from the UE that needs to be transferred to the H-SMF or that the V-SMF does not comprehend;

- the procedure transaction id received from the UE, if available.

###### 5.2.2.8.3.2 Home network requested PDU session modification

The requirements specified in subclause 5.2.2.8.3.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.8.3-1, with the following modifications.

The requestIndication shall be set to NW\_REQ\_PDU\_SES\_MOD.

As part of the modification instructions, the NF Service Consumer may request to modify QoS parameters applicable at the PDU session level (e.g. modify the authorized Session AMBR values) or at the QoS flow level (e.g. modify the MFBR of a particular QoS flow).   
  
The NF Service Consumer may request to establish, modify and/or release QoS flows by including the qosFlowsAddModifyRequestList IE and/or the qosFlowsReleaseRequestList IE in the payload body.

The NF Service Consumer may include epsBearerInfo IE(s), if the PDU session may be moved to EPS during its lifetime and the EPS Bearer(s) information has changed (e.g. a new EBI has been assigned or the mapped EPS bearer QoS for an existing EBI has changed).

The NF Service Consumer may include the revokeEbiList IE to request the V-SMF to release some EBI(s) and delete any corresponding EPS bearer context stored in the V-SMF.

2. Same as step 2 of Figure 5.2.2.8.3-1, with the following modifications.

The V-SMF may accept all or only a subset of the QoS flows requested to be created or modified within the request.  
  
The list of QoS flows which have been successfully setup or modified, and those which failed to be so, if any, shall be included in the qosFlowsAddModifyList IE and/or the qosFlowsFailedtoAddModifyList IE respectively.

If the NG-RAN rejects the establishment of a voice QoS flow due to EPS Fallback for IMS voice (see subclause 4.13 of 3GPP TS 23.502 [3]), the V-SMF shall return the cause indicating that "mobility due to EPS fallback for IMS voice is on-going" for the corresponding flow in the qosFlowsFailedtoAddModifyList IE.

The list of QoS flows which have been successfully released, and those which failed to be so, if any, shall be included in the qosFlowsReleaseList and/or qosFlowsFailedtoReleaseList IE respectively.  
  
For a QoS flow which failed to be modified, the V-SMF shall fall back to the configuration of the QoS flow as it was configured prior to the reception of the PDU session update request from the NF Service Consumer.

The V-SMF shall store any EPS bearer information received from the H-SMF. If the revokeEbiList IE is present in the request, the V-SMF shall request delete the corresponding EPS bearer contexts and request the AMF to release the EBIs listed in this IE.

###### 5.2.2.8.3.3 Home network requested PDU session release

The requirements specified in subclause 5.2.2.8.3.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.8.3-1, with the following modifications.

The requestIndication shall be set to NW\_REQ\_PDU\_SES\_REL.

###### 5.2.2.8.3.4 Handover between 3GPP and untrusted non-3GPP access, from 5GC-N3IWF to EPS or from 5GS to EPC/ePDG

The requirements specified in subclause 5.2.2.8.3.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.8.3-1, with the following modifications.

The NF Service Consumer shall request the source V-SMF to release the resources in the VPLMN without sending a PDU session release command to the UE, by setting the requestIndication IE to NW\_REQ\_PDU\_SES\_REL and the Cause IE indicating "Release due to Handover", in the following scenarios:

- Handover of a PDU session between 3GPP and untrusted non-3GPP access, when the UE is roaming and the selected N3IWF is in the HPLMN (see subclause 4.9.2.4.2 of 3GPP TS 23.502 [3]);

- Handover from 5GC-N3IWF to EPS (see subclause 4.11.3.2 of 3GPP TS 23.502 [3]);

- Handover from 5GS to EPC/ePDG (see subclause 4.11.4.2 of 3GPP TS 23.502 [3]).

2. Same as step 2 of Figure 5.2.2.8.3-1, with the following modifications.

The V-SMF shall initiate the release of the PDU session if it receives the requestIndication set to NW\_REQ\_PDU\_SES\_REL in the request; if the Cause IE indicates "Release due to Handover", the V-SMF shall not send a PDU session release command to the UE.

###### 5.2.2.8.3.5 EPS Bearer ID allocation

The requirements specified in subclause 5.2.2.8.3.1 shall apply with the following modifications.

1. Same as step 1 of Figure 5.2.2.8.3-1, with the following modifications.

The requestIndication shall be set to EBI\_ASSIGNMENT\_REQ.

The NF Service Consumer shall include the assignEbiList IE to request the allocation of EBI(s). The NF Service Consumer may include the revokeEbiList IE to request the V-SMF to release some EBI(s) and delete any corresponding EPS bearer context stored in the V-SMF.

Upon receipt of this request, the V-SMF shall request the AMF to assign (and release if required) EBIs (see subclause 5.2.2.6 of 3GPP TS 29.518 [20].

2a. Same as step 2a of Figure 5.2.2.8.3-1, with the following modifications.

If the AMF has successfully assigned all or part of the requested EBIs, the SMF shall respond with the status code 200 OK, and include the list of EBIs successfully allocated, those which failed to be so if any, and the list of EBIs released for this PDU session at AMF if any, in the assignedEbiList IE, the failedtoAssignEbiList IE and/or the releasedEbiList IE respectively.

2b. Same as step 2b of Figure 5.2.2.8.3-1, with the following modifications.

For a 4xx/5xx response, the message body shall contain a VsmfUpdateError structure, including the list of EBIs which failed to be allocated in the failedtoAssignEbiList IE.

#### 5.2.2.9 Release service operation

##### 5.2.2.9.1 General

The Release service operation shall be used to request an immediate and unconditional deletion of an invidual PDU session resource in the H-SMF, in HR roaming scenarios.

It is invoked by the V-SMF in the following procedures:

- UE initiated Deregistration (see subclause 4.2.2.3.2 of 3GPP TS 23.502 [3]);

- Network initiated Deregistration (see subclause 4.2.2.3.2 of 3GPP TS 23.502 [3]), e.g. AMF initiated deregistration;

- visited network requested PDU Session release (see subclause 4.3.4.3 of 3GPP TS 23.502 [3]), e.g. AMF initiated release when there is a mismatch of the PDU session status between the UE and the AMF or when a required user plane security enforcement cannot be fulfilled by the NG-RAN.

The NF Service Consumer (e.g. V-SMF) shall release a PDU session in the H-SMF by using the HTTP "release" custom operation as shown in Figure 5.2.2.9.1-1.



Figure 5.2.2.9.1-1: Pdu session release

1. The NF Service Consumer shall send a POST request to the resource representing the individual PDU session resource in the H-SMF. The payload body of the POST request shall contain any data that needs to be passed to the H-SMF.

2a. On success, the H-SMF shall return a "204 No Content" response with an empty payload body in the POST response.

2b. On failure, one of the HTTP status code listed in Table 6.1.3.6.4.3.2-2 shall be returned. For a 4xx/5xx response, the message body shall contain a ProblemDetails structure with the "cause" attribute set to one of the application error listed in Table 6.1.3.6.4.3.2-2.

#### 5.2.2.10 Notify Status service operation

##### 5.2.2.10.1 General

The Notify Status service operation shall be used to notify the NF Service Consumer about the status of a PDU session (e.g. when the PDU session is released), in HR roaming scenarios.

It is used in the following procedures:

- Home network requested PDU Session release (see subclause 4.3.4.3 of 3GPP TS 23.502 [3]), e.g. H-SMF initiated release.

The H-SMF shall notify the NF Service Consumer (e.g. V-SMF) by using the HTTP POST method as shown in Figure 5.2.2.10-1.



Figure 5.2.2.10-1: PDU session status notification

1. The H-SMF shall send a POST request to the resource representing the individual PDU session resource in the V-SMF. The payload body of the POST request shall contain the notification payload, with the status information.

2a. On success, "204 No Content" shall be returned and the payload body of the POST response shall be empty.

2b. On failure, one of the HTTP status code listed in Table 6.1.3.7.3.1-2 shall be returned. For a 4xx/5xx response, the message body shall contain a ProblemDetails structure with the "cause" attribute set to one of the application error listed in Table 6.1.3.7.3.1-2.

### 5.2.3 General procedures

#### 5.2.3.1 Transfer of NAS SM information between UE and H-SMF for Home Routed PDU sessions

##### 5.2.3.1.1 General

As specified in subclause 4.3.1 of 3GPP TS 23.502 [3], for Home Routed PDU sessions, there is NAS SM information that the V-SMF and H-SMF need to interpret, and NAS SM information that the V-SMF only needs to transfer between the UE and H-SMF but which it does not need to interpret.

NAS SM information that only needs to be transferred between the UE and H-SMF by the V-SMF can be extended in later versions or releases of the NAS specification, e.g. defining new fields or values within existing IEs, and the extensions should not impact the V-SMF.

Besides, in HR roaming scenarios, the V-SMF and H-SMF can comply to different versions or releases of the NAS specification. It should be possible to support new SM features only requiring support from the H-SMF without impacting the V-SMF, when the H-SMF complies with a more recent release than the V-SMF, e.g. defining new NAS SM IEs in signalling from the UE to the H-SMF and/or signalling from the H-SMF to the UE.

##### 5.2.3.1.2 V-SMF Behaviour

The V-SMF shall transfer NAS SM information that it only needs to transfer to the H-SMF (i.e. known IEs, and IEs that have an unknown value not set to "reserved" according to the release to which the V-SMF complies, that only need to be forwarded by the V-SMF) in n1SmInfoFromUe binary data within the HTTP payload. This carries N1 SM IE(s), encoded as specified in 3GPP TS 24.501 [7], including the Type field and, for TLV or TLV-E IEs, the Length field.

NOTE 1: N1 SM IEs defined without a Type field need to be defined over N16 as specific IEs.

The V-SMF shall transfer NAS SM information that it does not comprehend (i.e. unknown IEs, or known IEs to be interpreted by the V-SMF that have an unknown value not set to "reserved" according to the release to which the V-SMF complies) in unknownN1SmInfo binary data within the HTTP payload. This carries N1 SM IE(s), encoded as specified in 3GPP TS 24.501 [7], including the Type field and, for TLV or TLV-E IEs, the Length field.

When receiving n1SmInfoToUe binary data in the HTTP payload from the H-SMF, the V-SMF shall parse all the N1 SM IEs received in the binary data and construct the NAS SM message to the UE according to 3GPP TS 24.501 [7]. The V-SMF shall append unknown NAS SM IEs received in the binary data at the end of the NAS SM message it sends to the UE.

NOTE 2: The V-SMF can infer the length of an unknown IE based on the IEI value. See subclause 11.2.4 of 3GPP TS 24.007 [8].

The V-SMF shall comprehend, and be able to encode at their right place in a given NAS message, all the IEs of the version of the NAS specification it implements that do not need to be interpreted by the V-SMF and which precede the last interpreted IE that the V-SMF implements in a NAS message.

NOTE 3: The V-SMF encodes comprehended IEs at their right place in the NAS SM message

##### 5.2.3.1.3 H-SMF Behaviour

When receiving unknownN1SmInfo binary data in the HTTP payload from the V-SMF, the H-SMF shall process any N1 SM IE received in this binary data that do not require to be interpreted by the V-SMF. Other N1 SM IEs shall be dropped, e.g. IEs that the H-SMF comprehends but which require to be interpreted by the V-SMF.

The H-SMF shall transfer NAS SM information which the V-SMF does not need to interpret (i.e. that it only needs to transfer to the UE) in n1SmInfoToUe binary data within the HTTP payload. This carries N1 SM IE(s), encoded as specified in 3GPP TS 24.501 [7], including the Type field and, for TLV or TLV-E IEs, the Length field.

NOTE 1: N1 SM IEs defined without a Type field need to be defined over N16 as specific IEs.

The NAS SM IEs in n1SmInfoToUe binary data shall be encoded in the same order as specified in 3GPP TS 24.501 [7].

N1 SM information which does not require to be interpreted by the V-SMF is information that is not defined as specific IEs over N16.

# 6 API Definitions

## 6.1 Nsmf\_PDUSession Service API

### 6.1.1 API URI

URIs of this API shall have the following root:

{apiRoot}/{apiName}/{apiVersion}/

where the "apiName" shall be set to "nsmf-pdusession" and the "apiVersion" shall be set to "v1" for the current version of this specification.

### 6.1.2 Usage of HTTP

#### 6.1.2.1 General

HTTP/2, as defined in IETF RFC 7540 [14], shall be used as specified in clause 5 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in subclause 5.3 of 3GPP TS 29.500 [4].

HTTP messages and bodies for the Nsmf\_PDUSession service shall comply with the OpenAPI [15] specification contained in Annex A.

#### 6.1.2.2 HTTP standard headers

##### 6.1.2.2.1 General

The usage of HTTP standard headers shall be supported as specified in subclause 5.2.2 of 3GPP TS 29.500 [4].

##### 6.1.2.2.2 Content type

The following content types shall be supported:

- the JSON format (IETF RFC 8259 [11]). The use of the JSON format shall be signalled by the content type "application/json". See also subclause 5.4 of 3GPP TS 29.500 [4].

- the Problem Details JSON Object (IETF RFC 7807 [23]). The use of the Problem Details JSON object in a HTTP response body shall be signalled by the content type "application/problem+json".

NOTE: "application/json" is used in a response that includes a payload body containing an application-specific data structure, see subclause 4.8 of 3GPP TS 29.501 [5].

Multipart messages shall also be supported (see subclause 6.1.2.4) using the content type "multipart/related", comprising:

- one JSON body part with the "application/json" content type; and

- one or two binary body parts with 3gpp vendor specific content subtypes.

The 3gpp vendor specific content subtypes defined in Table 6.1.2.2.2-1 shall be supported.

Table 6.1.2.2.2-1: 3GPP vendor specific content subtypes

|  |  |
| --- | --- |
| content subtype | Description |
| vnd.3gpp.ngap | Binary encoded payload, encoding NG Application Protocol (NGAP) IEs, as specified in subclause 9.4 of 3GPP TS 38.413 [9] (ASN.1 encoded). |
| vnd.3gpp.5gnas | Binary encoded payload, encoding a 5GS NAS message or 5G NAS IEs, as specified in 3GPP TS 24.501 [7]. |
| NOTE: Using 3GPP vendor content subtypes allows to describe the nature of the opaque payload (e.g. NGAP or 5GS NAS information) without having to rely on metadata in the JSON payload. | |

See subclause 6.1.2.4 for the binary payloads supported in the binary body part of multipart messages.

#### 6.1.2.3 HTTP custom headers

##### 6.1.2.3.1 General

In this release of the specification, no specific custom headers are defined for the Nsmf\_PDUSession service.

For 3GPP specific HTTP custom headers used across all service based interfaces, see subclause 5.2.3 of 3GPP TS 29.500 [4].

#### 6.1.2.4 HTTP multipart messages

HTTP multipart messages shall be supported, to transfer opaque N1 and/or N2 SMpayloads, in the following service operations (and HTTP messages):

- Create SM Context Request and Response (POST);

- Update SM Context Request and Response (POST);

- Create Request and Response (POST);

- Update Request and Response (POST(modify)).

HTTP multipart messages shall include one JSON body part and one or two binary body parts comprising:

- an N1 SM payload, an N2 SM payload or both, over N11 (see subclause 6.1.6.4);

- one or two N1 SM payloads, over N16 (see subclause 6.1.6.4).

The JSON body part shall be the "root" body part of the multipart message. It shall be encoded as the first body part of the multipart message. The "Start" parameter does not need to be included.

The multipart message shall include a "type" parameter (see IETF RFC 2387 [10]) specifying the media type of the root body part, i.e. "application/json".

NOTE: The "root" body part (or "root" object) is the first body part the application processes when receiving a multipart/related message, see IETF RFC 2387 [10]. The default root is the first body within the multipart/related message. The "Start" parameter indicates the root body part, e.g. when this is not the first body part in the message.

For each binary body part in a HTTP multipart message, the binary body part shall include a Content-ID header (see IETF RFC 2045 [12]), and the JSON body part shall include an attribute, defined with the RefToBinaryData type, that contains the value of the Content-ID header field of the referenced binary body part.

Examples of multipart/related messages can be found in Annex B.

#### 6.1.2.5 HTTP/2 request retries

The principles specified in subclause 5.2.8 of 3GPP TS 29.500 [4] shall be applied with the following modifications.

The NF Service Consumer may retry any HTTP POST request on the same resource through a new TCP connection after a TCP connection failure.

The SMF shall support handling repeated retries successfully.

NOTE: See subclauses 5.2.2.2 and 5.2.2.7 for the handling by the SMF of an HTTP POST request that would have already been processed by the SMF and that would be retried by the NF Service Consumer.

HTTP conditional requests are not supported by the Nsmf\_PDUSession service in this version of the API.

### 6.1.3 Resources

#### 6.1.3.1 Overview

Figure 6.1.3.1-1 describes the resource URI structure of the Nsmf\_PDUSession API.



Figure 6.1.3.1-1: Resource URI structure of the Nsmf\_PDUSession API

NOTE 1: In the figure, a child node with a frame represents a sub-URI that has at least one supported operation associated; "modify", "retrieve" and "release" are custom operations associated to the invidual SM context or individual PDU session resource.

NOTE 2: The sm-contexts and pdu-sessions collection resources can be distributed on different processing instances or hosts. Thus, the authority and/or deployment-specific string of the apiRoot of the created individual sm context and pdu-session resources' URIs can differ from the authority and/or deployment-specific string of the apiRoot of the sm-contexts and pdu-sessions distributed collections' URIs.

Table 6.1.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 6.1.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method or custom operation | Description  (service operation) |
| SM contexts  collection | {apiRoot}/nsmf-pdusession/v1/sm-contexts | POST | Create SM Context |
| Individual SM context | {apiRoot}/nsmf-pdusession/v1/sm-contexts/{smContextRef}/retrieve | retrieve (POST) | Retrieve SM Context |
| {apiRoot}/nsmf-pdusession/v1/sm-contexts/{smContextRef}/modify | modify  (POST) | Update SM Context |
| {apiRoot}/ nsmf\_pdusession/v1/sm-contexts/{smContextRef}/release | release  (POST) | Release SM Context |
| PDU sessions collection  (H-SMF) | {apiRoot}/nsmf-pdusession/v1/pdu-sessions | POST | Create |
| Individual PDU session  (H-SMF) | {apiRoot}/nsmf-pdusession/v1/pdu-sessions/{pduSessionRef}/modify | modify  (POST) | Update  (initiated by V-SMF) |
| {apiRoot}/nsmf-pdusession/v1/pdu-sessions/{pduSessionRef}/release | release  (POST) | Release |
| Individual PDU session  (V-SMF) | {vsmfPduSessionUri}/modify | modify  (POST) | Updated  (initiated by H-SMF) |
| {vsmfPduSessionUri} | POST | Notify Status |

#### 6.1.3.2 Resource: SM contexts collection

##### 6.1.3.2.1 Description

This resource represents the collection of the individual SM contexts created in the SMF.

This resource is modelled with the Collection resource archetype (see subclause C.2 of 3GPP TS 29.501 [5]).

##### 6.1.3.2.2 Resource Definition

Resource URI: **{apiRoot}/nsmf-pdusession/v1/sm-contexts**

This resource shall support the resource URI variables defined in table 6.1.3.2.2-1.

Table 6.1.3.2.2-1: Resource URI variables for this resource

|  |  |
| --- | --- |
| Name | Definition |
| apiRoot | See subclause 6.1.1. |

##### 6.1.3.2.3 Resource Standard Methods

###### 6.1.3.2.3.1 POST

This method creates an individual SM context resource in the SMF, or in V-SMF in HR roaming scenarios.

This method shall support the URI query parameters specified in table 6.1.3.2.3.1-1.

Table 6.1.3.2.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 6.1.3.2.3.1-2 and the response data structures and response codes specified in table 6.1.3.2.3.1-3.

Table 6.1.3.2.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SmContextCreateData | M | 1 | Representation of the SM context to be created in the SMF. |

Table 6.1.3.2.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| SmContextCreatedData | M | 1 | 201 Created | Successful creation of an SM context. |
|  |  |  | 307 Temporary Redirect | Temporary redirection, during a UE requested PDU Session Establishment. The response should include a Location header field containing a different URI. The URI shall be an alternative URI of the SMF that was selected by the AMF. |
|  |  |  | 308 Permanent Redirect | Permanent redirection, during a UE requested PDU Session Establishment. The response should include a Location header field containing a different URI. The URI shall be an alternative URI of the SMF that was selected by the AMF. |
| SmContextCreateError | M | 1 | 400 Bad Request | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4]. |
| SmContextCreateError | M | 1 | 403 Forbidden | The "cause" attribute shall be set to one of the following application error:  - N1\_SM\_ERROR  - SNSSAI\_DENIED  - DNN\_DENIED  - PDUTYPE\_DENIED  - SSC\_DENIED  - SUBSCRIPTION\_DENIED  - DNN\_NOT\_SUPPORTED  - PDUTYPE\_NOT\_SUPPORTED  - SSC\_NOT\_SUPPORTED  - HOME\_ROUTED\_ROAMING\_REQUIRED  - OUT\_OF\_LADN\_SERVICE\_AREA  - NO\_EPS\_5GS\_CONTINUITY  - INTEGRITY\_PROTECTED\_MDR\_NOT\_ACCEPTABLE  See table 6.1.7.3-1 for the description of these errors. |
| SmContextCreateError | M | 1 | 404 Not Found | The "cause" attribute shall be set to one of the following application error:  - CONTEXT\_NOT\_FOUND  See table 6.1.7.3-1 for the description of these errors. |
| SmContextCreateError | M | 1 | 500 Internal Server Error | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4] or to one of the following application errors:  - INSUFFICIENT\_RESOURCES\_SLICE  - INSUFFICIENT\_RESOURCES\_SLICE\_DNN  See table 6.1.7.3-1 for the description of these errors. |
| SmContextCreateError | M | 1 | 503 Service Unavailable | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4] or to one of the following application errors:  - DNN\_CONGESTION  - S-NSSAI\_ CONGESTION  See table 6.1.7.3-1 for the description of these errors. |
| SmContextCreateError | M | 1 | 504 Gateway Timeout | The "cause" attribute shall be set to one of the following application error:  - PEER\_NOT\_RESPONDING  - NETWORK\_FAILURE  See table 6.1.7.3-1 for the description of these errors. |

##### 6.1.3.2.4 Resource Custom Operations

None.

#### 6.1.3.3 Resource: Individual SM context

##### 6.1.3.3.1 Description

This resource represents an individual SM context created in the SMF.

This resource is modelled with the Document resource archetype (see subclause C.1 of 3GPP TS 29.501 [5]).

##### 6.1.3.3.2 Resource Definition

Resource URI: **{apiRoot}/nsmf-pdusession/v1/sm-contexts/{smContextRef}**

This resource shall support the resource URI variables defined in table 6.1.3.3.2-1.

Table 6.1.3.3.2-1: Resource URI variables for this resource

|  |  |
| --- | --- |
| Name | Definition |
| apiRoot | See subclause 6.1.1. |
| smContextRef | SM context reference assigned by the SMF during the Create SM Context service operation. |

##### 6.1.3.3.3 Resource Standard Methods

None.

##### 6.1.3.3.4 Resource Custom Operations

###### 6.1.3.3.4.1 Overview

Table 6.1.3.3.4.1-1: Custom operations

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Custom operaration URI | | Mapped HTTP method | | Description | |
| {resourceUri}/modify | | POST | | Update SM Context service operation | |
| {resourceUri}/release | | POST | | Release SM Context service operation. | |
| {resourceUri}/retrieve | | POST | | Retrieve SM Context service operation | |

###### 6.1.3.3.4.2 Operation: modify

6.1.3.3.4.2.1 Description

6.1.3.3.4.2.2 Operation Definition

This custom operation updates an individual SM context resource and/or provide N1 or N2 SM information received from the UE or the AN, for a given PDU session, towards the SMF, or in V-SMF in HR roaming scenario.

This operation shall support the request data structures specified in table 6.1.3.3.4.2.2-1 and the response data structure and response codes specified in table 6.1.3.3.4.2.2-2.

Table 6.1.3.3.4.2.2-1: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SmContextUpdateData | M | 1 | Representation of the updates to apply to the SM context. |

Table 6.1.3.3.4.2.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| SmContextUpdatedData | C | 0..1 | 200 OK | Successful update of the SM context, when the SMF needs to return information in the response. |
|  |  |  | 204 No Content | Successful update of the SM context, when the SMF does not need to return information in the response. |
| SmContextUpdateError | M | 1 | 400 Bad Request | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4]. |
| SmContextUpdateError | M | 1 | 403 Forbidden | The "cause" attribute shall be set to one of the following application error:  - N1\_SM\_ERROR  - N2\_SM\_ERROR  - SUBSCRIPTION\_DENIED  - OUT\_OF\_LADN\_SERVICE\_AREA  - PRIORITIZED\_SERVICES\_ONLY  - PDU\_SESSION\_ANCHOR\_CHANGE  See table 6.1.7.3-1 for the description of these errors. |
| SmContextUpdateError | M | 1 | 404 Not Found | The "cause" attribute shall be set to one of the following application error:  - CONTEXT\_NOT\_FOUND  See table 6.1.7.3-1 for the description of these errors. |
| SmContextUpdateError | M | 1 | 500 Internal Server Error | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4]. |
| SmContextUpdateError | M | 1 | 503 Service Unavailable | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4] or to one of the following application errors:  - DNN\_CONGESTION  - S-NSSAI\_ CONGESTION  See table 6.1.7.3-1 for the description of these errors. |

###### 6.1.3.3.4.3 Operation: release

6.1.3.3.4.3.1 Description

6.1.3.3.4.3.2 Operation Definition

This custom operation releases an individual SM context resource in the SMF, or in V-SMF in HR roaming scenario

This operation shall support the request data structures specified in table 6.1.3.3.4.3.2-1 and the response data structure and response codes specified in table 6.1.3.3.4.3.2-2.

Table 6.1.3.3.4.3.2-1: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SmContextReleaseData | C | 0..1 | Representation of the data to be sent to the SMF when releasing the SM context. |

Table 6.1.3.3.4.3.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
|  |  |  | 204 No Content | Successful release of an SM context. |
| ProblemDetails | M | 1 | 404 Not Found | The "cause" attribute shall be set to one of the following application error:  - CONTEXT\_NOT\_FOUND  See table 6.1.7.3-1 for the description of these errors. |

###### 6.1.3.3.4.4 Operation: retrieve

6.1.3.3.4.4.1 Description

6.1.3.3.4.4.2 Operation Definition

This custom operation retrieves an individual SM context resource from the SMF, or from the V-SMF in HR roaming scenario.

This operation shall support the request data structures specified in table 6.1.3.3.4.4.2-1 and the response data structure and response codes specified in table 6.1.3.3.4.4.2-2.

Table 6.1.3.3.4.4.2-1: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SmContextRetrieveData | O | 0..1 | Optional parameters used to retrieve the SM context, e.g. target MME capabilities. |

Table 6.1.3.3.4.4.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| SmContextRetrievedData | M | 1 | 200 OK | Successful retrieval of the SM context. |
|  |  |  |  |  |
| ProblemDetails | M | 1 | 403 Forbidden | The "cause" attribute shall be set to one of the following application error:  - TARGET\_MME\_CAPABILITY  See table 6.1.7.3-1 for the description of these errors. |
| ProblemDetails | M | 1 | 404 Not Found | The "cause" attribute shall be set to one of the following application error:  - CONTEXT\_NOT\_FOUND  See table 6.1.7.3-1 for the description of these errors. |

#### 6.1.3.5 Resource: PDU sessions collection (H-SMF)

##### 6.1.3.5.1 Description

This resource represents the collection of the individual PDU sessions created in the H-SMF.

This resource is modelled with the Collection resource archetype (see subclause C.2 of 3GPP TS 29.501 [5]).

##### 6.1.3.5.2 Resource Definition

Resource URI: **{apiRoot}/nsmf-pdusession/v1/pdu-sessions**

This resource shall support the resource URI variables defined in table 6.1.3.5.2-1.

Table 6.1.3.5.2-1: Resource URI variables for this resource

|  |  |
| --- | --- |
| Name | Definition |
| apiRoot | See subclause 6.1.1. |

##### 6.1.3.5.3 Resource Standard Methods

###### 6.1.3.5.3.1 POST

This method creates an individual PDU session resource in the H-SMF.

This method shall support the URI query parameters specified in table 6.1.3.5.3.1-1.

Table 6.1.3.5.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 6.1.3.5.3.1-2 and the response data structures and response codes specified in table 6.1.3.5.3.1-3.

Table 6.1.3.5.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| PduSessionCreateData | M | 1 | Representation of the PDU session to be created in the H-SMF. |

Table 6.1.3.5.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| PduSessionCreatedData | M | 1 | 201 Created | Successful creation of a PDU session. |
|  |  |  | 307 Temporary Redirect | Temporary redirection, during a UE requested PDU Session Establishment. The response should include a Location header field containing a different URI. The URI shall be an alternative URI of the SMF that was selected by the AMF. |
|  |  |  | 308 Permanent Redirect | Permanent redirection, during a UE requested PDU Session Establishment. The response should include a Location header field containing a different URI. The URI shall be an alternative URI of the SMF that was selected by the AMF. |
| PduSessionCreateError | M | 1 | 400 Bad Request | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4]. |
| PduSessionCreateError | M | 1 | 403 Forbidden | The "cause" attribute shall be set to one of the following application error:  - N1\_SM\_ERROR  - SNSSAI\_DENIED  - DNN\_DENIED  - PDUTYPE\_DENIED  - SSC\_DENIED  - SUBSCRIPTION\_DENIED  - DNN\_NOT\_SUPPORTED  - PDUTYPE\_NOT\_SUPPORTED  - SSC\_NOT\_SUPPORTED  - NO\_EPS\_5GS\_CONTINUITY  - INTEGRITY\_PROTECTED\_MDR\_NOT\_ACCEPTABLE  See table 6.1.7.3-1 for the description of these errors. |
| PduSessionCreateError | M | 1 | 404 Not Found | The "cause" attribute shall be set to one of the following application error:  - CONTEXT\_NOT\_FOUND  See table 6.1.7.3-1 for the description of these errors. |
| PduSessionCreateError | M | 1 | 500 Internal Server Error | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4] or to one of the following application errors:  - INSUFFIC\_RESOURCES\_SLICE  - INSUFFIC\_RESOURCES\_SLICE\_DNN  See table 6.1.7.3-1 for the description of these errors. |
| PduSessionCreateError | M | 1 | 503 Service Unavailable | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4] or to one of the following application errors:  - DNN\_CONGESTION  - S-NSSAI\_ CONGESTION  See table 6.1.7.3-1 for the description of these errors. |
| PduSessionCreateError | M | 1 | 504 Gateway Timeout | The "cause" attribute shall be set to one of the following application error:  - PEER\_NOT\_RESPONDING  - NETWORK\_FAILURE  See table 6.1.7.3-1 for the description of these errors. |

##### 6.1.3.5.4 Resource Custom Operations

###### 6.1.3.5.4.1 Overview

Table 6.1.3.5.4.1-1: Custom operations

|  |  |  |
| --- | --- | --- |
| Custom operaration URI | Mapped HTTP method | Description |
| n/a |  |  |

#### 6.1.3.6 Resource: Individual PDU session (H-SMF)

##### 6.1.3.6.1 Description

This resource represents an individual PDU session created in the H-SMF.

This resource is modelled with the Document resource archetype (see subclause C.1 of 3GPP TS 29.501 [5]).

##### 6.1.3.6.2 Resource Definition

Resource URI: **{apiRoot}/nsmf-pdusession/v1/pdu-sessions/{pduSessionRef}**

This resource shall support the resource URI variables defined in table 6.1.3.6.2-1.

Table 6.1.3.6.2-1: Resource URI variables for this resource

|  |  |
| --- | --- |
| Name | Definition |
| apiRoot | See subclause 6.1.1. |
| pduSessionRef | PDU session reference assigned by the H-SMF during the Create service operation. |

##### 6.1.3.6.3 Resource Standard Methods

None.

##### 6.1.3.6.4 Resource Custom Operations

###### 6.1.3.6.4.1 Overview

Table 6.1.3.6.4.1-1: Custom operations

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Custom operation URI | | Mapped HTTP method | | Description | |
| {resourceUri}/modify | | POST | | Update service operation | |
| {resourceUri}/release | | POST | | Release service operation. | |

###### 6.1.3.6.4.2 Operation: modify

6.1.3.6.4.2.1 Description

6.1.3.6.4.2.2 Operation Definition

This custom operation updates an individual PDU session resource in the H-SMF and/or provide the H-SMF with information received by the V-SMF in N1 SM signalling from the UE.

This operation shall support the request data structures specified in table 6.1.3.6.4.2.2-1 and the response data structure and response codes specified in table 6.1.3.6.4.2.2-2.

Table 6.1.3.6.4.2.2-1: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| HsmfUpdateData | M | 1 | Representation of the updates to apply to the PDU session. |

Table 6.1.3.6.4.2.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| HsmfUpdatedData | C | 0..1 | 200 OK | This case represents a successful update of the PDU session, when the H-SMF needs to return information in the response. |
|  |  |  | 204 No Content | This case represents a successful update of the PDU session, when the H-SMF does not need to return information in the response. |
| HsmfUpdateError | M | 1 | 400 Bad Request | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4]. |
| HsmfUpdateError | M | 1 | 403 Forbidden | The "cause" attribute shall be set to one of the following application errors:  - N1\_SM\_ERROR  - SUBSCRIPTION\_DENIED  - PDU\_SESSION\_ANCHOR\_CHANGE  See table 6.1.7.3-1 for the description of these errors. |
| HsmfUpdateError | M | 1 | 404 Not Found | The "cause" attribute shall be set to one of the following application error:  - CONTEXT\_NOT\_FOUND  See table 6.1.7.3-1 for the description of these errors. |
| HsmfUpdateError | M | 1 | 500 Internal Server Error | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4]. |
| HsmfUpdateError | M | 1 | 503 Service Unavailable | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4] or to one of the following application errors:  - DNN\_CONGESTION  - S-NSSAI\_ CONGESTION  See table 6.1.7.3-1 for the description of these errors. |

###### 6.1.3.6.4.3 Operation: release

6.1.3.6.4.3.1 Description

6.1.3.6.4.3.2 Operation Definition

This custom operation releases an individual PDU session resource in the H-SMF, in HR roaming scenario.

This operation shall support the request data structures specified in table 6.1.3.6.4.3.2-1 and the response data structure and response codes specified in table 6.1.3.6.4.3.2-2.

Table 6.1.3.6.4.3.2-1: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| ReleaseData | C | 0..1 | Representation of the data to be sent to the H-SMF when releasing the PDU session. |

Table 6.1.3.6.4.3.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
|  |  |  | 204 No Content | Successful release of a PDU session. |
| ProblemDetails | M | 1 | 404 Not Found | The "cause" attribute shall be set to one of the following application error:  - CONTEXT\_NOT\_FOUND  See table 6.1.7.3-1 for the description of these errors. |

#### 6.1.3.7 Resource: Individual PDU session (V-SMF)

##### 6.1.3.7.1 Description

This resource represents an individual PDU session created in the V-SMF.

This resource is modelled with the Document resource archetype (see subclause C.1 of 3GPP TS 29.501 [5]).

##### 6.1.3.7.2 Resource Definition

Resource URI: **{vsmfPduSessionUri}**

This resource shall support the resource URI variables defined in table 6.1.3.7.2-1.

Table 6.1.3.7.2-1: Resource URI variables for this resource

|  |  |
| --- | --- |
| Name | Definition |
| vsmfPduSessionUri | PDU session reference assigned by the V-SMF during the Create service operation. |

##### 6.1.3.7.3 Resource Standard Methods

###### 6.1.3.7.3.1 POST

This method sends a status notification to the NF Service Consumer.

This method shall support the URI query parameters specified in table 6.1.3.7.3.1-1.

Table 6.1.3.7.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 6.1.3.7.3.1-2 and the response data structures and response codes specified in table 6.1.3.7.3.1-3.

Table 6.1.3.7.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| StatusNotification | M | 1 | Representation of the status notification. |

Table 6.1.3.7.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
|  |  |  | 204 No Content | Successful notification of status change |
| ProblemDetails | M | 1 | 404 Not Found | The "cause" attribute shall be set to one of the following application error:  - CONTEXT\_NOT\_FOUND  See table 6.1.7.3-1 for the description of these errors. |

##### 6.1.3.7.4 Resource Custom Operations

###### 6.1.3.7.4.1 Overview

Table 6.1.3.7.4.1-1: Custom operations

|  |  |  |
| --- | --- | --- |
| Custom operation URI | Mapped HTTP method | Description |
| {vsmfPduSessionUri}/modify | POST | Update service operation (initiated by H-SMF) |

###### 6.1.3.7.4.2 Operation: modify

6.1.3.7.4.2.1 Description

6.1.3.7.4.2.2 Operation Definition

This custom operation modifies an individual PDU session resource in the V-SMF, in HR roaming scenario.

This operation shall support the request data structures specified in table 6.1.3.7.4.2.2-1 and the response data structure and response codes specified in table 6.1.3.7.4.2.2-2.

Table 6.1.3.7.4.2.2-1: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| VsmfUpdateData | M | 1 | Representation of the updates to apply to the PDU session. |

Table 6.1.3.7.4.2.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| VsmfUpdatedData | M | 1 | 200 OK | This case represents a successful update of the PDU session, when the V-SMF needs to return information in the response. |
|  |  |  | 204 No Content | This case represents a successful update of the PDU session, when the V-SMF does not need to return information in the response. |
| VsmfUpdateError | M | 1 | 400 Bad Request | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4]. |
| VsmfUpdateError | M | 1 | 403 Forbidden | The "cause" attribute shall be set to one of the following application errors:  - N1\_SM\_ERROR  - UNABLE\_TO\_PAGE\_UE  - UE\_NOT\_RESPONDING  - REJECTED\_BY\_UE  - REJECTED\_DUE\_VPLMN\_POLICY  - HO\_TAU\_IN\_PROGRESS  - EBI\_EXHAUSTED  - EBI\_REJECTED\_LOCAL\_POLICY, if the EBI allocation was rejected due to local policies at the AMF as specified in subclause 4.11.1.4.1 of 3GPP TS 23.502 [3].  See table 6.1.7.3-1 for the description of these errors. |
| VsmfUpdateError | M | 1 | 404 Not Found | The "cause" attribute shall be set to one of the following application error:  - CONTEXT\_NOT\_FOUND  See table 6.1.7.3-1 for the description of these errors. |
| VsmfUpdateError | M | 1 | 500 Internal Server Error | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4]. |
| VsmfUpdateError | M | 1 | 503 Service Unavailable | The "cause" attribute shall be set to one of the errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4]. |
| VsmfUpdateError | M | 1 | 504 Gateway Timeout | The "cause" attribute shall be set to one of the following application errors:  - PEER\_NOT\_RESPONDING  - NETWORK\_FAILURE  See table 6.1.7.3-1 for the description of these errors. |

### 6.1.4 Custom Operations without associated resources

None.

### 6.1.5 Notifications

#### 6.1.5.1 General

This subclause specifies the notifications provided by the Nsmf\_PDUSession service.

The delivery of notifications shall be supported as specified in subclause 6.2 of 3GPP TS 29.500 [4] for Server-initiated communication.

Table 6.1.5.1-1: Notifications overview

|  |  |  |  |
| --- | --- | --- | --- |
| Notification | Resource URI | HTTP method or custom operation | Description  (service operation) |
| SM context status notification | {smContextStatusUri}  (NF Service Consumer provided callback reference) | POST | Notify SM Context Status |

#### 6.1.5.2 SM Context Status Notification

##### 6.1.5.2.1 Description

If the NF Service Consumer (e.g AMF) has provided the callback URI for getting notified about change of SM context status, the SMF shall notify the NF Service Consumer when the SM context status information is updated.

##### 6.1.5.2.2 Notification Definition

The POST method shall be used for SM context status notification and the URI shall be the callback reference provided by the NF Service Consumer during the subscription to this notification.

Resource URI: **{smContextStatusUri}**

Support of URI query parameters is specified in table 6.1.5.2.2-1.

Table 6.1.5.2.2-1: URI query parameters supported by the POST method

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

Support of request data structures is specified in table 6.1.5.2.2-2, and support of response data structures and response codes is specified in table 6.1.5.2-3.

Table 6.1.5.2.2-2: Data structures supported by the POST Request Body

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SmContextStatusNotification | M | 1 | Representation of the SM context status notification. |

Table 6.1.5.2.2-3: Data structures supported by the POST Response Body

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| n/a |  |  | 204 No Content | Successful notification of the SM context status change |
| ProblemDetails | M | 1 | 404 Not Found | The "cause" attribute shall be set to one of the following application error:  - CONTEXT\_NOT\_FOUND  See table 6.1.7.3-1 for the description of these errors. |
| n/a |  |  | 307 Temporary Redirect | The NF service consumer shall generate a Location header field containing a URI pointing to another NF service consumer to which the notification should be send. |

### 6.1.6 Data Model

#### 6.1.6.1 General

This subclause specifies the application data model supported by the API.

Table 6.1.6.1-1 specifies the data types defined for the Nsmf service based interface protocol.

Table 6.1.6.1-1: Nsmf specific Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Section defined | Description |
| SmContextCreateData | 6.1.6.2.2 | Information within Create SM Context Request |
| SmContextCreatedData | 6.1.6.2.3 | Information within Create SM Context Response |
| SmContextUpdateData | 6.1.6.2.4 | Information within Update SM Context Request |
| SmContextUpdatedData | 6.1.6.2.5 | Information within Update SM Context Response |
| SmContextReleaseData | 6.1.6.2.6 | Information within Release SM Context Request |
|  |  |  |
| SMContextRetrieveData | 6.1.6.2.7 | Information within Retrieve SM Context Request |
| SmContextStatusNotification | 6.1.6.2.8 | Information within Notify SM Context Status Request |
| PduSessionCreateData | 6.1.6.2.9 | Information within Create Request |
| PduSessionCreatedData | 6.1.6.2.10 | Information within Create Response |
| HsmfUpdateData | 6.1.6.2.11 | Information within Update Request towards H-SMF |
| HsmfUpdatedData | 6.1.6.2.12 | Information within Update Response from H-SMF |
| ReleaseData | 6.1.6.2.13 | Information within Release Request |
| HsmfUpdateError | 6.1.6.2.14 | Error within Update Response from H-SMF |
| VsmfUpdateData | 6.1.6.2.15 | Information within Update Request towards V-SMF |
| VsmfUpdatedData | 6.1.6.2.16 | Information within Update Response from V-SMF |
| StatusNotification | 6.1.6.2.17 | Information within Notify Status Request |
| QosFlowItem | 6.1.6.2.18 | Individual QoS flow |
| QosFlowSetupItem | 6.1.6.2.19 | Individual QoS flow to setup |
| QosFlowAddModifyRequestItem | 6.1.6.2.20 | Individual QoS flow requested to be created or modified |
| QosFlowReleaseRequestItem | 6.1.6.2.21 | Individual QoS flow requested to be released |
| QosFlowProfile | 6.1.6.2.22 | QoS flow profile |
| GbrQosFlowInformation | 6.1.6.2.23 | GBR QoS flow information |
| QosFlowNotifyItem | 6.1.6.2.24 | Notification related to a QoS flow |
| SMContextRetrievedData | 6.1.6.2.27 | Information within Retrieve SM Context Response |
| TunnelInfo | 6.1.6.2.28 | Tunnel Information |
| StatusInfo | 6.1.6.2.29 | Status of SM context or of PDU session |
| VsmfUpdateError | 6.1.6.2.30 | Error within Update Response from V-SMF |
| EpsPdnCnxInfo | 6.1.6.2.31 | EPS PDN Connection Information from H-SMF to V-SMF |
| EpsBearerInfo | 6.1.6.2.32 | EPS Bearer Information from H-SMF to V-SMF |
| PduSessionNotifyItem | 6.1.6.2.33 | Notification related to a PDU session |
| EbiArpMapping | 6.1.6.2.34 | EBI to ARP mapping |
| SmContextCreateError | 6.1.6.2.35 | Error within Create SM Context Response |
| SmContextUpdateError | 6.1.6.2.36 | Error within Update SM Context Response |
| PduSessionCreateError | 6.1.6.2.37 | Error within Create Response |
| MmeCapabilities | 6.1.6.2.38 | MME capabilities |
| GtpTeid | 6.1.6.3.2 | GTP Tunnel Endpoint Identifier |
| ProcedureTransactionId | 6.1.6.3.2 | Procedure Transaction Identifier |
| EpsPdnCnxContainer | 6.1.6.3.2 | UE EPS PDN Connection container from SMF to AMF |
| EpsBearerId | 6.1.6.3.2 | EPS Bearer Id |
| EpsBearerContainer | 6.1.6.3.2 | EPS Bearer container from SMF to AMF |
| UpCnxState | 6.1.6.3.3 | User Plane Connection State |
| HoState | 6.1.6.3.4 | Handover State |
| RequestType | 6.1.6.3.5 | Request Type in Create (SM context) service operation. |
| RequestIndication | 6.1.6.3.6 | Request Indication in Update (SM context) service operation. |
| NotificationCause | 6.1.6.3.7 | Cause for generating a notification |
| Cause | 6.1.6.3.8 | Cause information |
| ResourceStatus | 6.1.6.3.9 | Status of SM context or PDU session resource |
| DnnSelectionMode | 6.1.6.3.10 | DNN Selection Mode |
| EpsInterworkingIndication | 6.1.6.3.11 | EPS Interworking Indication |
| N2SmInfoType | 6.1.6.3.12 | N2 SM Information Type |

Table 6.1.6.1-2 specifies data types re-used by the Nsmf service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nsmf service based interface.

Table 6.1.6.1-2: Nsmf re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| Uint32 | 3GPP TS 29.571 [13] | Unsigned 32-bit integers |
| Ipv4Addr | 3GPP TS 29.571 [13] | IPv4 Address |
| Ipv6Prefix | 3GPP TS 29.571 [13] | IPv6 Prefix |
| Uri | 3GPP TS 29.571 [13] | Uniform Resource Identifier |
| Supi | 3GPP TS 29.571 [13] | Subscription Permanent Identifier |
| Pei | 3GPP TS 29.571 [13] | Permanent Equipment Identifier |
| Gpsi | 3GPP TS 29.571 [13] | General Public Subscription Identifier |
| AccessType | 3GPP TS 29.571 [13] | Access Type (3GPP or non-3GPP access) |
| SupportedFeatures | 3GPP TS 29.571 [13] | Supported features |
| Qfi | 3GPP TS 29.571 [13] | QoS Flow Identifier |
| pduSessionId | 3GPP TS 29.571 [13] | PDU Session Identifier |
| pduSessionType | 3GPP TS 29.571 [13] | PDU Session Type |
| Ambr | 3GPP TS 29.571 [13] | PDU Session Aggregate Maximum Bit Rate |
| 5Qi | 3GPP TS 29.571 [13] | 5G QoS Identifier |
| Arp | 3GPP TS 29.571 [13] | Allocation and Retention Priority |
| ReflectiveQoSAttribute | 3GPP TS 29.571 [13] | Reflective QoS Attribute |
| Dynamic5Qi | 3GPP TS 29.571 [13] | QoS characteristics for a 5QI that is neither standardized nor pre-configured. |
| NonDynamic5Qi | 3GPP TS 29.571 [13] | QoS characteristics that replace the default QoS characteristics for a standardized or pre-configured 5QI. |
| PacketLossRate | 3GPP TS 29.571 [13] | Packet Loss Rate |
| NotificationControl | 3GPP TS 29.571 [13] | Notification Control |
| Dnn | 3GPP TS 29.571 [13] | Data Network Name |
| Snssai | 3GPP TS 29.571 [13] | Single Network Slice Selection Assistance Information |
| NfInstanceId | 3GPP TS 29.571 [13] | NF Instance Identifier |
| UserLocation | 3GPP TS 29.571 [13] | User Location |
| TimeZone | 3GPP TS 29.571 [13] | Time Zone |
| ProblemDetails | 3GPP TS 29.571 [13] | Error description |
| UpSecurity | 3GPP TS 29.571 [13] | User Plane Security Policy Enforcement information |
| RefToBinaryData | 3GPP TS 29.571 [13] | Cross-Reference to binary data encoded within a binary body part in an HTTP multipart message. |
| Guami | 3GPP TS 29.571 [13] | Globally Unique AMF ID |
| BackupAmfInfo | 3GPP TS 29.571 [13] | Backup AMF Information |
| PresenceState | 3GPP TS 29.571 [13] | Indicates the UE presence in or out of a LADN service area |
| TraceData | 3GPP TS 29.571 [13] | Trace control and configuration parameters |
| PlmnId | 3GPP TS 29.571 [13] | PLMN Identity |
| RatType | 3GPP TS 29.571 [13] | RAT Type |
| NgApCause | 3GPP TS 29.571 [13] | NGAP Cause |
| 5GMmCause | 3GPP TS 29.571 [13] | 5G MM Cause |

#### 6.1.6.2 Structured data types

##### 6.1.6.2.1 Introduction

This subclause defines the structures to be used in resource representations.

##### 6.1.6.2.2 Type: SmContextCreateData

Table 6.1.6.2.2-1: Definition of type SmContextCreateData

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Attribute name | | Data type | | P | | Cardinality | | Description | |
| supi | | Supi | | C | | 0..1 | | This IE shall be present, except if the UE is emergency registered and UICCless.  When present, it shall contain the subscriber permanent identify. | |
| unauthenticatedSupi | | boolean | | C | | 0..1 | | This IE shall be present if the SUPI is present in the message but is not authenticated and is for an emergency registered UE.  When present, it shall be set as follows:  - true: unauthenticated SUPI;  - false (default): authenticated SUPI. | |
| pei | | Pei | | C | | 0..1 | | This IE shall be present if the UE is emergency registered and it is either UIClless or the SUPI is not authenticated.  For all other cases, this IE shall be present if it is available.  When present, it shall contain the permanent equipment identifier. | |
| gpsi | | Gpsi | | C | | 0..1 | | This IE shall be present if it is available. When present, it shall contain the user's GPSI. | |
| pduSessionId | | PduSessionId | | C | | 0..1 | | This IE shall be present, except during an EPS to 5GS Idle mode mobility or handover using the N26 interface.  When present, it shall contain the PDU Session ID. | |
| dnn | | Dnn | | C | | 0..1 | | This IE shall be present, except during an EPS to 5GS Idle mode mobility or handover using the N26 interface.  When present, it shall contain the requested DNN. | |
| sNssai | | Snssai | | C | | 0..1 | | This IE shall be present during the PDU session establishment procedure. In this case, it shall contain the requested S-NSSAI for the serving PLMN. This corresponds to an S-NSSAI from the allowed NSSAI.  This IE shall also be present during an EPS to 5GS idle mode mobility or handover using the N26 interface. In this case, it shall contain the S-NSSAI configured in the AMF for EPS interworking. | |
| hplmnSnssai | | Snssai | | C | | 0..1 | | This IE shall be present for a HR PDU session, except during an EPS to 5GS idle mode mobility or handover using the N26 interface.  When present, it shall contain the requested S-NSSAI for the HPLMN. This corresponds to an S-NSSAI from the subscribed S-NSSAI corresponding to the SNSSAI value included in the sNssai IE. | |
| servingNfId | | NfInstanceId | | M | | 1 | | This IE shall contain the identifier of the serving NF (e.g. serving AMF). | |
| guami | | Guami | | C | | 0..1 | | This IE shall contain the serving AMF's GUAMI.  It shall be included if the NF service consumer is an AMF. | |
| serviceName | | string | | O | | 0..1 | | When present, this IE shall contain the name of the AMF service to which SM context status notifications are to be sent (see see subclause 6.5.2.2 of 3GPP TS 29.500 [4]). This IE may be included if the NF service consumer is an AMF. | |
| servingNetwork | | PlmnId | | M | | 1 | | This IE shall contain the serving core network operator PLMN ID. | |
| requestType | | RequestType | | C | | 0..1 | | This IE shall be present if the request relates to an existing PDU session or an existing emergency PDU session, except during an EPS to 5GS idle mode mobility or handover using the N26 interface. It may be present otherwise.  When present, it shall indicate whether the request refers to a new PDU session or emergency PDU session, or to an existing PDU session or emergency PDU session. | |
| n1SmMsg | | RefToBinaryData | | C | | 0..1 | | This IE shall be present and reference the N1 SM Message binary data (see subclause 6.1.6.4.2), except during an EPS to 5GS Idle mode mobility or handover using N26. | |
| anType | | AccessType | | M | | 1 | | This IE shall indicate the Access Network Type to which the PDU session is to be associated. | |
| ratType | | RatType | | C | | 0..1 | | This IE shall be present and indicate the RAT Type used by the UE, if available. | |
| presenceInLadn | | PresenceState | | C | | 0..1 | | This IE shall be present if the DNN corresponds to a LADN. When present, it shall be set to "IN" or "OUT" to indicate that the UE is in or out of the LADN service area. | |
| ueLocation | | UserLocation | | C | | 0..1 | | This IE shall contain the UE location information, if it is available. See NOTE. | |
| ueTimeZone | | TimeZone | | C | | 0..1 | | This IE shall contain the UE Time Zone, if it is available. | |
| addUeLocation | | UserLocation | | O | | 0..1 | | Additional UE location.  This IE may be present, if anType indicates a non-3GPP access and valid 3GPP access user location information is available.  When present, it shall contain:  - the last known 3GPP access user location; and  - the timestamp, if available, indicating the UTC time when the addUeLocation information was acquired.  See NOTE. | |
| smContextStatusUri | | Uri | | M | | 1 | | This IE shall include the callback URI to receive notification of SM context status. | |
| hSmfUri | | Uri | | C | | 0..1 | | This IE shall be present in HR roaming scenarios. When present, it shall contain the URI of the Nsmf\_PDUSession service of the selected H-SMF. The URI shall be formatted as specified in subclause 6.1.1. | |
| oldPduSessionId | | PduSessionId | | C | | 0..1 | | This IE shall be present if this information is received from the UE.  When present, it shall contain the old PDU Session ID received from the UE. See subclauses 4.3.2.2.1 and 4.3.5.2 of 3GPP TS 23.502 [3]. | |
| pduSessionsActivateList | | array(PduSessionId) | | C | | 0..N | | This IE shall be present, during an EPS to 5GS Idle mode mobility using the N26 interface, if received in the Registration Request from the UE.  When present, it shall be set as received in the Registration Request. It indicates all the PDU session(s) requested to be re-activated by the UE. | |
| ueEpsPdnConnection | | EpsPdnCnxContainer | | C | | 0..1 | | This IE shall be present, during an EPS to 5GS Idle mode mobility or handover using the N26 interface.  When present, it shall contain an MME/SGSN UE EPS PDN connection including the EPS bearer context(s). | |
| hoState | | HoState | | C | | 0..1 | | This IE shall be present during an EPS to 5GS handover using N26 interface, to request the preparation of a handover of the PDU session.  When present, it shall be set as specified in subclause 5.2.2.2.3. | |
| additionalHsmfUri | | array(Uri) | | O | | 0..N | | This IE may be present in HR roaming scenarios. When present, it shall contain an array of URI of the Nsmf\_PDUSession service of the additional H-SMFs discovered by the AMF for the given DNN, hplmnSnssai and for this PDU session. If provided, the V-SMF shall use these additional H-SMF(s) if the V-SMF is not able to receive any response from the H-SMF identified by hSmfUri.  The URI shall be formatted as specified in subclause 6.1.1. | |
| pcfId | | NfInstanceId | | O | | 0..1 | | When present, this IE shall contain the identifier of the PCF selected by the AMF for the UE (for Access and Mobility Policy Control); it shall be the V-PCF in LBO roaming and the H-PCF in HR roaming. | |
| nrfUri | | Uri | | O | | 0..1 | | This IE may be present to indicate the NRF to use for PCF selection within the same network slice instance. When present, the SMF shall use the NRF URI to select the PCF. | |
| supportedFeatures | | SupportedFeatures | | C | | 0..1 | | This IE shall be present if at least one optional feature defined in subclause 6.1.8 is supported. | |
| selMode | | DnnSelectionMode | | C | | 0..1 | | This IE shall be present if it is available. When present, it shall indicate whether the requested DNN corresponds to an explicitly subscribed DNN or to the usage of a wildcard subscription. | |
| backupAmfInfo | | array(BackupAmfInfo) | | C | | 0..N | | This IE shall be included if the NF service consumer is an AMF and the AMF supports the AMF management without UDSF for the following cases:  - First interaction with SMF.  - Modification of the BackupAmfInfo. | |
| traceData | | TraceData | | C | | 0..1 | | This IE shall be included if trace is required to be activated (see 3GPP TS 32.422 [22]). | |
| epsInterworkingInd | | EpsInterworkingIndication | | O | | 0..1 | | The AMF may provide the indication when a PGW-C+SMF is selected to serve the PDU Session.  When present, this IE shall indicate whether the PDU session may possibly be moved to EPS and whether N26 interface to be used during EPS interworking procedures.  The AMF may derive the value of the indication from different sources, like UE radio capabilities (e.g. "S1 mode supported"), UE subscription data (e.g. "Core Network Type Restriction to EPC) and configurations. | |
| NOTE: In shared networks, when the message is sent from the VPLMN to the HPLMN, the PLMN ID that is communicated in this IE shall be that of the selected Core Network Operator.  In shared networks, when the AMF and SMF pertain to the same PLMN, the Primary PLMN ID shall be communicated in the ECGI or NCGI to the SMF. The Core Network Operator PLMN ID shall be communicated in the TAI and the Serving Network. | | | | | | | | | |

##### 6.1.6.2.3 Type: SMContextCreatedData

Table 6.1.6.2.3-1: Definition of type SmContextCreatedData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| hsmfUri | Uri | C | 0..1 | This IE shall be present in HR roaming scenarios if the additionalHsmfUri IE was received in the request and the V-SMF established the PDU session towards an alternative SMF listed in the additionalHsmfUri IE. When present, it shall contain the URI of the H-SMF towards which the PDU session was established. |
| pduSessionId | PduSessionId | C | 0..1 | This IE shall be present, during an EPS to 5GS Idle mode mobility or handover using the N26 interface.  When present, it shall be set to the PDU Session ID. |
| sNssai | Snssai | C | 0..1 | This IE shall be present during an EPS to 5GS Idle mode mobility or handover using the N26 interface.  When present, it shall contain the S-NSSAI assigned to the PDU session. |
| upCnxState | UpCnxState | C | 0..1 | This IE shall be present if the SMF was requested to activate the user plane connection of the PDU session in the corresponding request.  When present, it shall be set as specified in subclause 5.2.2.2.2. |
| n2SmInfo | RefToBinaryData | C | 0..1 | This IE shall be present if N2 SM Information needs to be sent to the AN. |
| n2SmInfoType | N2SmInfoType | C | 0..1 | This IE shall be present if "n2SmInfo" attribute is present.  When present, this IE shall indicate the NG AP IE type for the NG AP SMF related IE container carried in "n2SmInfo" attribute. |
| allocatedEbiList | array(EbiArpmapping) | C | 0..N | This IE shall be present if the consumer NF is an AMF and Inter-system mobility happens. When present, it shall contain an array of EBI to ARP mappings currently allocated to the PDU session. |
| hoState | HoState | C | 0..1 | This IE shall be present if the SMF was requested to prepare an EPS to 5GS handover for the PDU session in the corresponding request.  When present, it shall be set as specified in subclause 5.2.2.2.3. |
| supportedFeatures | SupportedFeatures | C | 0..1 | This IE shall be present if at least one optional feature defined in subclause 6.1.8 is supported. |

##### 6.1.6.2.4 Type: SMContextUpdateData

Table 6.1.6.2.4-1: Definition of type SmContextUpdateData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| pei | Pei | C | 0..1 | This IE shall be present if it is available and has not been provided earlier to the SMF.  When present, this IE shall contain the permanent equipment identifier. |
| gpsi | Gpsi | C | 0..1 | This IE shall be present if it is available and has not been provided earlier to the SMF or if it has changed. When present, it shall contain the user's GPSI. |
| servingNfId | NfInstanceId | C | 0..1 | This IE shall be present upon inter-AMF change or mobility, or upon a N2 handover execution with AMF change.  When present, it shall contain the identifier of the serving NF (e.g. AMF). |
| smContextStatusUri | Uri | C | 0..1 | This IE shall be present if the servingNfId IE is present. It may be present otherwise.  When present, this IE shall include the callback URI to receive notification of SM context status. |
| guami | Guami | C | 0..1 | This IE shall be present if the servingNfId of AMF is present.  When present, it shall contain the serving AMF's GUAMI. |
| servingNetwork | PlmnId | C | 0..1 | This IE shall be present if the servingNfId IE is present.  When present, it shall contain the serving core network operator PLMN ID. |
| backupAmfInfo | array(BackupAmfInfo) | C | 0..N | This IE shall be included for the modification of the BackupAmfInfo if the NF service consumer is an AMF and the AMF supports the AMF management without UDSF. |
| anType | AccessType | C | 0..1 | This IE shall be present upon a change of Access Network Type.  When present, this IE shall indicate the Access Network Type to which the PDU session is to be associated. |
| ratType | RatType | C | 0..1 | This IE shall be present and indicate the RAT Type used by the UE, if available, upon a change of RAT Type. |
| presenceInLadn | PresenceState | C | 0..1 | This IE shall be present during a Service Request procedure (see subclause 5.2.2.3.2.2) ), an Xn handover (see subclause 5.2.2.3.3) or a N2 handover execution (see subclause 5.2.2.3.4.3), if the DNN of the PDU session corresponds to a LADN. When present, it shall be set to "IN" or "OUT" to indicate that the UE is in or out of the LADN service area. |
| ueLocation | UserLocation | C | 0..1 | This IE shall be present if it is available and if it needs to be reported to the SMF (e.g. the user location has changed or the user plane of the PDU session is deactivated).  When present, this IE shall contain:  - the UE location information; and  - the timestamp, if available, indicating the UTC time when the UeLocation information was acquired.  See NOTE. |
| ueTimeZone | TimeZone | C | 0..1 | This IE shall be present if it is available, the UE Time Zone has changed and needs to be reported to the SMF.  When present, this IE shall contain the UE Time Zone. |
| addUeLocation | UserLocation | O | 0..1 | Additional UE location.  This IE may be present, if anType indicates a non-3GPP access and a valid 3GPP access user location information is available.  When present, it shall contain:  - the last known 3GPP access user location; and  - the timestamp, if available, indicating the UTC time when the addUeLocation information was acquired.  See NOTE. |
| upCnxState | UpCnxState | C | 0..1 | This IE shall be present to request the activation or the deactivation of the user plane connection of the PDU session.  When present, it shall be set as specified in subclause 5.2.2.3.2. |
| hoState | HoState | C | 0..1 | This IE shall be present to request the preparation, execution or cancellation of a handover of the PDU session.  When present, it shall be set as specified in subclause 5.2.2.3.4. |
| toBeSwitched | boolean | C | 0..1 | This IE shall be present during an Xn Handover (see subclause 5.2.2.3.3) to request to switch the PDU session to a new downlink N3 tunnel endpoint.  When present, it shall be set as follows:  - true: request to switch to the PDU session.  - false (default): no request to switch the PDU session. |
| failedToBeSwitched | boolean | C | 0..1 | This IE shall be present during an Xn Handover (see subclause 5.2.2.3.3) if the PDU session failed to be setup in the target RAN.  When present, it shall be to true to indicate that the PDU session failed to be setup in the target RAN. |
| n1SmMsg | RefToBinaryData | C | 0..1 | This IE shall be present if N1 SM Information has been received from the UE.  When present, this IE shall reference the N1 SM Message binary data (see subclause 6.1.6.4.2). |
| n2SmInfo | RefToBinaryData | C | 0..1 | This IE shall be present if N2 SM Information has been received from the AN.  When present, this IE shall reference the N2 SM Information binary data (see subclause 6.1.6.4.3). |
| n2SmInfoType | N2SmInfoType | C | 0..1 | This IE shall be present if "n2SmInfo" attribute is present.  When present, this IE shall indicate the NG AP IE type for the NG AP SMF related IE container carried in "n2SmInfo" attribute. |
| targetServingNfId | NfInstanceId | C | 0..1 | This IE shall be present during a N2 handover preparation with AMF change.  When present, it shall contain the identifier of the target serving NF (e.g. AMF). |
| dataForwarding | boolean | C | 0..1 | This IE shall be present and set as specified in subclause 5.2.2.3.9 during a 5GS to EPS handover.  When present, it shall be set as follows:  - true: indirect data forwarding is required;  - false (default): indirect data forwarding is not required. |
| epsBearerSetup | array(EpsBearerContainer) | C | 0..N | This IE shall be present during a 5GS to EPS handover using the N26 interface.  When present, it shall include the EPS bearer context(s) successfully setup in EPS. |
| revokeEbiList | array(EpsBearerId) | C | 0..N | This IE shall be present to request the SMF to revoke some EBIs (see subclause 4.11.1.4.1 of 3GPP TS 23.502 [3]). When present, it shall contain the EBIs to revoke. |
| release | boolean | C | 0..1 | This IE shall be used to indicate a network initiated PDU session release is requested.  This IE shall be present and set as specified in subclause 5.2.2.3.10 during P-CSCF restoration procedure.  When present, it shall be set as follows:  - true: PDU session release is required;  - false (default): PDU session release is not required. |
| cause | Cause | O | 0..1 | When present, this IE shall indicate the cause for the requested modification, e.g. the NF Service Consumer cause for requesting to deactivate the user plane connection of the PDU session. |
| ngApCause | NgApCause | C | 0..1 | This IE shall be present, if the information is available. When present, this IE shall indicate the cause for the requested modification, e.g. the NGAP cause for requesting to deactivate the user plane connection of the PDU session. |
| 5GMmCauseValue | 5GMmCause | C | 0..1 | This IE shall be included if the AMF received a 5GMM cause code from the UE during any network initiated PDU session modification or release procedure. (e.g 5GMM Status message in response to a Downlink NAS Transport message carrying 5GSM payload). |
| sNssai | Snssai | C | 0..1 | This IE shall be present, during an EPS to 5GS idle mode mobility or handover using the N26 interface, if the S-NSSAI for the serving PLMN derived from the S-NSSAI of the home PLMN differs from the S-NSSAI provided in the Create SM Context Request.  When present, it shall contain the S-NSSAI for the serving PLMN. |
| traceData | TraceData | C | 0..1 | This IE shall be included if trace is required to be activated, modified or deactivated (see 3GPP TS 32.422 [22]).  For trace modification, it shall contain a complete replacement of trace data.  For trace deactivation, it shall contain the Null value. |
| epsInterworkingInd | EpsInterworkingIndication | O | 0..1 | This IE may be present if the indication has been provided during the PDU session creation, and its value has changed after session creation or last update.  When present, this IE shall indicate whether the PDU session may possibly be moved to EPS and whether N26 interface to be used during EPS interworking procedures. |
| NOTE: In shared networks, when the message is sent from the VPLMN to the HPLMN, the PLMN ID that is communicated in this IE shall be that of the selected Core Network Operator.  In shared networks, when the AMF and SMF pertain to the same PLMN, the Primary PLMN ID shall be communicated in the ECGI or NCGI to the SMF. The Core Network Operator PLMN ID shall be communicated in the TAI and the Serving Network. | | | | |

##### 6.1.6.2.5 Type: SMContextUpdatedData

Table 6.1.6.2.5-1: Definition of type SmContextUpdatedData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| upCnxState | UpCnxState | C | 0..1 | This IE shall be present if the SMF was requested to activate or deactivate the user plane connection of the PDU session in the corresponding request.  When present, it shall be set as specified in subclause 5.2.2.3.2. |
| hoState | HoState | C | 0..1 | This IE shall be present if the SMF was requested to prepare, execute or cancel a handover for the PDU session in the corresponding request.  When present, it shall be set as specified in subclause 5.2.2.3.4. |
| releaseEbiList | array(EpsBearerId) | C | 0..N | This IE shall be present if the SMF determines that some EBIs are not needed. When present, it shall contain the EBIs to be released. |
| allocatedEbiList | array(EbiArpMapping) | C | 0..N | This IE shall be present if the consumer NF is an AMF and Inter-system mobility happens. When present, it shall contain an array of EBI to ARP mappings currently allocated to the PDU session. |
| modifiedEbiList | array(EbiArpMapping) | C | 0..N | This IE shall be present if a PDU session modification procedure resulted in the change of ARP for a QoS flow that was already allocated an EBI. |
| n1SmMsg | RefToBinaryData | C | 0..1 | This IE shall be present if N1 SM Information needs to be sent to the UE.  When present, this IE shall reference the N1 SM Message binary data (see subclause 6.1.6.4.2). |
| n2SmInfo | RefToBinaryData | C | 0..1 | This IE shall be present if N2 SM Information needs to be sent to the AN.  When present, this IE shall reference the N2 SM Information binary data (see subclause 6.1.6.4.3). |
| n2SmInfoType | N2SmInfoType | C | 0..1 | This IE shall be present if "n2SmInfo" attribute is present.  When present, this IE shall indicate the NG AP IE type for the NG AP SMF related IE container carried in "n2SmInfo" attribute. |
| epsBearerSetup | array(EpsBearerContainer) | C | 0..N | This IE shall be present during an EPS to 5GS handover using the N26 interface.  When present, it shall include the EPS bearer context(s) successfully handed over to 5GS. |
| dataForwarding | boolean | C | 0..1 | This IE shall be present if it was present in the corresponding request.  When present, it shall be set as specified in subclause 5.2.2.3.9. |

##### 6.1.6.2.6 Type: SMContextReleaseData

Table 6.1.6.2.6-1: Definition of type SmContextReleaseData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| cause | Cause | C | 0..1 | This IE shall be present, if the information is available. When present, this IE shall indicate the NF Service Consumer cause for the requested SM context release. |
| ngApCause | NgApCause | C | 0..1 | This IE shall be present, if the information is available. When present, this IE shall indicate the NGAP cause for the requested SM context release. |
| 5GMmCauseValue | 5GMmCause | C | 0..1 | This IE shall be included if the PDU session is released by the AMF due to any 5GMM failure. When present, this IE shall contain the 5GMM cause code value received from the UE. |
| ueLocation | UserLocation | C | 0..1 | This IE shall be present, if available.  When present, it shall contain the UE location information. See NOTE. |
| ueTimeZone | TimeZone | C | 0..1 | This IE shall be present, if available.  When present, it shall contain the UE location information. |
| addUeLocation | UserLocation | O | 0..1 | Additional UE location.  This IE may be present, if anType previously reported is a non-3GPP access and a valid 3GPP access user location information is available.  When present, it shall contain:  - the last known 3GPP access user location; and  - the timestamp, if available, indicating the UTC time when the addUeLocation information was acquired.  See NOTE. |
| vsmfReleaseOnly | boolean | C | 0..1 | This IE shall be present and set to "true" during a 5GS to EPS Idle mode mobility or handover, for a Home Routed PDU session. When present, it shall be set as follows:  - true: release the SM context and PDU session in the V-SMF only;  - false (default): release the SM context and PDU session in V-SMF and H-SMF. |
| NOTE: In shared networks, when the message is sent from the VPLMN to the HPLMN, the PLMN ID that is communicated in this IE shall be that of the selected Core Network Operator.  In shared networks, when the AMF and SMF pertain to the same PLMN, the Primary PLMN ID shall be communicated in the ECGI or NCGI to the SMF. The Core Network Operator PLMN ID shall be communicated in the TAI and the Serving Network. | | | | |

##### 6.1.6.2.7 Type: SMContextRetrieveData

Table 6.1.6.2.7-1: Definition of type SmContextRetrieveData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| targetMmeCap | MmeCapabilities | C | 0..1 | This IE shall be present if it is available. When present, it shall contain the target MME capabilities. |

##### 6.1.6.2.8 Type: SMContextStatusNotification

Table 6.1.6.2.8-1: Definition of type SmContextStatusNotification

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| statusInfo | StatusInfo | M | 1 | This IE shall contain status information about the SM context. |

##### 6.1.6.2.9 Type: PduSessionCreateData

Table 6.1.6.2.9-1: Definition of type PduSessionCreateData

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Attribute name | | Data type | | P | | Cardinality | | Description | |
| supi | | Supi | | C | | 0..1 | | This IE shall be present, except if the UE is emergency registered and UICCless.  When present, it shall contain the subscriber permanent identify. | |
| unauthenticatedSupi | | boolean | | C | | 0..1 | | This IE shall be present if the SUPI is present in the message but is not authenticated and is for an emergency registered UE.  When present, it shall be set as follows:  - true: unauthenticated SUPI;  - false (default): authenticated SUPI. | |
| pei | | Pei | | C | | 0..1 | | This IE shall be present if the UE is emergency registered and it is either UIClless or the SUPI is not authenticated.  For all other cases, this IE shall be present if it is available.  When present, it shall contain the permanent equipment identifier. | |
| pduSessionId | | PduSessionId | | C | | 0..1 | | This IE shall contain the PDU Session ID, except during an EPS to 5GS Idle mode mobility or handover using the N26 interface. | |
| dnn | | Dnn | | M | | 1 | | This IE shall contain the requested DNN. | |
| sNssai | | Snssai | | C | | 0..1 | | This IE shall be present, except during an EPS to 5GS idle mode mobility or handover using the N26 interface.  When present, it shall contain the requested S-NSSAI mapped to the HPLMN S-NSSAI by the VPLMN. | |
| vsmfId | | NfInstanceId | | M | | 1 | | This IE shall contain the identifier of the serving SMF. | |
| servingNetwork | | PlmnId | | M | | 1 | | This IE shall contain the serving core network operator PLMN ID. | |
| requestType | | RequestType | | C | | 0..1 | | This IE shall be present if the request relates to an existing PDU session or an existing emergency PDU session, except during an EPS to 5GS idle mode mobility or handover using the N26 interface. It may be present otherwise.  When present, it shall indicate whether the request refers to a new PDU session or emergency PDU session, or to an existing PDU session or emergency PDU session. | |
| epsBearerId | | array(EpsBearerId) | | C | | 0..N | | This IE shall be present during an EPS to 5GS Idle mode mobility or handover preparation using the N26 interface.  When present, it shall contain the list of EPS bearer Id(s) received from the MME. | |
| pgwS8cFteid | | Bytes | | C | | 0..1 | | This IE shall be present during an EPS to 5GS Idle mode mobility or handover preparation using the N26 interface.  When present, it shall contain Base64-encoded characters, encoding the PGW S8 F-TEID for Control Plane as specified in Figure 8.22-1 of 3GPP TS 29.274 [16], received from the MME. | |
| vsmfPduSessionUri | | Uri | | M | | 1 | | This IE shall include the URI representing the PDU session in the V-SMF. | |
| vcnTunnelInfo | | TunnelInfo | | M | | 1 | | This IE shall contain the N9 tunnel information on the visited CN side. | |
| anType | | AccessType | | M | | 1 | | This IE shall indicate the Access Network Type to which the PDU session is to be associated. | |
| ratType | | RatType | | C | | 0..1 | | This IE shall be present and indicate the RAT Type used by the UE, if available. | |
| ueLocation | | UserLocation | | C | | 0..1 | | This IE shall contain the UE location information, if it is available. See NOTE. | |
| ueTimeZone | | TimeZone | | C | | 0..1 | | This IE shall contain the UE Time Zone, if it is available. | |
| addUeLocation | | UserLocation | | O | | 0..1 | | Additional UE location.  This IE may be present, if anType indicates a non-3GPP access and a valid 3GPP access user location information is available.  When present, it shall contain:  - the last known 3GPP access user location; and  - the timestamp, if available, indicating the UTC time when the addUeLocation information was acquired.  See NOTE. | |
| gpsi | | Gpsi | | C | | 0..1 | | This IE shall be present if it is available. When present, it shall contain the user's GPSI. | |
| n1SmInfoFromUe | | RefToBinaryData | | C | | 0..1 | | This IE shall be present if the V-SMF has received known N1 SM information from the UE that does not need to be interpreted by the V-SMF. When present, this IE shall reference the n1SmInfoFromUe binary data (see subclause 6.1.6.4.4). | |
| unknownN1SmInfo | | RefToBinaryData | | C | | 0..1 | | This IE shall be present if the V-SMF has received unknown N1 SM information from the UE. When present, this IE shall reference the unknownN1SmInfo binary data (see subclause 6.1.6.4.4). | |
| supportedFeatures | | SupportedFeatures | | C | | 0..1 | | This IE shall be present if at least one optional feature defined in subclause 6.1.8 is supported. | |
| hPcfId | | NfInstanceId | | O | | 0..1 | | When present, this IE shall contain the identifier of the H-PCF selected by the AMF for the UE (for Access and Mobility Policy Control). | |
| hoPreparationIndication | | boolean | | C | | 0..1 | | This IE shall be present during an EPS to 5GS handover preparation using the N26 interface.  When present, it shall be set as follows:  - true: an EPS to 5GS handover preparation is in progress; the PGW-C/SMF shall not switch the DL user plane of the PDU session yet.  - false: there is no on-going EPS to 5GS handover preparation in progress. If a handover preparation was in progress, the handover has been completed. The PGW-C/SMF shall switch the DL user plane of the PDU session using the N9 tunnel information that has been received in the vcnTunnelInfo.  It shall be set to "true" during an EPS to 5GS handover preparation using the N26 interface. | |
| selMode | | DnnSelectionMode | | C | | 0..1 | | This IE shall be present if it is available. When present, it shall indicate whether the requested DNN corresponds to an explicitly subscribed DNN or to the usage of a wildcard subscription. | |
| epsInterworkingInd | | EpsInterworkingIndication | | O | | 0..1 | | This IE may be present if the indication has been received from AMF and is allowed to be forwarded to H-SMF by operator configuration.  When present, this IE shall indicate whether the PDU session may possibly be moved to EPS and whether N26 interface to be used during EPS interworking procedures. | |
| vSmfServiceInstanceId | | string | | O | | 0..1 | | When present, this IE shall contain the serviceInstanceId of the V-SMF service instance serving the PDU session.  This IE may be used by the H-SMF to identify PDU sessions affected by a failure or restart of the V-SMF service (see subclause 6.2 of 3GPP TS 23.527 [24]). | |
| NOTE: In shared networks, the PLMN ID that is communicated in this IE shall be that of the selected Core Network Operator. | | | | | | | | | |

##### 6.1.6.2.10 Type: PduSessionCreatedData

Table 6.1.6.2.10-1: Definition of type PduSessionCreatedData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| pduSessionType | PduSessionType | M | 1 | This IE shall indicate the selected PDU type. |
| sscMode | string | M | 1 | This IE shall indicate the SSC mode applicable to the PDU session.  When present, it shall be encoded as one character in hexadecimal representation, taking a value of "0" to "9" or "A" to "F", representing the 4 bits of the SSC mode value of the SSC mode IE specified in subclause 9.8.4.10 of 3GPP TS 24.501 [7].  Example: SSC mode 3 shall be encoded as "3".  See NOTE. |
| hcnTunnelInfo | TunnelInfo | M | 1 | This IE shall contain the N9 tunnel information on the home CN side. |
| sessionAmbr | Ambr | M | 1 | This IE shall contain the Session AMBR granted to the PDU session. |
| qosFlowsSetupList | array(QosFlowSetupItem) | M | 1..N | This IE shall contain the set of QoS flow(s) to establish for the PDU session. It shall contain at least the Qos flow associated to the default Qos rule. |
| pduSessionId | PduSessionId | C | 0..1 | This IE shall be present during an EPS to 5GS Idle mode mobility or handover preparation using the N26 interface.  When present, it shall be set to the PDU Session ID. |
| sNssai | Snssai | C | 0..1 | This IE shall be present during an EPS to 5GS Idle mode mobility or handover using the N26 interface.  When present, it shall contain the S-NSSAI assigned to the PDU session in the Home PLMN. |
| enablePauseCharging | boolean | C | 0..1 | This IE shall be present, based on operator's policy, to enable the use of Pause of Charging for the PDU session (see subclause 4.4.4 of 3GPP TS 23.502 [3]).  When present, it shall be set as follows:  - true: enable Pause of Charging;  - false (default): disable Pause of Charging. |
| ueIpv4Address | Ipv4Addr | C | 0..1 | This IE shall be present if the H-SMF assigns a UE IPv4 address to the PDU session. |
| ueIpv6Prefix | Ipv6Prefix | C | 0..1 | This IE shall be present if the H-SMF assigns a UE IPv6 prefix to the PDU session. |
| n1SmInfoToUe | RefToBinaryData | C | 0..1 | This IE shall be present if the H-SMF needs to send N1 SM information to the UE that does not need to be interpreted by the V-SMF. When present, this IE shall reference the n1SmInfoToUe binary data (see subclause 6.1.6.4.4). |
| epsPdnCnxInfo | EpsPdnCnxInfo | C | 0..1 | This IE shall be present if the PDU session may be moved to EPS during its lifetime. |
| epsBearerInfo | array(EpsBearerInfo) | C | 1..N | This IE shall be present if the PDU session may be moved to EPS during its lifetime. |
| supportedFeatures | SupportedFeatures | C | 0..1 | This IE shall be present if at least one optional feature defined in subclause 6.1.8 is supported. |
| upSecurity | UpSecurity | O | 0..1 | When present, this IE shall indicate the security policy for integrity protection and encryption for the user plane of the PDU session. |
| NOTE: This IE contains information that the V-SMF only needs to transfer to the UE (without interpretation). It is sent as a separate IE rather than within the n1SmInfoToUE binary data because the Selected SSC mode IE is defined as a "V" IE (i.e. without a Type field) in the NAS PDU Session Establishment Accept message. | | | | |

##### 6.1.6.2.11 Type: HsmfUpdateData

Table 6.1.6.2.11-1: Definition of type HsmfUpdateData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| requestIndication | RequestIndication | M | 1 | This IE shall indicate the request type. |
| pei | Pei | C | 0..1 | This IE shall be present if it is available and has not been provided earlier to the H-SMF.  When present, this IE shall contain the permanent equipment identifier. |
| vcnTunnelInfo | TunnelInfo | C | 1 | This IE shall be present if the N9 tunnel information on the visited CN side provided earlier to the H-SMF has changed.  When present, this IE shall contain the new N9 tunnel information on the visited CN side. |
| servingNetwork | PlmnId | C | 0..1 | This IE shall contain the serving core network operator PLMN ID, if it has changed. |
| anType | AccessType | C | 0..1 | This IE shall be present during if the Access Network Type provided earlier to the H-SMF has changed.  When present, this IE shall indicate the new Access Network Type to which the PDU session is to be associated. |
| ratType | RatType | C | 0..1 | This IE shall be present and indicate the RAT Type used by the UE, if available, upon a change of RAT Type. |
| ueLocation | UserLocation | C | 0..1 | This IE shall be present if it is available, the UE Location has changed and needs to be reported to the H-SMF.  When present, this IE shall contain:  - the new UE location information; and  - the timestamp, if available, indicating the UTC time when the UeLocation information was acquired.  See NOTE. |
| ueTimeZone | TimeZone | C | 0..1 | This IE shall be present if it is available, the UE Time Zone has changed and needs to be reported to the H-SMF.  When present, this IE shall contain the new UE Time Zone. |
| addUeLocation | UserLocation | O | 0..1 | Additional UE location.  This IE may be present, if anType indicates a non-3GPP access and a valid 3GPP access user location information is available.  When present, it shall contain:  - the last known 3GPP access user location; and  - the timestamp, if available, indicating the UTC time when the addUeLocation information was acquired.  See NOTE. |
| pauseCharging | boolean | C | 0..1 | This IE shall be present if the H-SMF enabled the use of Pause Pause of Charging for the PDU session during the PDU session establishment and  Pause of Charging needs to be started or stopped (see subclause 4.4.4 of 3GPP TS 23.502 [3]).  When present, it shall be set as follows:  - true: to Start Pause of Charging;  - false: to Stop Pause of Charging. |
| pti | ProcedureTransactionId | C | 0..1 | This IE shall be present if the requestIndication indicates a UE requested PDU session modification or release. When present, it shall contain the PTI value received from the UE. |
| n1SmInfoFromUe | RefToBinaryData | C | 0..1 | This IE shall be present if the V-SMF has received known N1 SM information from the UE that does not need to be interpreted by the V-SMF. When present, this IE shall reference the n1SmInfoFromUe binary data (see subclause 6.1.6.4.4). |
| unknownN1SmInfo | RefToBinaryData | C | 0..1 | This IE shall be present if the V-SMF has received unknown N1 SM information from the UE. When present, this IE shall reference the unknownN1SmInfo binary data (see subclause 6.1.6.4.4). |
| qosFlowsRelNotifyList | array(QosFlowItem) | C | 0..N | This IE shall be present if QoS flows have been released. |
| qosFlowsNotifyList | array(QosFlowNotifyItem) | C | 0..N | This IE shall be present if the QoS targets for GBR QoS flow(s) are not fulfilled anymore or when they are fulfilled again. |
| NotifyList | array(PduSessionNotifyItem) | C | 0..N | Description of notifications related to the PDU session. This IE shall be present if the NG-RAN has established user plane resources for the PDU session that do not fulfil the User Plane Security Enforcement with a value Preferred, or when the user plane security enforcement is fulfilled again. |
| epsBearerId | array(EpsBearerId) | C | 0..N | This IE shall be present during an EPS to 5GS handover execution using the N26 interface.  When present, it shall contain the list of EPS bearer Id(s)successfully handed over to 5GS. |
| hoPreparationIndication | boolean | C | 0..1 | This IE shall be present during an EPS to 5GS handover preparation and handover execution using the N26 interface.  When present, it shall be set as follows:  - true: an EPS to 5GS handover preparation is in progress; the PGW-C/SMF shall not switch the DL user plane of the PDU session yet.  - false: there is no on-going EPS to 5GS handover preparation in progress. If a handover preparation was in progress, the handover has been completed. The PGW-C/SMF shall switch the DL user plane of the PDU session using the N9 tunnel information that has been received in the vcnTunnelInfo.  It shall be set to "true" during an EPS to 5GS handover preparation using the N26 interface.  It shall be set to "false" during an EPS to 5GS handover execution using the N26 interface. |
| revokeEbiList | array(EpsBearerId) | C | 0..N | This IE shall be present to request the H-SMF to revoke some EBIs (see subclause 4.11.1.4.1 of 3GPP TS 23.502 [3]). When present, it shall contain the EBIs to revoke. |
| cause | Cause | C | 0..1 | This IE shall be present and set as specified in subclause 5.2.2.8.2.6 during P-CSCF restoration procedure for home-routed PDU session.  When present, this IE shall indicate the NF Service Consumer cause of the requested modification. |
| ngApCause | NgApCause | C | 0..1 | This IE shall be present, if the information is available and if this information is permitted to be sent to the H-SMF operator according to the V-SMF operator's policy. When present, this IE shall indicate the NGAP cause for the requested modification. |
| 5GMmCauseValue | 5GMmCause | C | 0..1 | The V-SMF shall include this IE if it received it from the AMF and if this information is permitted to be sent to the H-SMF operator according to the V-SMF operator's policy. |
| epsInterworkingInd | EpsInterworkingIndication | O | 0..1 | This IE may be present if the indication has been received from AMF and is allowed to be forwarded to H-SMF by operator configuration.  When present, this IE shall indicate whether the PDU session may possibly be moved to EPS and whether N26 interface to be used during EPS interworking procedures. |
| NOTE: In shared networks, the PLMN ID that is communicated in this IE shall be that of the selected Core Network Operator. | | | | |

##### 6.1.6.2.12 Type: HsmfUpdatedData

Table 6.1.6.2.12-1: Definition of type HsmfUpdatedData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| n1SmInfoToUe | RefToBinaryData | C | 0..1 | This IE shall be present if the H-SMF needs to send N1 SM information to the UE that does not need to be interpreted by the V-SMF. When present, this IE shall reference the n1SmInfoToUe binary data (see subclause 6.1.6.4.4). |

##### 6.1.6.2.13 Type: ReleaseData

Table 6.1.6.2.13-1: Definition of type ReleaseData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| cause | Cause | C | 0..1 | This IE shall be present, if the information is available. When present, this IE shall indicate the NF Service Consumer cause for the requested PDU session release. |
| ngApCause | NgApCause | C | 0..1 | This IE shall be present, if the information is available and if this information is permitted to be sent to the H-SMF operator according to the V-SMF operator's policy. When present, this IE shall indicate the NGAP cause for the requested PDU session release. |
| 5GMmCauseValue | 5GMmCause | C | 0..1 | The V-SMF shall include this IE if it received it from the AMF and if this information is permitted to be sent to the H-SMF operator according to the V-SMF operator's policy. |
| ueLocation | UserLocation | C | 0..1 | This IE shall be present, if available.  When present, it shall contain the UE location information. |
| ueTimeZone | TimeZone | C | 0..1 | This IE shall be present, if available.  When present, it shall contain the UE location information. |
| addUeLocation | UserLocation | O | 0..1 | Additional UE location.  This IE may be present, if anType previously reported is a non-3GPP access and a valid 3GPP access user location information is available.  When present, it shall contain:  - the last known 3GPP access user location; and  - the timestamp, if available, indicating the UTC time when the addUeLocation information was acquired. |

##### 6.1.6.2.14 Type: HsmfUpdateError

Table 6.1.6.2.14-1: Definition of type HsmfUpdateError

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | |
| error | ProblemDetails | M | 1 | More information on the error shall be provided in the "cause" attribute of the "ProblemDetails" structure. | |
| pti | ProcedureTransactionId | C | 0..1 | This IE shall be present if this is a response sent to a UE requested PDU session modification. When present, it shall contain the PTI value received in the corresponding request. | |
| n1smCause | string | C | 0..1 | This IE shall be present if the request included n1SmInfoFromUe.  When present, it shall contain the 5GSM cause the H-SMF requires the V-SMF to return to the UE. It shall be encoded as two characters in hexadecimal representation with each character taking a value of "0" to "9" or "A" to "F", and represent the cause value of the 5GSM cause IE specified in subclause 9.8.4.2 of 3GPP TS 24.501 [7].  Example: the cause "Invalid mandatory information" shall be encoded as "60".  See NOTE. | |
| n1SmInfoToUe | RefToBinaryData | C | 0..1 | This IE shall be present if the H-SMF needs to send N1 SM information to the UE that does not need to be interpreted by the V-SMF. When present, this IE shall reference the n1SmInfoToUe binary data (see subclause 6.1.6.4.4). | |
| NOTE: This IE contains information that the V-SMF shall transfer to the UE without interpretation. It is sent as a separate IE rather than within the n1SmInfoToUE binary data because the 5GSM cause IE is defined as a "V" IE (i.e. without a Type field) in the NAS PDU Session Modification Reject message. | | | | | |

##### 6.1.6.2.15 Type: VsmfUpdateData

Table 6.1.6.2.15-1: Definition of type VsmfUpdateData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| requestIndication | RequestIndication | M | 1 | This IE shall indicate the request type. |
| sessionAmbr | Ambr | C | 1 | This IE shall be present if the Session AMBR authorized for the PDU session is modified. When present, it shall contain the new Session AMBR authorized for the PDU session. |
| qosFlowsAddModRequestList | array(QosFlowAddModifyRequestItem) | C | 0..N | This IE shall be present if QoS flows are requested to be established or modified. |
| qosFlowsRelRequestList | array(QosFlowReleaseRequestItem) | C | 0..N | This IE shall be present if QoS flows are requested to be released. |
| epsBearerInfo | array(EpsBearerInfo) | C | 0..N | This IE shall be present if the PDU session may be moved to EPS during its lifetime and the ePSBearerInfo has changed.  When present, it shall only include epsBearerInfo IE(s) for new EBI or for EBIs for which the epsBearerInfo has changed. The complete epsBearerInfo shall be provided for an EBI that is included (i.e. the epsBearerInfo newly received for a given EBI replaces any epsBearerInfo previously received for this EBI). |
| assignEbiList | array(Arp) | C | 0..N | This IE shall be present if the H-SMF requests EBIs to be assigned. |
| revokeEbiList | array(EpsBearerId) | C | 0..N | This IE shall be present if the H-SMF requests the V-SMF to revoke some EBI(s). When present, it shall contain the EBIs to revoke. |
| modifiedEbiList | array(EbiArpMapping) | C | 0..N | This IE shall be present if a PDU session modification procedure resulted in the change of ARP for a QoS flow that was already allocated an EBI. |
| pti | ProcedureTransactionId | C | 0..1 | This IE shall be present if the request is sent in response to a UE requested PDU session modification or release. When present, it shall contain the PTI value received in the corresponding request. |
| n1SmInfoToUe | RefToBinaryData | C | 0..1 | This IE shall be present if the H-SMF needs to send N1 SM information to the UE that does not need to be interpreted by the V-SMF. When present, this IE shall reference the n1SmInfoToUe binary data (see subclause 6.1.6.4.4). |
| cause | Cause | O | 0..1 | When present, this IE shall indicate the cause for the requested modification. |

##### 6.1.6.2.16 Type: VsmfUpdatedData

Table 6.1.6.2.16-1: Definition of type VsmfUpdatedData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| qosFlowsAddModList | array(QosFlowItem) | C | 0..N | This IE shall be present if QoS flows have been successfully established or modified. |
| qosFlowsRelList | array(QosFlowItem) | C | 0..N | This IE shall be present if QoS flows have been successfully released. |
| qosFlowsFailedtoAddModList | array(QosFlowItem) | C | 0..N | This IE shall be present if QoS flows failed to be established or modified. |
| qosFlowsFailedtoRelList | array(QosFlowItem) | C | 0..N | This IE shall be present if QoS flows failed to be released. |
| n1SmInfoFromUe | RefToBinaryData | C | 0..1 | This IE shall be present if the V-SMF has received known N1 SM information from the UE that does not need to be interpreted by the V-SMF. When present, this IE shall reference the n1SmInfoFromUe binary data (see subclause 6.1.6.4.4). |
| unknownN1SmInfo | RefToBinaryData | C | 0..1 | This IE shall be present if the V-SMF has received unknown N1 SM information from the UE. When present, this IE shall reference the unknownN1SmInfo binary data (see subclause 6.1.6.4.4). |
| ueLocation | UserLocation | C | 0..1 | This IE shall be present if it is available and QoS flows have been successfully established, modified or released.  When present, this IE shall contain the UE location information. |
| ueTimeZone | TimeZone | C | 0..1 | This IE shall be present if it is available and QoS flows have been successfully established, modified or released.  When present, this IE shall contain the new UE Time Zone. |
| addUeLocation | UserLocation | O | 0..1 | Additional UE location.  This IE may be present, if anType previously reported is a non-3GPP access and a valid 3GPP access user location information is available.  When present, it shall contain:  - the last known 3GPP access user location; and  - the timestamp, if available, indicating the UTC time when the addUeLocation information was acquired. |
| assignedEbiList | array(EbiArpMapping) | C | 0..N | This IE shall be present if the AMF assigned the requested EBI(s). When present, it shall contain the EBIs that were successfully assigned. |
| failedToAssignEbiList | array(Arp) | C | 0..N | This IE shall be present if the AMF failed to assign EBIs for a set of ARPs. |
| releasedEbiList | array(EpsBearerId) | C | 0..N | This IE shall be present if the NF Service Consumer requested the revoke EBI(s) or if the AMF revoked already assigned EBI(s) for this PDU session towards the V-SMF. This IE shall contain the list of EBI(s) released for this PDU session at the AMF. |

##### 6.1.6.2.17 Type: StatusNotification

Table 6.1.6.2.17-1: Definition of type StatusNotification

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| statusInfo | StatusInfo | M | 1 | This IE shall contain status information about the PDU session. |

##### 6.1.6.2.18 Type: QosFlowItem

Table 6.1.6.2.18-1: Definition of type QosFlowItem

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| qfi | Qfi | M | 1 | This IE shall contain the QoS Flow Identifier. |
| cause | Cause | O | 0..1 | When present, this IE shall contain cause information. |

##### 6.1.6.2.19 Type: QosFlowSetupItem

Table 6.1.6.2.19-1: Definition of type QosFlowSetupItem

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| qfi | Qfi | M | 1 | This IE shall contain the QoS Flow Identifier. |
| qosRules | Bytes | M | 1 | This IE shall contain the QoS Rule(s) associated to the QoS flow to be sent to the UE. It shall be encoded as the Qos rules IE specified in subclause 9.8.4.7 of 3GPP TS 24.501 [7]. |
| qosFlowDescription | Bytes | O | 0..1 | When present, this IE shall contain the description of the QoS Flow level Qos parameters to be sent to the UE. It shall be encoded as the Qos flow descriptions IE specified in subclause 9.10.4.z of 3GPP TS 24.501 [7], encoding one single Qos flow description for the QoS flow to be set up. |
| qosFlowProfile | QosFlowProfile | O | 0..1 | When present, this IE shall contain the description of the QoS Flow level Qos parameters. |

##### 6.1.6.2.20 Type: QosFlowAddModifyRequestItem

Table 6.1.6.2.20-1: Definition of type QosFlowAddModifyRequestItem

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| qfi | Qfi | M | 1 | This IE shall contain the QoS Flow Identifier. |
| qosRules | Bytes | O | 0..1 | When present, this IE shall contain the QoS Rule(s) to be sent to the UE. It shall be encoded as the Qos rules IE specified in subclause 9.8.4.7 of 3GPP TS 24.501 [7]. |
| qosFlowDescription | Bytes | O | 0..1 | When present, this IE shall contain the description of the QoS Flow level Qos parameters to be sent to the UE. It shall be encoded as the Qos flow descriptions IE specified in subclause 9.10.4.z of 3GPP TS 24.501 [7], encoding one single Qos flow description for the QoS flow to be added or modified. |
| qosFlowProfile | QosFlowProfile | O | 0..1 | When present, this IE shall contain the description of the QoS Flow level QoS parameters.  When modifying a QoS flow, the IE shall only contain the QoS Flow profile's attributes which are modified. |

##### 6.1.6.2.21 Type: QosFlowReleaseRequestItem

Table 6.1.6.2.21-1: Definition of type QosFlowReleaseRequestItem

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| qfi | Qfi | M | 1 | This IE shall contain the QoS Flow Identifier. |
| qosRules | Bytes | O | 0..1 | When present, this IE shall contain the QoS Rule(s) to be sent to the UE. It shall be encoded as the Qos rules IE specified in subclause 9.8.4.7 of 3GPP TS 24.501 [7]. |
| qosFlowDescription | Bytes | O | 0..1 | When present, this IE shall contain the description of the QoS Flow level Qos parameters to be sent to the UE. It shall be encoded as the Qos flow descriptions IE specified in subclause 9.10.4.z of 3GPP TS 24.501 [7], encoding one single Qos flow description for the QoS flow to be released. |

##### 6.1.6.2.22 Type: QosFlowProfile

Table 6.1.6.2.22-1: Definition of type QosFlowProfile

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| 5qi | 5Qi | M | 1 | This IE shall contain the 5G QoS Identifier (5QI) of the QoS flow. |
| nonDynamic5Qi | NonDynamic5Qi | C | 0..1 | When present, this IE shall indicate the QoS Characteristics for a standardized or pre-configured 5QI for downlink and uplink.  See NOTE 1. |
| dynamic5Qi | Dynamic5Qi | C | 0..1 | When present, this IE shall indicate the QoS Characteristics for a Non-standardised or not pre-configured 5QI for downlink and uplink.  See NOTE 1. |
| arp | Arp | C | 0..1 | This IE shall be present when establishing a QoS flow; it may be present when modifying a QoS flow.  When present, this IE shall contain the Allocation and Retention Priority (ARP) assigned to the QoS flow. |
| gbrQosFlowInfo | GbrQosFlowInformation | C | 0..1 | This IE shall be present when establishing a GBR QoS flow or if the GBR QoS flow information is modified. |
| rqa | ReflectiveQoSAttribute | O | 0..1 | This IE may be present for a non-GBR QoS flow and it shall be ignored otherwise. When present, it shall indicate whether certain traffic on this QoS flow may be subject to Reflective QoS. |
| NOTE 1: Either the nonDynamic5Qi IE or the dynamic5Qi IE may be present when establishing a QoS flow. Either the nonDynamic5Qi IE or the dynamic5Qi IE may be present when modifying a QoS flow; when present, the received nonDynamic5Qi IE or dynamic5Qi IE shall replace any value received previously for this IE. | | | | |

##### 6.1.6.2.23 Type: GbrQosFlowInformation

Table 6.1.6.2.23-1: Definition of type GbrQosFlowInformation

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| maxFbrDl | BitRate | M | 1 | This IE shall contain the Maximum Bit Rate in Downlink. See 3GPP TS 23.501 [2]. |
| maxFbrUl | BitRate | M | 1 | This IE shall contain the Maximum Bit Rate in Uplink. See 3GPP TS 23.501 [2]. |
| guaFbrDl | BitRate | M | 1 | This IE shall contain the Guaranted Bit Rate in Downlink. See 3GPP TS 23.501 [2]. |
| guaFbrUl | BitRate | M | 1 | This IE shall contain the Guaranted Bit Rate in Uplink. See 3GPP TS 23.501 [2]. |
| notifControl | NotificationControl | O | 0..1 | When present, this IE shall indicate whether notifications are requested from the RAN when the GFBR can no longer (or again) be fulfilled for a QoS flow during the lifetime of the QoS flow. See 3GPP TS 23.501 [2]. |
| maxPacketLossRateDl | PacketLossRate | O | 0..1 | When present, this IE shall indicate the maximum rate for lost packets that can be tolerated in the downlink direction. See 3GPP TS 23.501 [2]. |
| maxPacketLossRateUl | PacketLossRate | O | 0..1 | When present, this IE shall indicatethe maximum rate for lost packets that can be tolerated in the Uplink direction. See 3GPP TS 23.501 [2]. |

##### 6.1.6.2.24 Type: QosFlowNotifyItem

Table 6.1.6.2.24-1: Definition of type QosFlowNotifyItem

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| qfi | Qfi | M | 1 | This IE shall contain the QoS Flow Identifier. |
| notificationCause | NotificationCause | M | 1 |  |

##### 6.1.6.2.25 Type: Void

##### 6.1.6.2.26 Type: Void

##### 6.1.6.2.27 Type: SMContextRetrievedData

Table 6.1.6.2.27-1: Definition of type SmContextRetrievedData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| ueEpsPdnConnection | EpsPdnCnxContainer | M | 1 | This IE shall contain an MME/SGSN UE EPS PDN Connection including the mapped EPS bearer context(s). |

##### 6.1.6.2.28 Type: TunnelInfo

Table 6.1.6.2.28-1: Definition of type TunnelInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| ipv4Addr | Ipv4Addr | C | 0..1 | When present, this IE shall contain the GTP tunnel IPv4 address.  At least one of the ipv4Addr or ipv6Addr shall be present. Both may be present. |
| ipv6Addr | Ipv6Addr | C | 0..1 | When present, this IE shall contain the GTP tunnel IPv6 address.  At least one of the ipv4Addr or ipv6Addr shall be present. Both may be present. |
| gtpTeid | Teid | M | 1 | This IE shall contain the 4-octet GTP tunnel endpoint identifier.  If both ipv4Addr and ipv6Addr are present, the TEID shall be shared by both addresses. |

##### 6.1.6.2.29 Type: StatusInfo

Table 6.1.6.2.29-1: Definition of type StatusInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| resourceStatus | ResourceStatus | M | 1 | This IE shall indicate the status of the SM context or PDU session resource. |
| cause | Cause | O | 0..1 | When present, this IE shall indicate the cause for the resource status change. |

##### 6.1.6.2.30 Type: VsmfUpdateError

Table 6.1.6.2.30-1: Definition of type VsmfUpdateError

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | |
| error | ProblemDetails | M | 1 | More information on the error shall be provided in the "cause" attribute of the "ProblemDetails" structure. | |
| pti | ProcedureTransactionId | C | 0..1 | This IE shall be present if available. When present, it shall contain the PTI value received from the UE. | |
| n1smCause | string | C | 0..1 | This IE shall be present if available.  When present, it shall contain the 5GSM cause received from the UE.  It shall be encoded as two characters in hexadecimal representation with each character taking a value of "0" to "9" or "A" to "F", and represent the cause value of the 5GSM cause IE specified in subclause 9.8.4.2 of 3GPP TS 24.501 [7].  Example: the cause "Invalid mandatory information" shall be encoded as "60".  See NOTE. | |
| n1SmInfoFromUe | RefToBinaryData | C | 0..1 | This IE shall be present if the V-SMF has received known N1 SM information from the UE that does not need to be interpreted by the V-SMF. When present, this IE shall reference the n1SmInfoFromUe binary data (see subclause 6.1.6.4.4). | |
| unknownN1SmInfo | RefToBinaryData | C | 0..1 | This IE shall be present if the V-SMF has received unknown N1 SM information from the UE. When present, this IE shall reference the unknownN1SmInfo binary data (see subclause 6.1.6.4.4). | |
| failedToAssignEbiList | array(Arp) | C | 0..N | This IE shall be present if the AMF failed to assign the requested EBIs. | |
| ngApCause | NgApCause | C | 0..1 | This IE shall be present, if the information is available and if this information is permitted to be sent to the H-SMF operator according to the V-SMF operator's policy. | |
| 5GMmCauseValue | 5GMmCause | C | 0..1 | The V-SMF shall include this IE if it received it from the AMF and if this information is permitted to be sent to the H-SMF operator according to the V-SMF operator's policy. | |
| NOTE: This IE is sent as a separate IE rather than within the n1SmInfoFromUE binary data because the 5GSM cause IE is defined as a "V" IE (i.e. without a Type field) in the NAS PDU Session Modification Reject message. | | | | | |

##### 6.1.6.2.31 Type: EpsPdnCnxInfo

Table 6.1.6.2.31-1: Definition of type EpsPdnCnxInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| pgwS8cFteid | Bytes | M | 1 | Base64-encoded characters, encoding the PGW S8 F-TEID for Control Plane as specified in Figure 8.22-1 of 3GPP TS 29.274 [16]. |
| pgwNodeName | Bytes | C | 0..1 | Base64-encoded characters, encoding the PGW FQDN IE as specified in Figure 8.66-1 of 3GPP TS 29.274 [16]. It shall be present, if it is available. |

##### 6.1.6.2.32 Type: EpsBearerInfo

Table 6.1.6.2.32-1: Definition of type EpsBearerInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| ebi | EpsBearerId | M | 1 | EPS Bearer ID |
| pgwS8uFteid | Bytes | M | 1 | Base64-encoded characters, encoding the PGW S8 F-TEID for User Plane as specified in Figure 8.22-1 of 3GPP TS 29.274 [16]. |
| bearerLevelQoS | Bytes | M | 1 | Base64-encoded characters, encoding the Bearer QoS IE as specified in Figure 8.15-1 of 3GPP TS 29.274 [16]. |

##### 6.1.6.2.33 Type: PduSessionNotifyItem

Table 6.1.6.2.33-1: Definition of type PduSessionNotifyItem

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| notificationCause | NotificationCause | M | 1 |  |

##### 6.1.6.2.34 Type: EbiArpMapping

Table 6.1.6.2.34-1: Definition of type EbiArpMapping

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| epsBearerId | EpsBearerId | M | 1 | This IE shall contain the EPS bearer identities. |
| arp | Arp | M | 1 | This IE shall contain the ARP corresponding to the EBI. |

##### 6.1.6.2.35 Type: SmContextCreateError

Table 6.1.6.2.35-1: Definition of type SmContextCreateError

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| error | ProblemDetails | M | 1 | More information on the error shall be provided in the "cause" attribute of the "ProblemDetails" structure. |
| n1SmMsg | RefToBinaryData | C | 0..1 | This IE shall be present, if an N1 SM information is received in the request and the SMF is able to return N1 SM information to the UE.  When present, it shall reference the N1 SM Message binary data (see subclause 6.1.6.4.2). |

##### 6.1.6.2.36 Type: SMContextUpdateError

Table 6.1.6.2.36-1: Definition of type SmContextUpdateError

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| error | ProblemDetails | M | 1 | More information on the error shall be provided in the "cause" attribute of the "ProblemDetails" structure. |
| n1SmMsg | RefToBinaryData | C | 0..1 | This IE shall be present, if N1 SM information needs to be returned to the UE.  When present, it shall reference the N1 SM Message binary data (see subclause 6.1.6.4.2). |
| n2SmInfo | RefToBinaryData | C | 0..1 | This IE shall be present, if N2 SM information needs to be returned to the NG-RAN.  When present, it shall reference the N2 SM Message binary data (see subclause 6.1.6.4.3). |
| n2SmInfoType | N2SmInfoType | C | 0..1 | This IE shall be present if "n2SmInfo" attribute is present.  When present, this IE shall indicate the NG AP IE type for the NG AP SMF related IE container carried in "n2SmInfo" attribute. |
| upCnxState | UpCnxState | C | 0..1 | This IE shall be present if the SMF was requested to activate or deactivate the user plane connection of the PDU session in the corresponding request.  When present, it shall be set as specified in subclause 5.2.2.3.2. |

##### 6.1.6.2.37 Type: PduSessionCreateError

Table 6.1.6.2.37-1: Definition of type PduSessionCreateError

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| error | ProblemDetails | M | 1 | More information on the error shall be provided in the "cause" attribute of the "ProblemDetails" structure. |
| n1smCause | string | C | 0..1 | This IE shall be present if the request included n1SmInfoFromUe.  When present, it shall contain the 5GSM cause the H-SMF requires the V-SMF to return to the UE. It shall be encoded as two characters in hexadecimal representation with each character taking a value of "0" to "9" or "A" to "F", and represent the cause value of the 5GSM cause IE specified in subclause 9.8.4.2 of 3GPP TS 24.501 [7].  Example: the cause "Invalid mandatory information" shall be encoded as "60".  See NOTE. |
| n1SmInfoToUe | RefToBinaryData | C | 0..1 | This IE shall be present if the H-SMF needs to send N1 SM information to the UE that does not need to be interpreted by the V-SMF. When present, this IE shall reference the n1SmInfoToUe binary data (see subclause 6.1.6.4.4). |
| NOTE: This IE contains information that the V-SMF shall transfer to the UE without interpretation. It is sent as a separate IE rather than within the n1SmInfoToUE binary data because the 5GSM cause IE is defined as a "V" IE (i.e. without a Type field) in the NAS PDU Session Establishment Reject message. | | | | |

##### 6.1.6.2.38 Type: MmeCapabilities

Table 6.1.6.2.38-1: Definition of type MmeCapabilities

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| nonIpSupported | boolean | C | 0..1 | This IE shall be present if non-IP PDN type is supported. It may be present otherwise. When present, this IE shall be set as follows:  - true: non-IP PDN type is supported;  - false (default): non-IP PDN type is not supported. |

##### 6.1.6.2.39 Type: Void

#### 6.1.6.3 Simple data types and enumerations

##### 6.1.6.3.1 Introduction

This subclause defines simple data types and enumerations that can be referenced from data structures defined in the previous subclauses.

##### 6.1.6.3.2 Simple data types

The simple data types defined in table 6.1.6.3.2-1 shall be supported.

Table 6.1.6.3.2-1: Simple data types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
| ProcedureTransactionId | integer | Unsigned integer representing a Procedure Transaction Identity, within the range 0 to 255, as specified in 3GPP TS 24.007 [8]. In an OpenAPI Specification [15] schema, the format shall be designated as "ProcedureTransactionId". |
| EpsBearerId | integer | Unsigned integer identifying an EPS bearer, within the range 0 to 15, as specified in 3GPP TS 24.007 [8]. In an OpenAPI Specification [15] schema, the format shall be designated as "EpsBearerId". |
| EpsPdnCnxContainer | string | String with format "byte" as defined in OpenAPI Specification [15], i.e. base64-encoded characters, encoding the UeEpsPdnConnection IE specified in Table 7.3.1-2 or Table 7.3.6-2 of 3GPP TS 29.274 [16] for the N26 interface.  In an OpenAPI Specification [15] schema, the format shall be designated as "EpsPdnCnxContainer". |
| EpsBearerContainer | string | String with format "byte" as defined in OpenAPI Specification [15], i.e. base64-encoded characters, encoding the Bearer Context IE specified in Table 7.3.2-2 of 3GPP TS 29.274 [16]. In an OpenAPI Specification [15] schema, the format shall be designated as "EpsBearerContainer". |
| Teid | string | 4-octet GTP tunnel endpoint identifier, as defined in 3GPP TS 29.274 [16], in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the TEID shall appear first in the string, and the character representing the 4 least significant bit of the TEID shall appear last in the string.  Pattern: "[A-Fa-f0-9]{8}"  Example:  A GTP TEID 0x5BD60076 shall be encoded as "5BD60076". |

##### 6.1.6.3.3 Enumeration: UpCnxState

The enumeration UpCnxState represents the state of the user plane connection of a PDU session. It shall comply with the provisions defined in table 6.1.6.3.3-1.

Table 6.1.6.3.3-1: Enumeration UpCnxState

|  |  |
| --- | --- |
| Enumeration value | Description |
| "ACTIVATED" | A N3 tunnel is established between the 5G-AN and UPF |
| "DEACTIVATED" | No N3 tunnel is established between the 5G-AN and UPF. |
| "ACTIVATING" | A N3 tunnel is being established (the 5G-AN's F-TEID for downlink traffic is not assigned yet). |

##### 6.1.6.3.4 Enumeration: HoState

The enumeration HoState represents the handover state of a PDU session. It shall comply with the provisions defined in table 6.1.6.3.4-1.

Table 6.1.6.3.4-1: Enumeration HoState

|  |  |
| --- | --- |
| Enumeration value | Description |
| "NONE" | No handover is in progress for the PDU session. |
| "PREPARING" | A handover is in preparation for the PDU session; see subclause 5.2.2.3.4.1. |
| "PREPARED" | A handover is prepared for the PDU session; see subclause 5.2.2.3.4.1. |
| "COMPLETED" | The handover is completed. |
| "CANCELLED" | The handover is cancelled. |

##### 6.1.6.3.5 Enumeration: RequestType

The enumeration RequestType indicates the type of a PDU session creation request. It shall comply with the provisions defined in table 6.1.6.3.5-1.

Table 6.1.6.3.5-1: Enumeration RequestType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "INITIAL\_REQUEST" | Request to establish a new PDU session. |
| "EXISTING\_PDU\_SESSION" | Request referring to an existing PDU session. |
| "INITIAL\_EMERGENCY\_REQUEST" | Request to establish a new PDU session for Emergency Services. |
| "EXISTING\_EMERGENCY\_PDU\_SESSION" | Request referring to an existing PDU session for Emergency Services. |

##### 6.1.6.3.6 Enumeration: RequestIndication

The enumeration RequestIndication indicates the request type. It shall comply with the provisions defined in table 6.1.6.3.6-1.

Table 6.1.6.3.6-1: Enumeration RequestIndication

|  |  |
| --- | --- |
| Enumeration value | Description |
| "UE\_REQ\_PDU\_SES\_MOD" | UE Requested PDU Session Modification |
| "UE\_REQ\_PDU\_SES\_REL" | UE Requested PDU Session Release |
| "PDU\_SES\_MOB" | PDU Session Mobility (e.g. between 3GPP and non-3GPP access, or from EPS to 5GS with N26 interface) |
| "NW\_REQ\_PDU\_SES\_AUTH" | Network Requested PDU Session Authentication |
| "NW\_REQ\_PDU\_SES\_MOD" | Network Requested PDU Session Modification |
| "NW\_REQ\_PDU\_SES\_REL" | Network Requested PDU Session Release |
| "EBI\_ASSIGNMENT\_REQ" | EPS Bearer ID Assignment Request |

##### 6.1.6.3.7 Enumeration: NotificationCause

The enumeration NotificationCause indicates the cause of a notification. It shall comply with the provisions defined in table 6.1.6.3.7-1.

Table 6.1.6.3.7-1: Enumeration NotificationCause

|  |  |
| --- | --- |
| Enumeration value | Description |
| "QOS\_FULFILLED" | The QoS targets are fulfilled again for the GBR QoS flow. |
| "QOS\_NOT\_FULFILLED" | The QoS targets are no longer fulfilled for the GBR QoS flow. |
| "UP\_SEC\_FULFILLED" | The user plane security enforcement "Preferred" is fulfilled again for the PDU session. |
| "UP\_SEC\_NOT\_FULFILLED" | The user plane security enforcement "Preferred" is not fulfilled for the PDU session. |

##### 6.1.6.3.8 Enumeration: Cause

The enumeration Cause indicates a cause information. It shall comply with the provisions defined in table 6.1.6.3.8-1.

Table 6.1.6.3.8-1: Enumeration Cause

|  |  |
| --- | --- |
| Enumeration value | Description |
| "REL\_DUE\_TO\_HO" | Release due to Handover |
| "EPS\_FALLBACK" | Mobility due to EPS fallback for IMS voice is on-going. |
| "REL\_DUE\_TO\_UP\_SEC" | Release due to user plane Security requirements that cannot be fulfilled. |
| "DNN\_CONGESTION" | Release due to the DNN based congestion control. |
| "S-NSSAI\_CONGESTION" | Release due to the S-NSSAI based congestion control. |
| "REL\_DUE\_TO\_REACTIVATION" | Release due to PDU session reactivation. |
| "5G\_AN\_NOT\_RESPONDING" | The 5G AN did not respond to the request initiated by the network. |
| "REL\_DUE\_TO\_SLICE\_NOT\_AVAILABLE" | Release due to the associated S-NSSAI becomes no longer available. |

##### 6.1.6.3.9 Enumeration: ResourceStatus

The enumeration ResourceStatus indicates the status of an SM context or PDU session resource. It shall comply with the provisions defined in table 6.1.6.3.9-1.

Table 6.1.6.3.9-1: Enumeration ResourceStatus

|  |  |
| --- | --- |
| Enumeration value | Description |
| "RELEASED" | The SM context or PDU session resource is released. |

##### 6.1.6.3.10 Enumeration: DnnSelectionMode

The enumeration DnnSelectionMode indicates whether the DNN of a PDU session being established corresponds to an explicitly subscribed DNN or to the usage of a wildcard subscription. It shall comply with the provisions defined in table 6.1.6.3.10-1.

Table 6.1.6.3.10-1: Enumeration DnnSelectionMode

|  |  |
| --- | --- |
| Enumeration value | Description |
| "VERIFIED" | UE or network provided DNN, subscription verified |
| "UE\_DNN\_NOT\_VERIFIED" | UE provided DNN, subscription not verified |
| "NW\_DNN\_NOT\_VERIFIED" | Network provided DNN, subscription not verified |

##### 6.1.6.3.11 Enumeration: EpsInterworkingIndication

The enumeration EpsInterworkingIndication indicates whether and how the PDU session will possibly be moved to EPS.

Table 6.1.6.3.11-1: Enumeration EpsInterworkingIndication

|  |  |
| --- | --- |
| Enumeration value | Description |
| "NONE" | The PDU session cannot be moved EPS. |
| "WITH\_N26" | The PDU session may possibly be moved to EPS, with N26 interface supported during EPS interworking procedures. |
| "WITHOUT\_N26" | The PDU session may possibly be moved to EPS, without N26 interface supported during EPS interworking procedures. |

##### 6.1.6.3.12 Enumeration: N2SmInfoType

Table 6.1.6.3.12-1: Enumeration N2SmInfoType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "PDU\_RES\_SETUP\_REQ" | PDU Session Resource Setup Request Transfer |
| "PDU\_RES\_SETUP\_RSP" | PDU Session Resource Setup Response Transfer |
| "PDU\_RES\_SETUP\_FAIL" | PDU Session Resource Setup Unsuccessful Transfer |
| "PDU\_RES\_REL\_CMD" | PDU Session Resource Release Command Transfer |
| "PDU\_RES\_REL\_RSP" | PDU Session Resource Release Response Transfer |
| "PDU\_RES\_MOD\_REQ" | PDU Session Resource Modify Request Transfer |
| "PDU\_RES\_MOD\_RSP" | PDU Session Resource Modify Response Transfer |
| "PDU\_RES\_MOD\_FAIL" | PDU Session Resource Modify Unsuccessful Transfer |
| "PDU\_RES\_NTY" | PDU Session Resource Notify Transfer |
| "PDU\_RES\_NTY\_REL" | PDU Session Resource Notify Released Transfer |
| "PDU\_RES\_MOD\_IND" | PDU Session Resource Modify Indication Transfer |
| "PDU\_RES\_MOD\_CFM" | PDU Session Resource Modify Confirm Transfer |
| "PATH\_SWITCH\_REQ" | Path Switch Request Transfer |
| "PATH\_SWITCH\_SETUP\_FAIL" | Path Switch Request Setup Failed Transfer |
| "PATH\_SWITCH\_REQ\_ACK" | Path Switch Request Acknowledge Transfer |
| "PATH\_SWITCH\_REQ\_FAIL" | Path Switch Request Unsuccessful Transfer |
| "HANDOVER\_REQUIRED" | Handover Required Transfer |
| "HANDOVER\_CMD" | Handover Command Transfer |
| "HANDOVER\_PREP\_FAIL" | Handover Preparation Unsuccessful Transfer |
| "HANDOVER\_REQ\_ACK" | Handover Request Acknowledge Transfer |
| "HANDOVER\_RES\_ALLOC\_FAIL" | Handover Resource Allocation Unsuccessful Transfer |

#### 6.1.6.4 Binary data

##### 6.1.6.4.1 Introduction

This subclause defines the binary data that shall be supported in a binary body part in an HTTP multipart message (see subclauses 6.1.2.2.2 and 6.1.2.4).

##### 6.1.6.4.2 N1 SM Message

N1 SM Messageshall encode a 5GS NAS SM message as specified in 3GPP TS 24.501 [7], using the vnd.3gpp.5gnas content-type.

N1 SM Message may encode any 5GS NAS SM message specified in 3GPP TS 24.501 [7], as summarized in Table 6.1.6.4.2-1.

Table 6.1.6.4.2-1: N1 SM Message content

|  |  |
| --- | --- |
| 5GS NAS message | Reference  (3GPP TS 24.501 [7]) |
| PDU session establishment request | 8.3.1 |
| PDU session establishment accept | 8.3.2 |
| PDU session establishment reject | 8.3.3 |
| PDU session authentication command | 8.3.4 |
| PDU session authentication complete | 8.3.5 |
| PDU session modification request | 8.3.6 |
| PDU session modification reject | 8.3.7 |
| PDU session modification command | 8.3.8 |
| PDU session modification complete | 8.3.9 |
| PDU session modification command reject | 8.3.10 |
| PDU session release request | 8.3.11 |
| PDU session release reject | 8.3.12 |
| PDU session release command | 8.3.13 |
| PDU session release complete | 8.3.14 |
| 5GSM status | 8.3.15 |

##### 6.1.6.4.3 N2 SM Information

N2 SM Information shall encode NG Application Protocol (NGAP) IEs, as specified in subclause 9.4 of 3GPP TS 38.413 [9] (ASN.1 encoded), using the vnd.3gpp.ngap content-type.

N2 SM Information may encode any NGAP SMF related IE specified in 3GPP TS 38.413 [9], as summarized in Table 6.1.6.4.3-1.

Table 6.1.6.4.3-1: N2 SM Information content

|  |  |  |
| --- | --- | --- |
| N2 SM IE | Reference  (3GPP TS 38.413 [9]) | Related NGAP message |
| PDU Session Resource Setup Request Transfer | 9.3.4.1 | PDU Session Resource Setup Request, Initial Context Setup Request |
| PDU Session Resource Setup Response Transfer | 9.3.4.2 | PDU Session Resource Setup Response, Initial Context Setup Response |
| Additional PDU Session Resource Setup Response Transfer | 9.3.4.2 | PDU Session Resource Setup Response |
| PDU Session Resource Release Command Transfer | 9.3.4.3 | PDU Session Resource Release Command |
| PDU Session Resource Release Response Transfer | 9.3.4.4 | PDU Session Resource Release Response |
| PDU Session Resource Modify Request Transfer | 9.3.4.5 | PDU Session Resource Modify Request |
| PDU Session Resource Modify Response Transfer | 9.3.4.6 | PDU Session Resource Modify Response |
| PDU Session Resource Notify Transfer | 9.3.4.7 | PDU Session Resource Notify |
| PDU Session Resource Modify Indication Transfer | 9.3.4.8 | PDU Session Resource Modify Indication |
| PDU Session Resource Modify Confirm Transfer | 9.3.4.9 | PDU Session Resource Modify Confirm |
| Path Switch Request Transfer | 9.3.4.10 | Path Switch Request |
| Path Switch Request Acknowledge Transfer | 9.3.4.11 | Path Switch Request Acknowledge |
| Handover Required Transfer | 9.3.4.1 | Handover Required |
| Handover Command Transfer | 9.3.4.12 | Handover Command |
| Handover Request Transfer | 9.3.4.1 | Handover Request |
| Handover Request Acknowledge Transfer | 9.3.4.1 | Handover Request Acknowledge |

##### 6.1.6.4.4 n1SmInfoFromUe, n1SmInfoToUe, unknownN1SmInfo

n1SmInfoFromUe, n1SmInfoToUe and unknownN1SmInfo shall encode one or more NAS SM IEs, including the Type and Length fields, as specified in 3GPP TS 24.501 [7], using the vnd.3gpp.5gnas content-type.

Subclause 5.2.3.1 specifies the information that shall be included in these payloads.

n1SmInfoFromUe and n1SmInfoToUe may encode the 5GS NAS IEs listed in tables 6.1.6.4.4-1 and 6.1.6.4.4-2.

Table 6.1.6.4.4-1: n1SmInfoFromUE content

|  |  |  |
| --- | --- | --- |
| 5GS NAS IE | Reference  (3GPP TS 24.501 [7]) | Related NAS SM message |
| Message type | 9.7 | All NAS SM messages |
| PDU session type | 9.8.4.6 | PDU Session Establishment Request |
| SSC mode | 9.8.4.10 | PDU Session Establishment Request |
| SM PDU DN request container | 9.8.4.9 | PDU Session Establishment Request |
| Extended protocol configuration options | 9.8.4.3 | PDU Session Establishment Request  PDU Session Authentication Complete  PDU Session Modification Request  PDU Session Modification Complete  PDU Session Modification Command Reject  PDU Session Release Request  PDU Session Release Complete |
| EAP message | 9.8.3.14 | PDU Session Authentication Complete |
| Requested QoS rules | 9.8.4.7 | PDU Session Modification Request |
| Requested QoS flow descriptions | 9.10.4.z | PDU Session Modification Request |
| 5GSM capability | 9.8.4.1 | PDU Session Establishment Request  PDU Session Modification Request  See NOTE. |
| NOTE: The 5GSM capability IE shall be encoded as received from the UE. It may contain UE capabilities that the V-SMF only needs to transfer to the H-SMF, e.g. support of reflective QoS, and/or capabilities to be interpreted and used by the V-SMF. | | |

Table 6.1.6.4.4-2: n1SmInfoToUE parameters

|  |  |  |
| --- | --- | --- |
| 5GS NAS IE | Reference  (3GPP TS 24.501 [7]) | Related NAS SM message |
| Message type | 9.7 | All NAS SM messages |
| RQ timer value | 9.8.4.4 | PDU Session Establishment Accept  PDU Session Modification Command |
| EAP message | 9.8.3.16 | PDU Session Establishment Accept  PDU Session Establishment Reject  PDU Session Authentication Command |
| Extended protocol configuration options | 9.8.4.3 | PDU Session Establishment Accept  PDU Session Establishment Reject  PDU Session Authentication Command  PDU Session Modification Reject  PDU Session Modification Command  PDU Session Release Reject  PDU Session Release Command |
| 5GSM cause | 9.8.4.2 | PDU Session Establishment Accept  PDU Session Modification Command  See NOTE. |
| NOTE: This IE indicates the 5GSM cause the H-SMF requires the V-SMF to send to the UE. The V-SMF shall transfer the received value to the UE without interpretation.  This information is defined as a "V" IE (i.e. without a Type field) in other NAS messages, e.g. PDU Session Establishment Reject message, in which case it shall be sent as a separate n1SmCause IE over N16 and not within the n1SmInfoToUE binary data. | | |

The Message Type shall be present and encoded as the first 5GS NAS IE in any n1SmInfoFromUe, n1SmInfoToUe and unknownN1SmInfo binary data, to enable the receiver to decode the 5GS NAS IEs.

NOTE: The Information Element Identifier (see subclause 11.2.1.1.3 of 3GPP TS 24.007 [8]) of a 5GS NAS IE uniquely identifies an IE in a given message.

### 6.1.7 Error Handling

#### 6.1.7.1 General

HTTP error handling shall be supported as specified in subclause 5.2.4 of 3GPP TS 29.500 [4].

#### 6.1.7.2 Protocol Errors

Protocol errors handling shall be supported as specified in subclause 5.2.7 of 3GPP TS 29.500 [4].

#### 6.1.7.3 Application Errors

The common application errors defined in Table 5.2.7.2-1 of 3GPP TS 29.500 [4] may be used for the Nsmf\_PDUSession service.

The following application errors listed in Table 6.1.7.3-1 are specific to the Nsmf\_PDUSession service.

Table 6.1.7.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| Application Error | HTTP status code | Description |
| N1\_SM\_ERROR | 403 Forbidden | This indicates that an error, other than those listed in this table, was detected when processing the N1 SM information received in the request, e.g. N1 SM protocol error. |
| SNSSAI\_DENIED | 403 Forbidden | The subscriber does not have the necessary subscription to access the SNSSAI. |
| DNN\_DENIED | 403 Forbidden | The subscriber does not have the necessary subscription to access the DNN. |
| PDUTYPE\_DENIED | 403 Forbidden | The subscriber does not have the necessary subscription for the requested PDU session type. |
| SSC\_DENIED | 403 Forbidden | The subscriber does not have the necessary subscription for the requested SSC mode. |
| SUBSCRIPTION\_DENIED | 403 Forbidden | This indicates an error, other than those listed in this table, due to lack of necessary subscription to serve the UE request. |
| DNN\_NOT\_SUPPORTED | 403 Forbidden | The DNN is not supported by the SMF. |
| PDUTYPE\_NOT\_SUPPORTED | 403 Forbidden | The requested PDU session type is not supported by the SMF for the PDN corresponding to the DNN. |
| SSC\_NOT\_SUPPORTED | 403 Forbidden | The requested SSC mode is not supported by the SMF for the PDN corresponding to the DNN. |
| HOME\_ROUTED\_ROAMING\_REQUIRED | 403 Forbidden | It is used in LBO roaming, if the V-SMF is not able to process some part of the N1 SM information that requires Home Routed Roaming. |
| OUT\_OF\_LADN\_SERVICE\_AREA | 403 Forbidden | The PDU session corresponds to a LADN and the UE is outside of the LADN Service Area. |
| N2\_SM\_ERROR | 403 Forbidden | This indicates that an error, other than those listed in this table, was detected when processing the N2 SM information received in the request, e.g. N2 SM protocol error. |
| PRIORITIZED\_SERVICES\_ONLY | 403 Forbidden | The SMF was notified that the UE is reachable only for regulatory prioritized service and the PDU Session to be activated is not for a regulatory prioritized service. |
| PDU\_SESSION\_ANCHOR\_CHANGE | 403 Forbidden | The SMF decided to change the PDU Session Anchor for the PDU Session. |
| TARGET\_MME\_CAPABILITY | 403 Forbidden | A request to retrieve an SM context is rejected due to the target MME not capable to support the PDU session. |
| NO\_EPS\_5GS\_CONTINUITY | 403 Forbidden | It is used during an EPS to 5GS Idle mode mobility or handover, if the PDU session does not support seamless session continuity to 5GS. |
| UNABLE\_TO\_PAGE\_UE | 403 Forbidden | The request is rejected due to a temporarily inability to page the UE. |
| UE\_NOT\_RESPONDING | 403 Forbidden | The UE did not respond to the request initiated by the network, e.g. paging. |
| REJECTED\_BY\_UE | 403 Forbidden | The request is rejected by the UE. |
| REJECTED\_DUE\_VPLMN\_POLICY | 403 Forbidden | The request is rejected due to VPLMN operator policy. |
| HO\_TAU\_IN\_PROGRESS | 403 Forbidden | The request is rejected temporarily due to a mobilty procedure in progress. |
| INTEGRITY\_PROTECTED\_MDR\_NOT\_ACCEPTABLE | 403 Forbidden | The integrity protected maximum data rate value provided by the UE is not acceptable for the PDU session based on local policy at the SMF. This error is applicable when the UP Security Policy for the PDU Session is determined to have Integrity Protection set to "Required".  An NF service consumer that receives this error cause may use it for maintaining KPIs. |
| EBI\_EXHAUSTED | 403 Forbidden | The allocation of EPS Bearer ID failed due to exhaustion of EBI as the maximum number of EBIs has already been allocated to the UE. |
| CONTEXT\_NOT\_FOUND | 404 Not Found | It is used when no context corresponding to the request exists in the SMF. |
| INSUFFICIENT\_RESOURCES\_SLICE | 500 Internal Server Error | The request cannot be provided due to insufficient resources for the specific slice. |
| INSUFFICIENT\_RESOURCES\_SLICE\_DNN | 500 Internal Server Error | The request cannot be provided due to insufficient resources for the specific slice and DNN. |
| DNN\_CONGESTION | 503 Service Unavailable | The SMF has detected congestion for the requested DNN and performs overload control for that DNN which does not allow the PDU session to be established. |
| S-NSSAI\_CONGESTION | 503 Service Unavailable | The SMF has detected congestion for the requested S-NSSAI and performs overload control for that S-NSSAI which does not allow the PDU session to be established. |
| PEER\_NOT\_RESPONDING | 504 Gateway Timeout | No response is received from a remote peer, e.g. from the H-SMF for a HR PDU session. |
| NETWORK\_FAILURE | 504 Gateway Timeout | The request is rejected due to a network problem. |

### 6.1.8 Feature Negotiation

The feature negotiation mechanism specified in subclause 6.6 of 3GPP TS 29.500 [4] shall be used to negotiate the optional features applicable between the SMF and the NF Service Consumer, for the Nsmf\_PDUSession service, if any.

The NF Service Consumer shall indicate the optional features it supports for the Nsmf\_PDUSession service, if any, by including the supportedFeatures attribute in the HTTP POST request when requesting the SMF to create an SM context or a PDU session resource.

The SMF shall determine the supported features for the created SM context or PDU session resource as specified in subclause 6.6 of 3GPP TS 29.500 [4] and shall indicate the supported features by including the supportedFeatures attribute in the representation of the SM context or PDU session resource it returns in the HTTP response confirming the creation of the resource.

The syntax of the supportedFeatures attribute is defined in subclause 5.2.2 of 3GPP TS 29.571 [13].

The following features are defined for the Nsmf\_PDUSession service.

Table 6.1.8-1: Features of supportedFeatures attribute used by Nsmf\_PDUSession service

|  |  |  |  |
| --- | --- | --- | --- |
| Feature Number | Feature | M/O | Description |
|  |  |  |  |
| Feature number: The order number of the feature within the supportedFeatures attribute (starting with 1).  Feature: A short name that can be used to refer to the bit and to the feature.  M/O: Defines if the implementation of the feature is mandatory ("M") or optional ("O").  Description: A clear textual description of the feature. | | | |

### 6.1.9 Security

As indicated in 3GPP TS 33.501 [17], the access to the Nsmf\_PDUSession API shall be authorized by means of the OAuth2 protocol (see IETF RFC 6749 [18]), using the "Client Credentials" authorization grant, where the NRF (see 3GPP TS 29.510 [19]) plays the role of the authorization server.

An NF Service Consumer, prior to consuming services offered by the Nsmf\_PDUSession API, shall obtain a "token" from the authorization server, by invoking the Access Token Request service, as described in 3GPP TS 29.510 [19], subclause 5.4.2.2.

NOTE 1: When multiple NRFs are deployed in a network, the NRF used as authorization server is the same NRF that the NF Service Consumer used for discovering the Nsmf\_PDUSession service.

NOTE 2: The security credentials for accessing a child resource URI of an sm-contexts or pdu-sessions collection distributed on different processing instances or hosts are the same as for accessing the collection URI.

The Nsmf\_PDUSession API does not define any scopes for OAuth2 authorization.

Annex A (normative):  
OpenAPI specification

## A.1 General

This Annex specifies the formal definition of the Nsmf\_PDUSession service. It consists of OpenAPI 3.0.0 specifications, in YAML format.

## A.2 Nsmf\_PDUSession API

openapi: 3.0.0

info:

version: '1.PreR15.1.0'

title: 'Nsmf\_PDUSession'

description: 'SMF PDU Session Service'

servers:

- url: '{apiRoot}/nsmf-pdusession/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501. The sm-contexts and pdu-sessions resources can be distributed on different processing instances or hosts. Thus the authority and/or deployment-specific string of the apiRoot of the created individual sm context and pdu-session resources' URIs may differ from the authority and/or deployment-specific string of the apiRoot of the sm-contexts and pdu-sessions collections' URIs.

security:

- {}

- oAuth2Clientcredentials: []

paths:

/sm-contexts:

post:

summary: Create SM Context

tags:

- SM contexts collection

operationId: PostSmContexts

requestBody:

description: representation of the SM context to be created in the SMF

required: true

content:

multipart/related:

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextCreateData'

binaryDataN1SmMessage:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

callbacks:

smContextStatusNotification:

'{$request.body#/smContextStatusUri}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SmContextStatusNotification'

responses:

'204':

description: successful notification

'307':

description: temporary redirect

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'501':

$ref: 'TS29571\_CommonData.yaml#/components/responses/501'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

responses:

'201':

description: successful creation of an SM context

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextCreatedData'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextCreatedData'

binaryDataN2SmInformation:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN2SmInformation:

contentType: application/vnd.3gpp.ngap

headers:

Content-Id:

schema:

type: string

'307':

description: temporary redirect

'308':

description: permanent redirect

'400':

description: unsuccessful creation of an SM context - bad request

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextCreateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextCreateError'

binaryDataN1SmMessage:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

'403':

description: unsuccessful creation of an SM context - forbidden

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextCreateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextCreateError'

binaryDataN1SmMessage:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

'404':

description: unsuccessful creation of an SM context - not found

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextCreateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextCreateError'

binaryDataN1SmMessage:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'500':

description: unsuccessful creation of an SM context - internal server error

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextCreateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextCreateError'

binaryDataN1SmMessage:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

'501':

$ref: 'TS29571\_CommonData.yaml#/components/responses/501'

'503':

description: unsuccessful creation of an SM context - service unavailable

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextCreateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextCreateError'

binaryDataN1SmMessage:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

'504':

description: unsuccessful creation of an SM context - gateway timeout

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextCreateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextCreateError'

binaryDataN1SmMessage:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/sm-contexts/{smContextRef}/retrieve:

post:

summary: Retrieve SM Context

tags:

- Individual SM context

operationId: RetrieveSmContext

parameters:

- name: smContextRef

in: path

description: SM context reference

required: true

schema:

type: string

requestBody:

description: parameters used to retrieve the SM context

required: false

content:

application/json:

schema:

$ref: '#/components/schemas/SmContextRetrieveData'

responses:

'200':

description: successful retrieval of an SM context

content:

application/json:

schema:

$ref: '#/components/schemas/SmContextRetrievedData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'501':

$ref: 'TS29571\_CommonData.yaml#/components/responses/501'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/sm-contexts/{smContextRef}/modify:

post:

summary: Update SM Context

tags:

- Individual SM context

operationId: UpdateSmContext

parameters:

- name: smContextRef

in: path

description: SM context reference

required: true

schema:

type: string

requestBody:

description: representation of the updates to apply to the SM context

required: true

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextUpdateData'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextUpdateData'

binaryDataN1SmMessage:

type: string

format: binary

binaryDataN2SmInformation:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

binaryDataN2SmInformation:

contentType: application/vnd.3gpp.ngap

headers:

Content-Id:

schema:

type: string

responses:

'200':

description: successful update of an SM context with content in the response

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextUpdatedData'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextUpdatedData'

binaryDataN1SmMessage:

type: string

format: binary

binaryDataN2SmInformation:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

binaryDataN2SmInformation:

contentType: application/vnd.3gpp.ngap

headers:

Content-Id:

schema:

type: string

'204':

description: successful update of an SM context without content in the response

'400':

description: unsuccessful update of an SM context - bad request

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextUpdateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextUpdateError'

binaryDataN1SmMessage:

type: string

format: binary

binaryDataN2SmInformation:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

binaryDataN2SmInformation:

contentType: application/vnd.3gpp.ngap

headers:

Content-Id:

schema:

type: string

'403':

description: unsuccessful update of an SM context - forbidden

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextUpdateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextUpdateError'

binaryDataN1SmMessage:

type: string

format: binary

binaryDataN2SmInformation:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

binaryDataN2SmInformation:

contentType: application/vnd.3gpp.ngap

headers:

Content-Id:

schema:

type: string

'404':

description: unsuccessful update of an SM context - not found

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextUpdateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextUpdateError'

binaryDataN1SmMessage:

type: string

format: binary

binaryDataN2SmInformation:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

binaryDataN2SmInformation:

contentType: application/vnd.3gpp.ngap

headers:

Content-Id:

schema:

type: string

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'500':

description: unsuccessful update of an SM context - Internal server error

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextUpdateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextUpdateError'

binaryDataN1SmMessage:

type: string

format: binary

binaryDataN2SmInformation:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

binaryDataN2SmInformation:

contentType: application/vnd.3gpp.ngap

headers:

Content-Id:

schema:

type: string

'501':

$ref: 'TS29571\_CommonData.yaml#/components/responses/501'

'503':

description: unsuccessful update of an SM context - Service Unavailable

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/SmContextUpdateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/SmContextUpdateError'

binaryDataN1SmMessage:

type: string

format: binary

binaryDataN2SmInformation:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmMessage:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

binaryDataN2SmInformation:

contentType: application/vnd.3gpp.ngap

headers:

Content-Id:

schema:

type: string

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/sm-contexts/{smContextRef}/release:

post:

summary: Release SM Context

tags:

- Individual SM context

operationId: ReleaseSmContext

parameters:

- name: smContextRef

in: path

description: SM context reference

required: true

schema:

type: string

requestBody:

description: representation of the data to be sent to the SMF when releasing the SM context

required: false

content:

application/json:

schema:

$ref: '#/components/schemas/SmContextReleaseData'

responses:

'204':

description: successful release of an SM context without content in the response

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'501':

$ref: 'TS29571\_CommonData.yaml#/components/responses/501'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/pdu-sessions:

post:

summary: Create

tags:

- PDU sessions collection

operationId: PostPduSessions

requestBody:

description: representation of the PDU session to be created in the H-SMF

required: true

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/PduSessionCreateData'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/PduSessionCreateData'

binaryDataN1SmInfoFromUe:

type: string

format: binary

binaryDataUnknownN1SmInfo:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmInfoFromUe:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

binaryDataUnknownN1SmInfo:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

callbacks:

statusNotification:

'{$request.body#/vsmfPduSessionUri}':

post:

summary: Notify Status

tags:

- Individual PDU session (V-SMF)

operationId: NotifyStatus

requestBody:

description: representation of the status notification

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/StatusNotification'

responses:

'204':

description: successful notificationof the status change

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'501':

$ref: 'TS29571\_CommonData.yaml#/components/responses/501'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

update:

'{$request.body#/vsmfPduSessionUri}/modify':

post:

summary: Update (initiated by H-SMF)

tags:

- Individual PDU session (V-SMF)

operationId: ModifyPduSession

requestBody:

description: representation of updates to apply to the PDU session

required: true

content:

application/+json: # message without binary body part

schema:

$ref: '#/components/schemas/VsmfUpdateData'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/VsmfUpdateData'

binaryDataN1SmInfoToUe:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmInfoToUe:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

responses:

'200':

description: successful update of a PDU session with content in the response

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/VsmfUpdatedData'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/VsmfUpdatedData'

binaryDataN1SmInfoFromUe:

type: string

format: binary

binaryDataUnknownN1SmInfo:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmInfoFromUe:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

binaryDataUnknownN1SmInfo:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

'204':

description: successful update of a PDU session without content in the response

'400':

$ref: '#/components/responses/VsmfUpdateError'

'403':

$ref: '#/components/responses/VsmfUpdateError'

'404':

$ref: '#/components/responses/VsmfUpdateError'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'500':

$ref: '#/components/responses/VsmfUpdateError'

'501':

$ref: 'TS29571\_CommonData.yaml#/components/responses/501'

'503':

$ref: '#/components/responses/VsmfUpdateError'

'504':

$ref: '#/components/responses/VsmfUpdateError'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: successful creation of a PDU session

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/PduSessionCreatedData'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/PduSessionCreatedData'

binaryDataN1SmInfoToUe:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmInfoToUe:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

'307':

description: temporary redirect

'308':

description: permanent redirect

'400':

$ref: '#/components/responses/PduSessionCreateError'

'403':

$ref: '#/components/responses/PduSessionCreateError'

'404':

$ref: '#/components/responses/PduSessionCreateError'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'500':

$ref: '#/components/responses/PduSessionCreateError'

'501':

$ref: 'TS29571\_CommonData.yaml#/components/responses/501'

'503':

$ref: '#/components/responses/PduSessionCreateError'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/pdu-sessions/{pduSessionRef}/modify:

post:

summary: Update (initiated by V-SMF)

tags:

- Individual PDU session (H-SMF)

operationId: UpdatePduSession

parameters:

- name: pduSessionRef

in: path

description: PDU session reference

required: true

schema:

type: string

requestBody:

description: representation of the updates to apply to the PDU session

required: true

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/HsmfUpdateData'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/HsmfUpdateData'

binaryDataN1SmInfoFromUe:

type: string

format: binary

binaryDataUnknownN1SmInfo:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmInfoFromUe:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

binaryDataUnknownN1SmInfo:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

responses:

'200':

description: successful update of a PDU session with content in the response

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/HsmfUpdatedData'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/HsmfUpdatedData'

binaryDataN1SmInfoToUe:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmInfoToUe:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

'204':

description: successful update of a PDU session without content in the response

'400':

$ref: '#/components/responses/HsmfUpdateError'

'403':

$ref: '#/components/responses/HsmfUpdateError'

'404':

$ref: '#/components/responses/HsmfUpdateError'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'500':

$ref: '#/components/responses/HsmfUpdateError'

'501':

$ref: 'TS29571\_CommonData.yaml#/components/responses/501'

'503':

$ref: '#/components/responses/HsmfUpdateError'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/pdu-sessions/{pduSessionRef}/release:

post:

summary: Release

tags:

- Individual PDU session (H-SMF)

operationId: ReleasePduSession

parameters:

- name: pduSessionRef

in: path

description: PDU session reference

required: true

schema:

type: string

requestBody:

description: representation of the data to be sent to H-SMF when releasing the PDU session

required: false

content:

application/json:

schema:

$ref: '#/components/schemas/ReleaseData'

responses:

'204':

description: successful release of a PDU session

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'501':

$ref: 'TS29571\_CommonData.yaml#/components/responses/501'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes: {}

schemas:

#

# STRUCTURED DATA TYPES

#

SmContextCreateData:

type: object

properties:

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

unauthenticatedSupi:

type: boolean

default: false

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

pduSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

sNssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

hplmnSnssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

servingNfId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

guami:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

serviceName:

type: string

servingNetwork:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

requestType:

$ref: '#/components/schemas/RequestType'

n1SmMsg:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

anType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

presenceInLadn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceState'

ueLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

addUeLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

smContextStatusUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

hSmfUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

additionalHsmfUri:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

oldPduSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

pduSessionsActivateList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

minItems: 0

ueEpsPdnConnection:

$ref: '#/components/schemas/EpsPdnCnxContainer'

hoState:

$ref: '#/components/schemas/HoState'

pcfId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

nrfUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

selMode:

$ref: '#/components/schemas/DnnSelectionMode'

backupAmfInfo:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BackupAmfInfo'

traceData:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TraceData'

epsInterworkingInd:

$ref: '#/components/schemas/EpsInterworkingIndication'

required:

- servingNfId

- servingNetwork

- anType

- smContextStatusUri

SmContextCreatedData:

type: object

properties:

hSmfUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

pduSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

sNssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

upCnxState:

$ref: '#/components/schemas/UpCnxState'

n2SmInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

n2SmInfoType:

$ref: '#/components/schemas/N2SmInfoType'

allocatedEbiList:

type: array

items:

$ref: '#/components/schemas/EbiArpMapping'

minItems: 0

hoState:

$ref: '#/components/schemas/HoState'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

SmContextUpdateData:

type: object

properties:

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

servingNfId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

guami:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

servingNetwork:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

backupAmfInfo:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BackupAmfInfo'

anType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

presenceInLadn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceState'

ueLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

addUeLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

upCnxState:

$ref: '#/components/schemas/UpCnxState'

hoState:

$ref: '#/components/schemas/HoState'

toBeSwitched:

type: boolean

default: false

failedToBeSwitched:

type: boolean

n1SmMsg:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

n2SmInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

n2SmInfoType:

$ref: '#/components/schemas/N2SmInfoType'

targetServingNfId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

smContextStatusUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

dataForwarding:

type: boolean

default: false

epsBearerSetup:

type: array

items:

$ref: '#/components/schemas/EpsBearerContainer'

minItems: 0

revokeEbiList:

type: array

items:

$ref: '#/components/schemas/EpsBearerId'

minItems: 0

release:

type: boolean

default: false

cause:

$ref: '#/components/schemas/Cause'

ngApCause:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NgApCause'

5GMmCauseValue:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5GMmCause'

sNssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

traceData:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TraceData'

epsInterworkingInd:

$ref: '#/components/schemas/EpsInterworkingIndication'

SmContextUpdatedData:

type: object

properties:

upCnxState:

$ref: '#/components/schemas/UpCnxState'

hoState:

$ref: '#/components/schemas/HoState'

releaseEbiList:

type: array

items:

$ref: '#/components/schemas/EpsBearerId'

minItems: 0

allocatedEbiList:

type: array

items:

$ref: '#/components/schemas/EbiArpMapping'

minItems: 0

modifiedEbiList:

type: array

items:

$ref: '#/components/schemas/EbiArpMapping'

minItems: 0

n1SmMsg:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

n2SmInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

n2SmInfoType:

$ref: '#/components/schemas/N2SmInfoType'

epsBearerSetup:

type: array

items:

$ref: '#/components/schemas/EpsBearerContainer'

minItems: 0

dataForwarding:

type: boolean

SmContextReleaseData:

type: object

properties:

cause:

$ref: '#/components/schemas/Cause'

ngApCause:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NgApCause'

5GMmCauseValue:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5GMmCause'

ueLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

addUeLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

vsmfReleaseOnly:

type: boolean

default: false

SmContextStatusNotification:

type: object

properties:

statusInfo :

$ref: '#/components/schemas/StatusInfo'

required:

- statusInfo

PduSessionCreateData:

type: object

properties:

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

unauthenticatedSupi:

type: boolean

default: false

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

pduSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

sNssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

vsmfId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

servingNetwork:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

requestType:

$ref: '#/components/schemas/RequestType'

epsBearerId:

type: array

items:

$ref: '#/components/schemas/EpsBearerId'

minItems: 0

pgwS8cFteid:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

vsmfPduSessionUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

vcnTunnelInfo:

$ref: '#/components/schemas/TunnelInfo'

anType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

ueLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

addUeLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

n1SmInfoFromUe:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

unknownN1SmInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

hPcfId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

hoPreparationIndication:

type: boolean

selMode:

$ref: '#/components/schemas/DnnSelectionMode'

epsInterworkingInd:

$ref: '#/components/schemas/EpsInterworkingIndication'

vSmfServiceInstanceId:

type: string

required:

- dnn

- vsmfId

- servingNetwork

- vsmfPduSessionUri

- vcnTunnelInfo

- anType

PduSessionCreatedData:

type: object

properties:

pduSessionType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

sscMode:

type: string

hcnTunnelInfo:

$ref: '#/components/schemas/TunnelInfo'

sessionAmbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

qosFlowsSetupList:

type: array

items:

$ref: '#/components/schemas/QosFlowSetupItem'

minItems: 1

pduSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

sNssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

enablePauseCharging:

type: boolean

default: false

ueIpv4Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ueIpv6Prefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

n1SmInfoToUe:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

epsPdnCnxInfo:

$ref: '#/components/schemas/EpsPdnCnxInfo'

epsBearerInfo:

type: array

items:

$ref: '#/components/schemas/EpsBearerInfo'

minItems: 1

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

upSecurity:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UpSecurity'

required:

- pduSessionType

- sscMode

- hcnTunnelInfo

- sessionAmbr

- qosFlowsSetupList

HsmfUpdateData:

type: object

properties:

requestIndication:

$ref: '#/components/schemas/RequestIndication'

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

vcnTunnelInfo:

$ref: '#/components/schemas/TunnelInfo'

servingNetwork:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

anType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

ueLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

addUeLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

pauseCharging:

type: boolean

pti:

$ref: '#/components/schemas/ProcedureTransactionId'

n1SmInfoFromUe:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

unknownN1SmInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

qosFlowsRelNotifyList:

type: array

items:

$ref: '#/components/schemas/QosFlowItem'

minItems: 0

qosFlowsNotifyList:

type: array

items:

$ref: '#/components/schemas/QosFlowNotifyItem'

minItems: 0

NotifyList:

type: array

items:

$ref: '#/components/schemas/PduSessionNotifyItem'

minItems: 0

epsBearerId:

type: array

items:

$ref: '#/components/schemas/EpsBearerId'

minItems: 0

hoPreparationIndication:

type: boolean

revokeEbiList:

type: array

items:

$ref: '#/components/schemas/EpsBearerId'

minItems: 0

cause:

$ref: '#/components/schemas/Cause'

ngApCause:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NgApCause'

5GMmCauseValue:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5GMmCause'

epsInterworkingInd:

$ref: '#/components/schemas/EpsInterworkingIndication'

required:

- requestIndication

HsmfUpdatedData:

type: object

properties:

n1SmInfoToUe:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

ReleaseData:

type: object

properties:

cause:

$ref: '#/components/schemas/Cause'

ngApCause:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NgApCause'

5GMmCauseValue:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5GMmCause'

ueLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

addUeLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ReleasedData:

type: object

VsmfUpdateData:

type: object

properties:

requestIndication:

$ref: '#/components/schemas/RequestIndication'

sessionAmbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

qosFlowsAddModRequestList:

type: array

items:

$ref: '#/components/schemas/QosFlowAddModifyRequestItem'

minItems: 0

qosFlowsRelRequestList:

type: array

items:

$ref: '#/components/schemas/QosFlowReleaseRequestItem'

minItems: 0

epsBearerInfo:

type: array

items:

$ref: '#/components/schemas/EpsBearerInfo'

minItems: 0

assignEbiList:

type: array

items:

$ref: '#/components/schemas/EpsBearerId'

minItems: 0

revokeEbiList:

type: array

items:

$ref: '#/components/schemas/EpsBearerId'

minItems: 0

modifiedEbiList:

type: array

items:

$ref: '#/components/schemas/EbiArpMapping'

minItems: 0

pti:

$ref: '#/components/schemas/ProcedureTransactionId'

n1SmInfoToUe:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

cause:

$ref: '#/components/schemas/Cause'

required:

- requestIndication

VsmfUpdatedData:

type: object

properties:

qosFlowsAddModList:

type: array

items:

$ref: '#/components/schemas/QosFlowItem'

minItems: 0

qosFlowsRelList:

type: array

items:

$ref: '#/components/schemas/QosFlowItem'

minItems: 0

qosFlowsFailedtoAddModList:

type: array

items:

$ref: '#/components/schemas/QosFlowItem'

minItems: 0

qosFlowsFailedtoRelList:

type: array

items:

$ref: '#/components/schemas/QosFlowItem'

minItems: 0

n1SmInfoFromUe:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

unknownN1SmInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

ueLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

addUeLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

assignedEbiList:

type: array

items:

$ref: '#/components/schemas/EbiArpMapping'

minItems: 0

failedToAssignEbiList:

type: array

items:

$ref: '#/components/schemas/EpsBearerId'

minItems: 0

releasedEbiList:

type: array

items:

$ref: '#/components/schemas/EpsBearerId'

minItems: 0

StatusNotification:

type: object

properties:

statusInfo :

$ref: '#/components/schemas/StatusInfo'

required:

- statusInfo

QosFlowItem:

type: object

properties:

qfi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

cause:

$ref: '#/components/schemas/Cause'

required:

- qfi

QosFlowSetupItem:

type: object

properties:

qfi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

qosRules:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

qosFlowDescription:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

qosFlowProfile:

$ref: '#/components/schemas/QosFlowProfile'

required:

- qfi

- qosRules

QosFlowAddModifyRequestItem:

type: object

properties:

qfi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

qosRules:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

qosFlowDescription:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

qosFlowProfile:

$ref: '#/components/schemas/QosFlowProfile'

required:

- qfi

QosFlowReleaseRequestItem:

type: object

properties:

qfi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

qosRules:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

qosFlowDescription:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

required:

- qfi

QosFlowProfile:

type: object

properties:

5qi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

nonDynamic5Qi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NonDynamic5Qi'

dynamic5Qi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dynamic5Qi'

arp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Arp'

gbrQosFlowInfo:

$ref: '#/components/schemas/GbrQosFlowInformation'

rqa:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ReflectiveQoSAttribute'

required:

- 5qi

GbrQosFlowInformation:

type: object

properties:

maxFbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

maxFbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

guaFbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

guaFbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

notifControl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NotificationControl'

maxPacketLossRateDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRate'

maxPacketLossRateUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRate'

required:

- maxFbrDl

- maxFbrUl

- guaFbrDl

- guaFbrUl

QosFlowNotifyItem:

type: object

properties:

qfi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

notificationCause:

$ref: '#/components/schemas/NotificationCause'

required:

- qfi

- notificationCause

SmContextRetrieveData:

type: object

properties:

targetMmeCap:

$ref: '#/components/schemas/MmeCapabilities'

SmContextRetrievedData:

type: object

properties:

ueEpsPdnConnection:

$ref: '#/components/schemas/EpsPdnCnxContainer'

required:

- ueEpsPdnConnection

MmeCapabilities:

type: object

properties:

nonIpSupported:

type: boolean

default: false

TunnelInfo:

type: object

properties:

ipv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

gtpTeid:

$ref: '#/components/schemas/Teid'

required:

- gtpTeid

StatusInfo:

type: object

properties:

resourceStatus:

$ref: '#/components/schemas/ResourceStatus'

cause:

$ref: '#/components/schemas/Cause'

required:

- resourceStatus

EpsPdnCnxInfo:

type: object

properties:

pgwS8cFteid:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

pgwNodeName:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

required:

- pgwS8cFteid

EpsBearerInfo:

type: object

properties:

ebi:

$ref: '#/components/schemas/EpsBearerId'

pgwS8uFteid:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

bearerLevelQoS:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

required:

- ebi

- pgwS8uFteid

- bearerLevelQoS

PduSessionNotifyItem:

type: object

properties:

notificationCause:

$ref: '#/components/schemas/NotificationCause'

required:

- notificationCause

EbiArpMapping:

type: object

properties:

epsBearerId:

$ref: '#/components/schemas/EpsBearerId'

arp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Arp'

required:

- epsBearerId

- arp

SmContextCreateError:

type: object

properties:

error:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

n1SmMsg:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

required:

- error

SmContextUpdateError:

type: object

properties:

error:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

n1SmMsg:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

n2SmInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

n2SmInfoType:

$ref: '#/components/schemas/N2SmInfoType'

upCnxState:

$ref: '#/components/schemas/UpCnxState'

required:

- error

PduSessionCreateError:

type: object

properties:

error:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

n1smCause:

type: string

n1SmInfoToUe:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

required:

- error

HsmfUpdateError:

type: object

properties:

error:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

pti:

$ref: '#/components/schemas/ProcedureTransactionId'

n1smCause:

type: string

n1SmInfoToUe:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

required:

- error

VsmfUpdateError:

type: object

properties:

error:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

pti:

$ref: '#/components/schemas/ProcedureTransactionId'

n1smCause:

type: string

n1SmInfoFromUe:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

unknownN1SmInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

failedToAssignEbiList:

type: array

items:

$ref: '#/components/schemas/EpsBearerId'

minItems: 0

ngApCause:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NgApCause'

5GMmCauseValue:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5GMmCause'

required:

- error

#

# SIMPLE DATA TYPES

#

ProcedureTransactionId:

type: integer

format: ProcedureTransactionId

minimum: 0

maximum: 255

EpsBearerId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

EpsPdnCnxContainer:

type: string

format: EpsPdnCnxContainer

EpsBearerContainer:

type: string

format: EpsBearerContainer

Teid:

type: string

pattern: '^[A-F0-9]{8}$'

#

# ENUMERATIONS

#

UpCnxState:

anyOf:

- type: string

enum:

- ACTIVATED

- DEACTIVATED

- ACTIVATING

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- ACTIVATED

- DEACTIVATED

- ACTIVATING

HoState:

anyOf:

- type: string

enum:

- NONE

- PREPARING

- PREPARED

- COMPLETED

- CANCELLED

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- NONE

- PREPARING

- PREPARED

- COMPLETED

- CANCELLED

RequestType:

anyOf:

- type: string

enum:

- INITIAL\_REQUEST

- EXISTING\_PDU\_SESSION

- INITIAL\_EMERGENCY\_REQUEST

- EXISTING\_EMERGENCY\_PDU\_SESSION

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- INITIAL\_REQUEST

- EXISTING\_PDU\_SESSION

- INITIAL\_EMERGENCY\_REQUEST

- EXISTING\_EMERGENCY\_PDU\_SESSION

RequestIndication:

anyOf:

- type: string

enum:

- UE\_REQ\_PDU\_SES\_MOD

- UE\_REQ\_PDU\_SES\_REL

- PDU\_SES\_MOB

- NW\_REQ\_PDU\_SES\_AUTH

- NW\_REQ\_PDU\_SES\_MOD

- NW\_REQ\_PDU\_SES\_REL

- EBI\_ASSIGNMENT\_REQ

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- UE\_REQ\_PDU\_SES\_MOD

- UE\_REQ\_PDU\_SES\_REL

- PDU\_SES\_MOB

- NW\_REQ\_PDU\_SES\_AUTH

- NW\_REQ\_PDU\_SES\_MOD

- NW\_REQ\_PDU\_SES\_REL

- EBI\_ASSIGNMENT\_REQ

NotificationCause:

anyOf:

- type: string

enum:

- QOS\_FULFILLED

- QOS\_NOT\_FULFILLED

- UP\_SEC\_FULFILLED

- UP\_SEC\_NOT\_FULFILLED

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- QOS\_FULFILLED

- QOS\_NOT\_FULFILLED

- UP\_SEC\_FULFILLED

- UP\_SEC\_NOT\_FULFILLED

Cause:

anyOf:

- type: string

enum:

- REL\_DUE\_TO\_HO

- EPS\_FALLBACK

- REL\_DUE\_TO\_UP\_SEC

- DNN\_CONGESTION

- S-NSSAI\_CONGESTION

- REL\_DUE\_TO\_REACTIVATION

- 5G\_AN\_NOT\_RESPONDING

- REL\_DUE\_TO\_SLICE\_NOT\_AVAILABLE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- REL\_DUE\_TO\_HO

- EPS\_FALLBACK

- REL\_DUE\_TO\_UP\_SEC

- DNN\_CONGESTION

- S-NSSAI\_CONGESTION

- REL\_DUE\_TO\_REACTIVATION

- 5G\_AN\_NOT\_RESPONDING

- REL\_DUE\_TO\_SLICE\_NOT\_AVAILABLE

ResourceStatus:

anyOf:

- type: string

enum:

- RELEASED

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- RELEASED

DnnSelectionMode:

anyOf:

- type: string

enum:

- VERIFIED

- UE\_DNN\_NOT\_VERIFIED

- NW\_DNN\_NOT\_VERIFIED

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- VERIFIED

- UE\_DNN\_NOT\_VERIFIED

- NW\_DNN\_NOT\_VERIFIED

EpsInterworkingIndication:

anyOf:

- type: string

enum:

- NONE

- WITH\_N26

- WITHOUT\_N26

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- NONE

- WITH\_N26

- WITHOUT\_N26

N2SmInfoType:

anyOf:

- type: string

enum:

- PDU\_RES\_SETUP\_REQ

- PDU\_RES\_SETUP\_RSP

- PDU\_RES\_SETUP\_FAIL

- PDU\_RES\_REL\_CMD

- PDU\_RES\_REL\_RSP

- PDU\_RES\_MOD\_REQ

- PDU\_RES\_MOD\_RSP

- PDU\_RES\_MOD\_FAIL

- PDU\_RES\_NTY

- PDU\_RES\_NTY\_REL

- PDU\_RES\_MOD\_IND

- PDU\_RES\_MOD\_CFM

- PATH\_SWITCH\_REQ

- PATH\_SWITCH\_SETUP\_FAIL

- PATH\_SWITCH\_REQ\_ACK

- PATH\_SWITCH\_REQ\_FAIL

- HANDOVER\_REQUIRED

- HANDOVER\_CMD

- HANDOVER\_PREP\_FAIL

- HANDOVER\_REQ\_ACK

- HANDOVER\_RES\_ALLOC\_FAIL

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- PDU\_RES\_SETUP\_REQ

- PDU\_RES\_SETUP\_RSP

- PDU\_RES\_SETUP\_FAIL

- PDU\_RES\_REL\_CMD

- PDU\_RES\_REL\_RSP

- PDU\_RES\_MOD\_REQ

- PDU\_RES\_MOD\_RSP

- PDU\_RES\_MOD\_FAIL

- PDU\_RES\_NTY

- PDU\_RES\_NTY\_REL

- PDU\_RES\_MOD\_IND

- PDU\_RES\_MOD\_CFM

- PATH\_SWITCH\_REQ

- PATH\_SWITCH\_SETUP\_FAIL

- PATH\_SWITCH\_REQ\_ACK

- PATH\_SWITCH\_REQ\_FAIL

- HANDOVER\_REQUIRED

- HANDOVER\_CMD

- HANDOVER\_PREP\_FAIL

- HANDOVER\_REQ\_ACK

- HANDOVER\_RES\_ALLOC\_FAIL

#

# HTTP responses

#

responses:

'PduSessionCreateError':

description: unsuccessful creation of a PDU session

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/PduSessionCreateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/PduSessionCreateError'

binaryDataN1SmInfoToUe:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmInfoToUe:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

'HsmfUpdateError':

description: unsuccessful update of a PDU session

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/HsmfUpdateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/HsmfUpdateError'

binaryDataN1SmInfoToUe:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmInfoToUe:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

'VsmfUpdateError':

description: unsuccessful update of a PDU session

content:

application/json: # message without binary body part

schema:

$ref: '#/components/schemas/VsmfUpdateError'

multipart/related: # message with binary body part(s)

schema:

type: object

properties: # Request parts

jsonData:

$ref: '#/components/schemas/VsmfUpdateError'

binaryDataN1SmInfoFromUe:

type: string

format: binary

binaryDataUnknownN1SmInfo:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryDataN1SmInfoFromUe:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

binaryDataUnknownN1SmInfo:

contentType: application/vnd.3gpp.5gnas

headers:

Content-Id:

schema:

type: string

Annex B (Informative):  
HTTP Multipart Messages

## B.1 Example of HTTP multipart message

### B.1.1 General

This subclause provides a (partial) example of HTTP multipart message. The example does not aim to be a complete representation of the HTTP message, e.g. additional information or headers can be included.

This Annex is informative and the normative descriptions in this specification prevail over the description in this Annex if there is any difference.

### B.1.2 Example HTTP multipart message with N1 SM Message binary data

POST /example.com/nsmf-pdusession/v1/sm-contexts HTTP/2

Content-Type: multipart/related; boundary=----Boundary

Content-Length: xyz

------Boundary

Content-Type: application/json

{

"supi": "imsi-<IMSI>",

"pduSessionId": 235,

"dnn": "<DNN>",

"sNssai": {

"sst": 0

},

"amfId": "<AMF Identifier>",

"n1SmMsg": {

"contentId": "n1msg"

},

"anType": "3GPP\_ACCESS",

"smContextStatusUri": "<URI>"

}

------Boundary

Content-Type: application/vnd.3gpp.5gnas

Content-Id: n1msg

{ … N1 SM Message binary data …}

------Boundary

Annex C (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-10 | CT4#80 | C4-175050 |  |  |  | Initial Draft. | 0.1.0 |
| 2017-10 | CT4#80 | C4-175392 |  |  |  | Inclusion of pCRs agreed during CT4#80. | 0.2.0 |
| 2017-12 | CT4#81 | C4-176435 |  |  |  | Inclusion of pCRs agreed during CT4#81. | 0.3.0 |
| 2018-01 | CT4#82 | C4-181389 |  |  |  | Inclusion of pCRs agreed during CT4#82. | 0.4.0 |
| 2018-03 | CT4#83 | C4-182432 |  |  |  | Inclusion of pCRs agreed during CT4#83. | 0.5.0 |
| 2018-03 | CT#79 | CP-180030 |  |  |  | Presented for information | 1.0.0 |
| 2018-04 | CT4#84 | C4-183514 |  |  |  | Inclusion of pCRs agreed during CT4#84. | 1.1.0 |
| 2018-05 | CT4#85 | C4-184619 |  |  |  | Inclusion of pCRs agreed during CT4#85. | 1.2.0 |
| 2018-06 | CT#80 | CP-181100 |  |  |  | Presented for approval | 2.0.0 |
| 2018-06 | CT#80 |  |  |  |  | Approved in CT#80. | 15.0.0 |
| 2018-09 | CT#81 | CP-182055 | 0002 |  | F | Corrections to missing application errors in API response body description | 15.1.0 |
| 2018-09 | CT#81 | CP-182068 | 0006 |  | B | Add support for 5G Trace | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0007 |  | F | Error Responses | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0015 |  | F | Network Sharing | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0016 |  | F | RAT Type in Create and Update (SM Context) service operations | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0001 | 1 | F | Application specific error cause for Not Acceptable Integrity Protection Max Data Rate | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0008 | 1 | F | EBI Assignment for Home Routed PDU sessions | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0010 | 1 | F | Returning the H-SMF URI to the AMF | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0014 | 1 | F | N2 SM signalling | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0017 | 1 | F | Supporting AMF changes | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0018 | 1 | F | VPLMN S-NSSAI during mobility from EPS to 5GC with N26 | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0009 | 2 | F | HTTP message retransmissions and requests colliding with existing contexts | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0029 |  | F | Rejected PDU session during Xn handover | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0033 |  | F | Description of Structured data types | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0034 |  | F | Handling of LADN service area during handovers | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0036 |  | F | Mapping to stage 2 service operation names | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0039 |  | F | Stateless AMF support updates | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0040 |  | F | QoS rule structure improvement | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0020 | 1 | F | NRF URI for PCF Selection | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0022 | 1 | F | BackUp AMF Info | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0031 | 1 | F | NGAP causes | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0024 | 1 | F | EPS Interworking Ind | 15.1.0 |
| 2018-09 | CT#81 | CP-182050 | 0021 | 2 | F | References to common NonDynamic5Qi and Dynamic5Qi data types | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0025 | 1 | F | Not Allowed Slice | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0005 | 3 | F | N2 SM Information Type Definition | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0028 | 1 | F | OpenAPI corrections | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0032 | 1 | F | Age of User Location | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0037 | 1 | F | Detecting SMF Failure and Restart | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0041 |  | F | PresenceState reference | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0030 | 2 | F | URIs of created SM context and PDU session resources | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0023 | 2 | F | 5G MM Cause | 15.1.0 |
| 2018-09 | CT#81 | CP-182055 | 0042 |  | F | API version number update | 15.1.0 |